(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6002)
    (drawings 419)
    (tracks 264)
    (zones 0)
    (modules 28)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3175)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 0.9 0.4)
    (user_via 1 0.6)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.254)
    (pcb_text_width 0.254)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.12)
    (mod_text_size 0.75 0.75)
    (mod_text_width 0.12)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-+3V3)
  (net 2 Board_1-+5V)
  (net 3 Board_1-/PMS_RX)
  (net 4 Board_1-/PMS_TX)
  (net 5 Board_1-/RGB)
  (net 6 Board_1-/SCL)
  (net 7 Board_1-/SDA)
  (net 8 Board_1-/U0RXD)
  (net 9 Board_1-/U0TXD)
  (net 10 Board_1-/USB_D+)
  (net 11 Board_1-/USB_D-)
  (net 12 Board_1-/VCC_ALS)
  (net 13 Board_1-/VCC_BME)
  (net 14 Board_1-/~BOOT)
  (net 15 Board_1-/~PMS_RST)
  (net 16 Board_1-/~PMS_SET)
  (net 17 Board_1-/~RST)
  (net 18 Board_1-GND)
  (net 19 "Board_1-Net-(J1-PadA5)")
  (net 20 "Board_1-Net-(J1-PadB5)")
  (net 21 "Board_1-Net-(M1-Pad6)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-+3V3)
    (add_net Board_1-+5V)
    (add_net Board_1-/PMS_RX)
    (add_net Board_1-/PMS_TX)
    (add_net Board_1-/RGB)
    (add_net Board_1-/SCL)
    (add_net Board_1-/SDA)
    (add_net Board_1-/U0RXD)
    (add_net Board_1-/U0TXD)
    (add_net Board_1-/USB_D+)
    (add_net Board_1-/USB_D-)
    (add_net Board_1-/VCC_ALS)
    (add_net Board_1-/VCC_BME)
    (add_net Board_1-/~BOOT)
    (add_net Board_1-/~PMS_RST)
    (add_net Board_1-/~PMS_SET)
    (add_net Board_1-/~RST)
    (add_net Board_1-GND)
    (add_net "Board_1-Net-(J1-PadA5)")
    (add_net "Board_1-Net-(J1-PadB5)")
    (add_net "Board_1-Net-(M1-Pad6)")
  )
  (net_class USB_D ""
    (clearance 0.254)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.127)
  )
  (net_class VCC ""
    (clearance 0.127)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class VIN ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.127)
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 131 77.5)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference H1 (at 0 -2.9 unlocked) (layer F.SilkS) hide)
    (fp_text value MP (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at -1.2 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers B.Cu B.Mask)
      (net 18 Board_1-GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 169 122.5)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference H2 (at 0 -2.9 unlocked) (layer F.SilkS) hide)
    (fp_text value MP (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers B.Cu B.Mask)
      (net 18 Board_1-GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 169 77.5)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference H3 (at 0 -2.9 unlocked) (layer F.SilkS) hide)
    (fp_text value MP (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers B.Cu B.Mask)
      (net 18 Board_1-GND))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 131 122.5)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (attr virtual)
    (fp_text reference H4 (at 0 -2.9 unlocked) (layer F.SilkS) hide)
    (fp_text value MP (at 0 2.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.6 2.6) (drill 2.2) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers F.Cu F.Mask)
      (net 18 Board_1-GND))
    (pad 1 connect circle (at 0 0) (size 3.8 3.8) (layers B.Cu B.Mask)
      (net 18 Board_1-GND))
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 153.48 101.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.675 0 unlocked) (layer F.SilkS))
    (fp_text value 1u (at -1.1 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/VCC_BME))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 151 116 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 1.6 0 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at -1.1 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/VCC_BME))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139 95.5)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -1.85 0 unlocked) (layer F.SilkS))
    (fp_text value 4k7 (at -1.15 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-/SCL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139 93.5)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.85 0 unlocked) (layer F.SilkS))
    (fp_text value 4k7 (at -1.15 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 2 smd roundrect (at 0.51 0) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-/SDA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 150.52 101.5 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.875 0 unlocked) (layer F.SilkS))
    (fp_text value 1u (at -1.125 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Board_1-/VCC_ALS))
    (pad 2 smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 148 113.7 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 1.5 0.2 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at -1.125 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Board_1-/VCC_ALS))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 11-My-Edits:Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering (layer F.Cu) (tedit 60713966)
    (at 145.75 122 90)
    (descr "Bosch  LGA, 8 Pin (https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BME680-DS001-00.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "Bosch LGA NoLead")
    (attr smd)
    (fp_text reference U2 (at 2.3 0 unlocked) (layer F.SilkS))
    (fp_text value BME68x (at -2 0.05) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at -1.2 1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/VCC_BME))
    (pad 7 smd roundrect (at -0.4 1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 6 smd roundrect (at 0.4 1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/VCC_BME))
    (pad 5 smd roundrect (at 1.2 1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 4 smd roundrect (at 1.2 -1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-/SCL))
    (pad 3 smd roundrect (at 0.4 -1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-/SDA))
    (pad 2 smd roundrect (at -0.4 -1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/VCC_BME))
    (pad 1 smd roundrect (at -1.2 -1.1875 90) (size 0.5 0.525) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model :SnapEDA-3D:BME680--3DModel-STEP-56544.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 12-Collected-Footprints:PMSA003 locked (layer B.Cu) (tedit 6071464E)
    (at 150 97.5)
    (fp_text reference M1 (at 0 -0.75 unlocked) (layer B.SilkS))
    (fp_text value PMSA003 (at 0 0.75 unlocked) (layer B.SilkS))
    (pad "" np_thru_hole circle (at 16.5 15) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -16.5 -15) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at -11.5 12.17 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 Board_1-/~PMS_RST))
    (pad 1 thru_hole rect (at -14.04 12.17 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (pad 7 thru_hole oval (at -10.23 12.17 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 Board_1-/PMS_RX))
    (pad 6 thru_hole oval (at -11.5 10.9 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Board_1-Net-(M1-Pad6)"))
    (pad 3 thru_hole oval (at -12.77 12.17 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (pad 10 thru_hole oval (at -8.96 10.9 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 Board_1-/~PMS_SET))
    (pad 9 thru_hole oval (at -8.96 12.17 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 Board_1-/PMS_TX))
    (pad 8 thru_hole oval (at -10.23 10.9 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 "Board_1-Net-(M1-Pad6)"))
    (pad 2 thru_hole oval (at -14.04 10.9 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 Board_1-+5V))
    (pad 4 thru_hole oval (at -12.77 10.9 270) (size 1 1) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_2x05_P1.27mm_Vertical.wrl
      (offset (xyz -8.949999999999999 10.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model :SnapEDA-3D:PMSA003-body.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 180))
    )
    (model :SnapEDA-3D:PMSA003-fan-blk.wrl
      (offset (xyz 14.35 -32.75 -14.35))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz -90 0 180))
    )
  )
  (module 11-My-Edits:MultiALS-LTR303-TIOPT3K (layer F.Cu) (tedit 60751DBB)
    (at 145.75 113.5 180)
    (descr "ambient light sensor, i2c interface, 6-pin chipled package, http://optoelectronics.liteon.com/upload/download/DS86-2013-0004/LTR-303ALS-01_DS_V1.pdf")
    (tags "ambient light sensor chipled")
    (attr smd)
    (fp_text reference U3 (at 0 1.875 unlocked) (layer F.SilkS))
    (fp_text value OPT3001DNPT (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 6 smd roundrect (at 0.9 -0.65 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-/SDA))
    (pad 5 smd roundrect (at 0.9 0 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at 0.9 0.65 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-/SCL))
    (pad 3 smd roundrect (at -0.9 0.65 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 2 smd roundrect (at -0.9 0 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 1 smd roundrect (at -0.9 -0.65 180) (size 0.65 0.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Board_1-/VCC_ALS))
    (pad 7 thru_hole circle (at 0 0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 18 Board_1-GND) (solder_mask_margin 0.001))
    (pad 7 smd rect (at 0 0 180) (size 0.65 1.35) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND) (solder_mask_margin 0.07))
    (pad 7 thru_hole circle (at 0 -0.4 180) (size 0.2 0.2) (drill 0.2) (layers *.Cu *.Mask)
      (net 18 Board_1-GND) (solder_mask_margin 0.001))
    (model ":SnapEDA-3D:APA102-2020 MODEL v15.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 0.393700787 0.393700787 0.393700787))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 136.825 111.875)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at -2.625 0 unlocked) (layer F.SilkS))
    (fp_text value 10u (at -1.85 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Board_1-+5V))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 136.825 113.425)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at -2.625 0 unlocked) (layer F.SilkS))
    (fp_text value 10u (at -1.85 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Board_1-+5V))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 143.25 103.5 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 2.5 0 unlocked) (layer F.SilkS))
    (fp_text value XC6210B332MR (at 0.25 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-+5V))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-+5V))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 140.8 104.5 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.05 90 unlocked) (layer F.SilkS))
    (fp_text value 10u (at 1.1 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Board_1-+5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 140.8 102.5 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 1.05 90 unlocked) (layer F.SilkS))
    (fp_text value 10u (at -1.1 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139 87.5)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -1.85 0 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at -1.12 0 -270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-/~RST))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 11-My-Edits:TC2030_IDCBox_2x03_P1.25mm_Vertical_3D (layer F.Cu) (tedit 607596E6)
    (at 166 85.05 270)
    (descr "Harwin Gecko Connector, 6 pins, dual row male, vertical entry, no latches, PN:G125-MVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at -6.05 0.45 unlocked) (layer F.SilkS))
    (fp_text value ESP-PROG (at 0 -3.675 90) (layer F.Fab))
    (fp_text user KEEPOUT (at 0 0.025 90) (layer Cmts.User))
    (pad "" np_thru_hole circle (at 2.54 1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 0 270) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -1.27 -0.635) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 1.27 -0.635) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 Board_1-/~BOOT))
    (pad 5 thru_hole oval (at 1.27 0.635) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 Board_1-/U0RXD))
    (pad 4 thru_hole oval (at 0 -0.635) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 18 Board_1-GND))
    (pad 1 thru_hole rect (at -1.27 0.635) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 Board_1-/~RST))
    (pad 3 thru_hole oval (at 0 0.635) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 9 Board_1-/U0TXD))
    (model :SnapEDA-3D:Samtec/SHF-103-01-L-D-TH.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 11-My-Edits:ESP-12H locked (layer F.Cu) (tedit 6105131F)
    (at 150 87)
    (descr "Wi-Fi Module, http://wiki.ai-thinker.com/_media/esp8266/docs/aithinker_esp_12f_datasheet_en.pdf")
    (tags "Wi-Fi Module")
    (attr smd)
    (fp_text reference U1 (at -10 -6 unlocked) (layer F.SilkS))
    (fp_text value ESP32-C3F (at -0.06 -12.78) (layer F.Fab))
    (fp_text user Antenna (at -0.06 -7 180) (layer Cmts.User))
    (fp_text user "KEEP-OUT ZONE" (at 0.03 -9.55 180) (layer Cmts.User))
    (pad 1 smd rect (at -7.6 -3.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 3 Board_1-/PMS_RX))
    (pad 2 smd rect (at -7.6 -1.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 4 Board_1-/PMS_TX))
    (pad 3 smd rect (at -7.6 0.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-/~RST))
    (pad 4 smd rect (at -7.6 2.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 16 Board_1-/~PMS_SET))
    (pad 5 smd rect (at -7.6 4.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 15 Board_1-/~PMS_RST))
    (pad 6 smd rect (at -7.6 6.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-/SDA))
    (pad 7 smd rect (at -7.6 8.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 6 Board_1-/SCL))
    (pad 8 smd rect (at -7.6 10.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3V3))
    (pad 9 smd rect (at -5 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -3 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 1 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 12 Board_1-/VCC_ALS))
    (pad 13 smd rect (at 3 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 13 Board_1-/VCC_BME))
    (pad 14 smd rect (at 5 12) (size 1 1.8) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 7.6 10.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad 16 smd rect (at 7.6 8.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 7.6 6.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 Board_1-/RGB))
    (pad 18 smd rect (at 7.6 4.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-/~BOOT))
    (pad 19 smd rect (at 7.6 2.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 10 Board_1-/USB_D+))
    (pad 20 smd rect (at 7.6 0.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 11 Board_1-/USB_D-))
    (pad 21 smd rect (at 7.6 -1.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 8 Board_1-/U0RXD))
    (pad 22 smd rect (at 7.6 -3.5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 9 Board_1-/U0TXD))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP-12E.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 41-EasyEDA-Edits:USB-C-SMD_TYPEC-304S-ACP16 locked (layer F.Cu) (tedit 603B3D05)
    (at 158.5 113.05)
    (attr smd)
    (fp_text reference J1 (at -4.25 -4.175 unlocked) (layer F.SilkS))
    (fp_text value USB_C_Receptacle_USB2.0_304S-ACP16 (at 0 0.25) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 4.445) (layer F.Fab))
    (pad "" np_thru_hole circle (at 2.89 -1.102) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -1.102) (size 0.7 0.7) (drill 0.7) (layers *.Cu *.Mask))
    (pad S1 smd rect (at 5.07 2.547) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad S1 smd rect (at -5.07 2.547) (size 1.8 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad S1 smd rect (at 5.07 -1.633) (size 1.8 1.45) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad S1 smd rect (at -5.07 -1.633) (size 1.8 1.45) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad B1A12 smd rect (at 3.22 -2.547) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad B4A9 smd rect (at 2.45 -2.547) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-+5V))
    (pad B5 smd rect (at 1.75 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Board_1-Net-(J1-PadB5)"))
    (pad A8 smd rect (at 1.25 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask))
    (pad B6 smd rect (at 0.75 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 10 Board_1-/USB_D+))
    (pad A7 smd rect (at 0.25 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 11 Board_1-/USB_D-))
    (pad A6 smd rect (at -0.25 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 10 Board_1-/USB_D+))
    (pad B7 smd rect (at -0.75 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 11 Board_1-/USB_D-))
    (pad A5 smd rect (at -1.26 -2.533) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 19 "Board_1-Net-(J1-PadA5)"))
    (pad B8 smd rect (at -1.75 -2.547) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask))
    (pad A4B9 smd rect (at -2.45 -2.547) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-+5V))
    (pad A1B12 smd rect (at -3.225 -2.547) (size 0.6 1.45) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (model ${EASY_EDA_3D}/../../Libraries/EasyEDA-Scraped/EasyEDA.3dshapes/USB-C-SMD_TYPEC-304S-ACP16.wrl
      (offset (xyz 0 0 0.65))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 167.5 117.8 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -1.875 0.025 unlocked) (layer F.SilkS))
    (fp_text value 5k1 (at 1.15 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Board_1-Net-(J1-PadA5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 167.5 116.7 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1.875 0 unlocked) (layer F.SilkS))
    (fp_text value 5k1 (at 1.15 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 Board_1-GND))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Board_1-Net-(J1-PadB5)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 21-SnapEDA-zip:LED_APA104-12-3535 (layer F.Cu) (tedit 61126FEC)
    (at 166 97.5 180)
    (attr smd)
    (fp_text reference D1 (at 0 -2.625) (layer F.SilkS))
    (fp_text value APA104-12-3535 (at 0 2.2) (layer F.Fab))
    (pad 1 smd rect (at -1.75 -0.875 180) (size 1.6 0.85) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.75 0.875 180) (size 1.6 0.85) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad 3 smd rect (at 1.75 0.875 180) (size 1.6 0.85) (layers F.Cu F.Paste F.Mask)
      (net 5 Board_1-/RGB))
    (pad 4 smd rect (at 1.75 -0.875 180) (size 1.6 0.85) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-+5V))
    (model ":SnapEDA-3D:SMD3535 RGB.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module 41-EasyEDA-Edits:SW-SMD_SKSLLAE010-3D (layer F.Cu) (tedit 611279CD)
    (at 130.375 107 270)
    (attr smd)
    (fp_text reference SW1 (at 0 0.875 90) (layer F.Fab))
    (fp_text value Reset (at -3.75 -0.5 unlocked) (layer F.SilkS))
    (pad MP smd rect (at 2.35 0.7) (size 1.85 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad MP smd rect (at -2.35 0.7) (size 1.85 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad 2 smd rect (at 0.85 -0.7) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-/~RST))
    (pad 1 smd rect (at -0.85 -0.7) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (model :SnapEDA-3D:ALPS/SKSLLA.STEP
      (offset (xyz 0 -1.4 0.55))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 41-EasyEDA-Edits:SW-SMD_SKSLLAE010-3D (layer F.Cu) (tedit 611279CD)
    (at 169.625 107 90)
    (attr smd)
    (fp_text reference SW2 (at 0 0.875 90) (layer F.Fab))
    (fp_text value Boot (at 3.75 -0.375 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.85 -0.7 180) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad 2 smd rect (at 0.85 -0.7 180) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-/~BOOT))
    (pad MP smd rect (at -2.35 0.7 180) (size 1.85 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (pad MP smd rect (at 2.35 0.7 180) (size 1.85 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-GND))
    (model :SnapEDA-3D:ALPS/SKSLLA.STEP
      (offset (xyz 0 -1.4 0.55))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 10-My-Footprints:neggle-logo-0.12 (layer F.Cu) (tedit 612095D0)
    (at 160 103.5)
    (fp_text reference LOGO1 (at 0 -1.75) (layer F.SilkS) hide)
    (fp_text value "neggles logo" (at 0 1) (layer F.Fab) hide)
  )
  (gr_line (start 142.95 116.476) (end 142.8778 116.4797) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.55 116.476) (end 142.95 116.476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.6222 116.4797) (end 148.55 116.476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.6937 116.4908) (end 148.6222 116.4797) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.7636 116.5091) (end 148.6937 116.4908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.8313 116.5345) (end 148.7636 116.5091) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.8961 116.5666) (end 148.8313 116.5345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.9572 116.6052) (end 148.8961 116.5666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.0141 116.6499) (end 148.9572 116.6052) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.066 116.7002) (end 149.0141 116.6499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1126 116.7555) (end 149.066 116.7002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1533 116.8152) (end 149.1126 116.7555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1877 116.8788) (end 149.1533 116.8152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2153 116.9456) (end 149.1877 116.8788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.236 117.0149) (end 149.2153 116.9456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2495 117.086) (end 149.236 117.0149) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2557 117.158) (end 149.2495 117.086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2545 117.2303) (end 149.2557 117.158) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2458 117.3021) (end 149.2545 117.2303) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2299 117.3726) (end 149.2458 117.3021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.2069 117.4411) (end 149.2299 117.3726) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1769 117.507) (end 149.2069 117.4411) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.1404 117.5694) (end 149.1769 117.507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.0977 117.6277) (end 149.1404 117.5694) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 149.0493 117.6814) (end 149.0977 117.6277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.0521 118.6771) (end 149.0493 117.6814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.9602 118.7592) (end 148.0521 118.6771) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8597 118.8305) (end 147.9602 118.7592) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7518 118.8902) (end 147.8597 118.8305) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.638 118.9373) (end 147.7518 118.8902) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.5196 118.9714) (end 147.638 118.9373) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.398 118.9921) (end 147.5196 118.9714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.275 118.999) (end 147.398 118.9921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.225 118.999) (end 147.275 118.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.1016 118.9921) (end 144.225 118.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.9798 118.9714) (end 144.1016 118.9921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.8611 118.9372) (end 143.9798 118.9714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.7469 118.8899) (end 143.8611 118.9372) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.6388 118.8301) (end 143.7469 118.8899) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.538 118.7586) (end 143.6388 118.8301) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.4459 118.6763) (end 143.538 118.7586) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4507 117.6814) (end 143.4459 118.6763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4023 117.6277) (end 142.4507 117.6814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3596 117.5694) (end 142.4023 117.6277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3231 117.507) (end 142.3596 117.5694) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2931 117.4411) (end 142.3231 117.507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2701 117.3726) (end 142.2931 117.4411) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2542 117.3021) (end 142.2701 117.3726) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2455 117.2303) (end 142.2542 117.3021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2443 117.158) (end 142.2455 117.2303) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2505 117.086) (end 142.2443 117.158) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.264 117.0149) (end 142.2505 117.086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2847 116.9456) (end 142.264 117.0149) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3123 116.8788) (end 142.2847 116.9456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3467 116.8152) (end 142.3123 116.8788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3874 116.7555) (end 142.3467 116.8152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.434 116.7002) (end 142.3874 116.7555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4859 116.6499) (end 142.434 116.7002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.5428 116.6052) (end 142.4859 116.6499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.6039 116.5666) (end 142.5428 116.6052) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.6687 116.5345) (end 142.6039 116.5666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.7364 116.5091) (end 142.6687 116.5345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.8063 116.4908) (end 142.7364 116.5091) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.8778 116.4797) (end 142.8063 116.4908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5537 105.6978) (end 169.551 105.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5619 105.6463) (end 169.5537 105.6978) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5754 105.5958) (end 169.5619 105.6463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5941 105.547) (end 169.5754 105.5958) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.6179 105.5005) (end 169.5941 105.547) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.6463 105.4567) (end 169.6179 105.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.6792 105.4161) (end 169.6463 105.4567) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.7161 105.3792) (end 169.6792 105.4161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.7567 105.3463) (end 169.7161 105.3792) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.8005 105.3179) (end 169.7567 105.3463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.847 105.2941) (end 169.8005 105.3179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.8958 105.2754) (end 169.847 105.2941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.9463 105.2619) (end 169.8958 105.2754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.9978 105.2537) (end 169.9463 105.2619) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.05 105.251) (end 169.9978 105.2537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2 105.251) (end 170.05 105.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2314 105.2494) (end 171.2 105.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2625 105.2444) (end 171.2314 105.2494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.293 105.2363) (end 171.2625 105.2444) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3224 105.225) (end 171.293 105.2363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3505 105.2106) (end 171.3224 105.225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.377 105.1935) (end 171.3505 105.2106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4014 105.1737) (end 171.377 105.1935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4237 105.1514) (end 171.4014 105.1737) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4435 105.1269) (end 171.4237 105.1514) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4606 105.1005) (end 171.4435 105.1269) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.475 105.0725) (end 171.4606 105.1005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4863 105.0431) (end 171.475 105.0725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4944 105.0125) (end 171.4863 105.0431) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4993 104.9815) (end 171.4944 105.0125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.501 104.9501) (end 171.4993 104.9815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.501 77.4999) (end 171.501 104.9501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4873 77.2385) (end 171.501 77.4999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4464 76.9801) (end 171.4873 77.2385) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3786 76.7272) (end 171.4464 76.9801) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2848 76.4828) (end 171.3786 76.7272) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.166 76.2495) (end 171.2848 76.4828) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.0234 76.03) (end 171.166 76.2495) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.8586 75.8265) (end 171.0234 76.03) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.6735 75.6414) (end 170.8586 75.8265) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.4701 75.4767) (end 170.6735 75.6414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.2505 75.3341) (end 170.4701 75.4767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.0172 75.2152) (end 170.2505 75.3341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.7728 75.1214) (end 170.0172 75.2152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.52 75.0537) (end 169.7728 75.1214) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.2614 75.0127) (end 169.52 75.0537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.9999 74.999) (end 169.2614 75.0127) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.72 75.0147) (end 168.9999 74.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.4435 75.0617) (end 168.72 75.0147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.174 75.1393) (end 168.4435 75.0617) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.9149 75.2467) (end 168.174 75.1393) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.6693 75.3824) (end 167.9149 75.2467) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.4407 75.5446) (end 167.6693 75.3824) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.2316 75.7315) (end 167.4407 75.5446) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.7564 78.2064) (end 167.2316 75.7315) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.6729 78.281) (end 164.7564 78.2064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.5815 78.3459) (end 164.6729 78.281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.4834 78.4001) (end 164.5815 78.3459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3799 78.4429) (end 164.4834 78.4001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.2723 78.474) (end 164.3799 78.4429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.1619 78.4927) (end 164.2723 78.474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.05 78.499) (end 164.1619 78.4927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.9571 78.499) (end 164.05 78.499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.8453 78.4927) (end 135.9571 78.499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.7348 78.474) (end 135.8453 78.4927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.6272 78.4429) (end 135.7348 78.474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.5237 78.4001) (end 135.6272 78.4429) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.4256 78.3459) (end 135.5237 78.4001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.3342 78.281) (end 135.4256 78.3459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.2507 78.2064) (end 135.3342 78.281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.7685 75.7315) (end 135.2507 78.2064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.5593 75.5446) (end 132.7685 75.7315) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.3306 75.3823) (end 132.5593 75.5446) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.0851 75.2467) (end 132.3306 75.3823) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.8261 75.1394) (end 132.0851 75.2467) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.5565 75.0617) (end 131.8261 75.1394) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.28 75.0147) (end 131.5565 75.0617) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.0001 74.999) (end 131.28 75.0147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.7385 75.0127) (end 131.0001 74.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.48 75.0537) (end 130.7385 75.0127) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.2272 75.1214) (end 130.48 75.0537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.9827 75.2152) (end 130.2272 75.1214) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.7495 75.3341) (end 129.9827 75.2152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.53 75.4766) (end 129.7495 75.3341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.3265 75.6414) (end 129.53 75.4766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.1414 75.8265) (end 129.3265 75.6414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.9767 76.0299) (end 129.1414 75.8265) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.834 76.2495) (end 128.9767 76.0299) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7152 76.4828) (end 128.834 76.2495) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6214 76.7271) (end 128.7152 76.4828) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5536 76.9801) (end 128.6214 76.7271) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5127 77.2386) (end 128.5536 76.9801) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.499 77.5) (end 128.5127 77.2386) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.499 104.9501) (end 128.499 77.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5006 104.9814) (end 128.499 104.9501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5056 105.0125) (end 128.5006 104.9814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5137 105.0431) (end 128.5056 105.0125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.525 105.0725) (end 128.5137 105.0431) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5394 105.1005) (end 128.525 105.0725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5565 105.127) (end 128.5394 105.1005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5763 105.1514) (end 128.5565 105.127) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5986 105.1737) (end 128.5763 105.1514) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.623 105.1935) (end 128.5986 105.1737) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6495 105.2106) (end 128.623 105.1935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6775 105.225) (end 128.6495 105.2106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7069 105.2363) (end 128.6775 105.225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7375 105.2444) (end 128.7069 105.2363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7686 105.2494) (end 128.7375 105.2444) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.8 105.251) (end 128.7686 105.2494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.95 105.251) (end 128.8 105.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.0022 105.2537) (end 129.95 105.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.0537 105.2619) (end 130.0022 105.2537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.1042 105.2754) (end 130.0537 105.2619) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.153 105.2941) (end 130.1042 105.2754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.1995 105.3179) (end 130.153 105.2941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.2433 105.3463) (end 130.1995 105.3179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.2839 105.3792) (end 130.2433 105.3463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.3208 105.4161) (end 130.2839 105.3792) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.3537 105.4567) (end 130.3208 105.4161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.3821 105.5005) (end 130.3537 105.4567) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4059 105.547) (end 130.3821 105.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4246 105.5958) (end 130.4059 105.547) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4381 105.6463) (end 130.4246 105.5958) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4463 105.6978) (end 130.4381 105.6463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.449 105.75) (end 130.4463 105.6978) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.449 108.25) (end 130.449 105.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4463 108.3022) (end 130.449 108.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4381 108.3537) (end 130.4463 108.3022) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4246 108.4042) (end 130.4381 108.3537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4059 108.453) (end 130.4246 108.4042) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.3821 108.4995) (end 130.4059 108.453) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.3537 108.5433) (end 130.3821 108.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.3208 108.5839) (end 130.3537 108.5433) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.2839 108.6208) (end 130.3208 108.5839) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.2433 108.6537) (end 130.2839 108.6208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.1995 108.6821) (end 130.2433 108.6537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.153 108.7059) (end 130.1995 108.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.1042 108.7246) (end 130.153 108.7059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.0537 108.7381) (end 130.1042 108.7246) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.0022 108.7463) (end 130.0537 108.7381) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.95 108.749) (end 130.0022 108.7463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.8 108.749) (end 129.95 108.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7685 108.7507) (end 128.8 108.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7374 108.7556) (end 128.7685 108.7507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.707 108.7637) (end 128.7374 108.7556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6775 108.775) (end 128.707 108.7637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6495 108.7894) (end 128.6775 108.775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6231 108.8065) (end 128.6495 108.7894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5986 108.8263) (end 128.6231 108.8065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5763 108.8486) (end 128.5986 108.8263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5565 108.873) (end 128.5763 108.8486) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5393 108.8995) (end 128.5565 108.873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.525 108.9276) (end 128.5393 108.8995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5137 108.9569) (end 128.525 108.9276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5056 108.9875) (end 128.5137 108.9569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5006 109.0186) (end 128.5056 108.9875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.499 109.0499) (end 128.5006 109.0186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.499 122.5) (end 128.499 109.0499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5127 122.7614) (end 128.499 122.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5536 123.0199) (end 128.5127 122.7614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6214 123.2728) (end 128.5536 123.0199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.7152 123.5172) (end 128.6214 123.2728) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.834 123.7505) (end 128.7152 123.5172) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.9766 123.97) (end 128.834 123.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.1414 124.1735) (end 128.9766 123.97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.3265 124.3586) (end 129.1414 124.1735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.5299 124.5233) (end 129.3265 124.3586) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.7495 124.6659) (end 129.5299 124.5233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.9827 124.7848) (end 129.7495 124.6659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.2272 124.8786) (end 129.9827 124.7848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.4801 124.9464) (end 130.2272 124.8786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.7386 124.9873) (end 130.4801 124.9464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.0001 125.001) (end 130.7386 124.9873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.2614 124.9873) (end 131.0001 125.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.52 124.9463) (end 131.2614 124.9873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.7729 124.8786) (end 131.52 124.9463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.0173 124.7848) (end 131.7729 124.8786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.2505 124.6659) (end 132.0173 124.7848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.4701 124.5233) (end 132.2505 124.6659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.6735 124.3586) (end 132.4701 124.5233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.8586 124.1735) (end 132.6735 124.3586) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.0234 123.97) (end 132.8586 124.1735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.1659 123.7505) (end 133.0234 123.97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.2848 123.5173) (end 133.1659 123.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.3786 123.2728) (end 133.2848 123.5173) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.4464 123.0199) (end 133.3786 123.2728) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.4873 122.7614) (end 133.4464 123.0199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.501 122.5001) (end 133.4873 122.7614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.501 120.75) (end 133.501 122.5001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.5147 120.4888) (end 133.501 120.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.5556 120.2304) (end 133.5147 120.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.6233 119.9778) (end 133.5556 120.2304) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.7171 119.7336) (end 133.6233 119.9778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.8358 119.5005) (end 133.7171 119.7336) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.9783 119.2811) (end 133.8358 119.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.1429 119.0778) (end 133.9783 119.2811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.3278 118.8929) (end 134.1429 119.0778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.5311 118.7283) (end 134.3278 118.8929) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.7505 118.5858) (end 134.5311 118.7283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.9836 118.4671) (end 134.7505 118.5858) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.2278 118.3733) (end 134.9836 118.4671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.4804 118.3056) (end 135.2278 118.3733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.7388 118.2647) (end 135.4804 118.3056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136 118.251) (end 135.7388 118.2647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.5 118.251) (end 136 118.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.7798 118.2667) (end 138.5 118.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.0561 118.3137) (end 138.7798 118.2667) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.3254 118.3912) (end 139.0561 118.3137) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5843 118.4985) (end 139.3254 118.3912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.8295 118.634) (end 139.5843 118.4985) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.0581 118.7962) (end 139.8295 118.634) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.2671 118.983) (end 140.0581 118.7962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.5171 121.2329) (end 140.2671 118.983) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.7038 121.4419) (end 142.5171 121.2329) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.866 121.6705) (end 142.7038 121.4419) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.0015 121.9157) (end 142.866 121.6705) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.1088 122.1746) (end 143.0015 121.9157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.1863 122.4439) (end 143.1088 122.1746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.2333 122.7202) (end 143.1863 122.4439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.2572 123.1568) (end 143.2333 122.7202) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.2818 123.312) (end 143.2572 123.1568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.3224 123.4638) (end 143.2818 123.312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.3787 123.6105) (end 143.3224 123.4638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.4501 123.7505) (end 143.3787 123.6105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.5356 123.8822) (end 143.4501 123.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.6345 124.0043) (end 143.5356 123.8822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.7457 124.1155) (end 143.6345 124.0043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.8677 124.2143) (end 143.7457 124.1155) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 143.9995 124.2999) (end 143.8677 124.2143) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.1395 124.3713) (end 143.9995 124.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.2862 124.4276) (end 144.1395 124.3713) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.4379 124.4682) (end 144.2862 124.4276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.5931 124.4928) (end 144.4379 124.4682) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.75 124.501) (end 144.5931 124.4928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.75 124.501) (end 144.75 124.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9069 124.4928) (end 146.75 124.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.0621 124.4682) (end 146.9069 124.4928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.2139 124.4275) (end 147.0621 124.4682) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.3606 124.3712) (end 147.2139 124.4275) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.5005 124.2999) (end 147.3606 124.3712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.6323 124.2143) (end 147.5005 124.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7544 124.1154) (end 147.6323 124.2143) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8655 124.0043) (end 147.7544 124.1154) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.9644 123.8822) (end 147.8655 124.0043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.0499 123.7505) (end 147.9644 123.8822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1213 123.6105) (end 148.0499 123.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.1776 123.4638) (end 148.1213 123.6105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.2182 123.312) (end 148.1776 123.4638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.2428 123.1569) (end 148.2182 123.312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.2667 122.7202) (end 148.2428 123.1569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.3137 122.4439) (end 148.2667 122.7202) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.3912 122.1746) (end 148.3137 122.4439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4985 121.9157) (end 148.3912 122.1746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.634 121.6705) (end 148.4985 121.9157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.7962 121.4419) (end 148.634 121.6705) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.983 121.2329) (end 148.7962 121.4419) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.2329 118.9829) (end 148.983 121.2329) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.4419 118.7962) (end 151.2329 118.9829) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.6705 118.634) (end 151.4419 118.7962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.9157 118.4985) (end 151.6705 118.634) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.1746 118.3912) (end 151.9157 118.4985) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.4439 118.3137) (end 152.1746 118.3912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.7202 118.2667) (end 152.4439 118.3137) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 153 118.251) (end 152.7202 118.2667) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164 118.251) (end 153 118.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.2612 118.2647) (end 164 118.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.5196 118.3056) (end 164.2612 118.2647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.7722 118.3733) (end 164.5196 118.3056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0164 118.4671) (end 164.7722 118.3733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.2495 118.5858) (end 165.0164 118.4671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.4689 118.7283) (end 165.2495 118.5858) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.6722 118.8929) (end 165.4689 118.7283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.8571 119.0778) (end 165.6722 118.8929) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.0217 119.2811) (end 165.8571 119.0778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.1642 119.5005) (end 166.0217 119.2811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.2829 119.7336) (end 166.1642 119.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.3767 119.9778) (end 166.2829 119.7336) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.4444 120.2304) (end 166.3767 119.9778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.4853 120.4888) (end 166.4444 120.2304) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.499 120.75) (end 166.4853 120.4888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.499 122.5001) (end 166.499 120.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.5127 122.7615) (end 166.499 122.5001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.5536 123.0199) (end 166.5127 122.7615) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.6214 123.2729) (end 166.5536 123.0199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.7152 123.5172) (end 166.6214 123.2729) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.834 123.7505) (end 166.7152 123.5172) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.9766 123.97) (end 166.834 123.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.1414 124.1735) (end 166.9766 123.97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.3265 124.3586) (end 167.1414 124.1735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.5299 124.5233) (end 167.3265 124.3586) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.7495 124.666) (end 167.5299 124.5233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 167.9828 124.7848) (end 167.7495 124.666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.2271 124.8786) (end 167.9828 124.7848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.4801 124.9464) (end 168.2271 124.8786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.7386 124.9873) (end 168.4801 124.9464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.9999 125.001) (end 168.7386 124.9873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.2615 124.9873) (end 168.9999 125.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.52 124.9463) (end 169.2615 124.9873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.7728 124.8786) (end 169.52 124.9463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.0173 124.7848) (end 169.7728 124.8786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.2505 124.6659) (end 170.0173 124.7848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.47 124.5234) (end 170.2505 124.6659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.6735 124.3586) (end 170.47 124.5234) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.8586 124.1735) (end 170.6735 124.3586) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.0234 123.97) (end 170.8586 124.1735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.166 123.7505) (end 171.0234 123.97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2848 123.5172) (end 171.166 123.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3786 123.2729) (end 171.2848 123.5172) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4464 123.0199) (end 171.3786 123.2729) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4873 122.7614) (end 171.4464 123.0199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.501 122.5) (end 171.4873 122.7614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.501 109.05) (end 171.501 122.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4994 109.0186) (end 171.501 109.05) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4944 108.9875) (end 171.4994 109.0186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4863 108.9569) (end 171.4944 108.9875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.475 108.9276) (end 171.4863 108.9569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4607 108.8995) (end 171.475 108.9276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4435 108.873) (end 171.4607 108.8995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4237 108.8486) (end 171.4435 108.873) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4014 108.8263) (end 171.4237 108.8486) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3769 108.8065) (end 171.4014 108.8263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3505 108.7894) (end 171.3769 108.8065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.3225 108.775) (end 171.3505 108.7894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.293 108.7637) (end 171.3225 108.775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2626 108.7556) (end 171.293 108.7637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2315 108.7507) (end 171.2626 108.7556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2 108.749) (end 171.2315 108.7507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.05 108.749) (end 171.2 108.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.9978 108.7463) (end 170.05 108.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.9463 108.7381) (end 169.9978 108.7463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.8958 108.7246) (end 169.9463 108.7381) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.847 108.7059) (end 169.8958 108.7246) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.8005 108.6821) (end 169.847 108.7059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.7567 108.6537) (end 169.8005 108.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.7161 108.6208) (end 169.7567 108.6537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.6792 108.5839) (end 169.7161 108.6208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.6463 108.5433) (end 169.6792 108.5839) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.6179 108.4995) (end 169.6463 108.5433) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5941 108.453) (end 169.6179 108.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5754 108.4042) (end 169.5941 108.453) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5619 108.3537) (end 169.5754 108.4042) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.5537 108.3022) (end 169.5619 108.3537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.551 108.25) (end 169.5537 108.3022) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.551 105.75) (end 169.551 108.25) (layer Edge.Cuts) (width 0.1))
  (gr_text IO0/~BOOT (at 169.5 116.5) (layer B.SilkS))
  (gr_text Reset (at 130.5 116.5) (layer B.SilkS))
  (gr_text JLCJLCJLCJLC (at 133.25 93.5 270) (layer B.SilkS))
  (gr_text neg2led.github.io/esp-pmsa (at 132.5 84.5 270) (layer F.SilkS))
  (gr_text v1.0 (at 129.5 80.5) (layer F.SilkS))
  (zone (net 18) (net_name Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.1905) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 172 125.5) (xy 128 125.5) (xy 128 74.5) (xy 131.25 74.5) (xy 139 82.25)
        (xy 161 82.25) (xy 168.75 74.5) (xy 172 74.5)
      )
    )
  )
  (zone (net 18) (net_name Board_1-GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.154))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 172 125.5) (xy 128 125.5) (xy 128 74.5) (xy 131.25 74.5) (xy 139 82.25)
        (xy 161 82.25) (xy 168.75 74.5) (xy 172 74.5)
      )
    )
  )
)
