(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6002)
    (drawings 1561)
    (tracks 668)
    (zones 0)
    (modules 153)
    (nets 107)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3175)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.762)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 0.9 0.4)
    (user_via 1 0.6)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.254)
    (pcb_text_width 0.254)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.127)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.1524)
    (pad_size 2.5 1.75)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 0 0)
    (grid_origin 100 77)
    (visible_elements 7FFFBFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-Board_1-+3V3)
  (net 2 Board_1-Board_1-+48V)
  (net 3 Board_1-Board_1-/CAN+)
  (net 4 Board_1-Board_1-/CAN-)
  (net 5 Board_1-Board_1-/CAN_RX)
  (net 6 Board_1-Board_1-/CAN_TX)
  (net 7 Board_1-Board_1-/LED_D)
  (net 8 Board_1-Board_1-/MTCK)
  (net 9 Board_1-Board_1-/MTDI)
  (net 10 Board_1-Board_1-/MTDO)
  (net 11 Board_1-Board_1-/MTMS)
  (net 12 Board_1-Board_1-/OLED_SCL)
  (net 13 Board_1-Board_1-/OLED_SDA)
  (net 14 Board_1-Board_1-/QW_SCL)
  (net 15 Board_1-Board_1-/QW_SDA)
  (net 16 Board_1-Board_1-/U0RXD)
  (net 17 Board_1-Board_1-/U0TXD)
  (net 18 Board_1-Board_1-/U1RX0)
  (net 19 Board_1-Board_1-/USB_D+)
  (net 20 Board_1-Board_1-/USB_D-)
  (net 21 Board_1-Board_1-/USB_ID)
  (net 22 Board_1-Board_1-/VBUS)
  (net 23 Board_1-Board_1-/VDD_SPI)
  (net 24 Board_1-Board_1-/VPP)
  (net 25 Board_1-Board_1-/xPSRAM_CS)
  (net 26 Board_1-Board_1-/~BOOT)
  (net 27 Board_1-Board_1-/~CAN_EN)
  (net 28 Board_1-Board_1-/~DFU)
  (net 29 Board_1-Board_1-/~RST)
  (net 30 Board_1-Board_1-/~SW_L)
  (net 31 Board_1-Board_1-/~SW_R)
  (net 32 Board_1-Board_1-/~SW_S)
  (net 33 Board_1-Board_1-GND)
  (net 34 Board_1-Board_1-GNDPWR)
  (net 35 "Board_1-Board_1-Net-(D2-Pad1)")
  (net 36 "Board_1-Board_1-Net-(D3-Pad1)")
  (net 37 "Board_1-Board_1-Net-(JP2-Pad1)")
  (net 38 "Board_1-Board_1-Net-(PS1-Pad4)")
  (net 39 "Board_1-Board_1-Net-(PS1-Pad6)")
  (net 40 "Board_1-Board_1-Net-(U1-Pad10)")
  (net 41 "Board_1-Board_1-Net-(U1-Pad11)")
  (net 42 "Board_1-Board_1-Net-(U1-Pad12)")
  (net 43 "Board_1-Board_1-Net-(U1-Pad13)")
  (net 44 "Board_1-Board_1-Net-(U1-Pad14)")
  (net 45 "Board_1-Board_1-Net-(U1-Pad15)")
  (net 46 "Board_1-Board_1-Net-(U1-Pad16)")
  (net 47 "Board_1-Board_1-Net-(U1-Pad17)")
  (net 48 "Board_1-Board_1-Net-(U1-Pad24)")
  (net 49 "Board_1-Board_1-Net-(U1-Pad27)")
  (net 50 "Board_1-Board_1-Net-(U1-Pad28)")
  (net 51 "Board_1-Board_1-Net-(U1-Pad6)")
  (net 52 "Board_1-Board_1-Net-(U1-Pad9)")
  (net 53 "Board_1-Board_1-Net-(U3-Pad4)")
  (net 54 Board_2-Board_1-+3V3)
  (net 55 Board_2-Board_1-+48V)
  (net 56 Board_2-Board_1-/CAN+)
  (net 57 Board_2-Board_1-/CAN-)
  (net 58 Board_2-Board_1-/CAN_RX)
  (net 59 Board_2-Board_1-/CAN_TX)
  (net 60 Board_2-Board_1-/LED_D)
  (net 61 Board_2-Board_1-/MTCK)
  (net 62 Board_2-Board_1-/MTDI)
  (net 63 Board_2-Board_1-/MTDO)
  (net 64 Board_2-Board_1-/MTMS)
  (net 65 Board_2-Board_1-/OLED_SCL)
  (net 66 Board_2-Board_1-/OLED_SDA)
  (net 67 Board_2-Board_1-/QW_SCL)
  (net 68 Board_2-Board_1-/QW_SDA)
  (net 69 Board_2-Board_1-/U0RXD)
  (net 70 Board_2-Board_1-/U0TXD)
  (net 71 Board_2-Board_1-/U1RX0)
  (net 72 Board_2-Board_1-/USB_D+)
  (net 73 Board_2-Board_1-/USB_D-)
  (net 74 Board_2-Board_1-/USB_ID)
  (net 75 Board_2-Board_1-/VBUS)
  (net 76 Board_2-Board_1-/VDD_SPI)
  (net 77 Board_2-Board_1-/VPP)
  (net 78 Board_2-Board_1-/xPSRAM_CS)
  (net 79 Board_2-Board_1-/~BOOT)
  (net 80 Board_2-Board_1-/~CAN_EN)
  (net 81 Board_2-Board_1-/~DFU)
  (net 82 Board_2-Board_1-/~RST)
  (net 83 Board_2-Board_1-/~SW_L)
  (net 84 Board_2-Board_1-/~SW_R)
  (net 85 Board_2-Board_1-/~SW_S)
  (net 86 Board_2-Board_1-GND)
  (net 87 Board_2-Board_1-GNDPWR)
  (net 88 "Board_2-Board_1-Net-(D2-Pad1)")
  (net 89 "Board_2-Board_1-Net-(D3-Pad1)")
  (net 90 "Board_2-Board_1-Net-(JP2-Pad1)")
  (net 91 "Board_2-Board_1-Net-(PS1-Pad4)")
  (net 92 "Board_2-Board_1-Net-(PS1-Pad6)")
  (net 93 "Board_2-Board_1-Net-(U1-Pad10)")
  (net 94 "Board_2-Board_1-Net-(U1-Pad11)")
  (net 95 "Board_2-Board_1-Net-(U1-Pad12)")
  (net 96 "Board_2-Board_1-Net-(U1-Pad13)")
  (net 97 "Board_2-Board_1-Net-(U1-Pad14)")
  (net 98 "Board_2-Board_1-Net-(U1-Pad15)")
  (net 99 "Board_2-Board_1-Net-(U1-Pad16)")
  (net 100 "Board_2-Board_1-Net-(U1-Pad17)")
  (net 101 "Board_2-Board_1-Net-(U1-Pad24)")
  (net 102 "Board_2-Board_1-Net-(U1-Pad27)")
  (net 103 "Board_2-Board_1-Net-(U1-Pad28)")
  (net 104 "Board_2-Board_1-Net-(U1-Pad6)")
  (net 105 "Board_2-Board_1-Net-(U1-Pad9)")
  (net 106 "Board_2-Board_1-Net-(U3-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-Board_1-+3V3)
    (add_net Board_1-Board_1-+48V)
    (add_net Board_1-Board_1-/CAN+)
    (add_net Board_1-Board_1-/CAN-)
    (add_net Board_1-Board_1-/CAN_RX)
    (add_net Board_1-Board_1-/CAN_TX)
    (add_net Board_1-Board_1-/LED_D)
    (add_net Board_1-Board_1-/MTCK)
    (add_net Board_1-Board_1-/MTDI)
    (add_net Board_1-Board_1-/MTDO)
    (add_net Board_1-Board_1-/MTMS)
    (add_net Board_1-Board_1-/OLED_SCL)
    (add_net Board_1-Board_1-/OLED_SDA)
    (add_net Board_1-Board_1-/QW_SCL)
    (add_net Board_1-Board_1-/QW_SDA)
    (add_net Board_1-Board_1-/U0RXD)
    (add_net Board_1-Board_1-/U0TXD)
    (add_net Board_1-Board_1-/U1RX0)
    (add_net Board_1-Board_1-/USB_D+)
    (add_net Board_1-Board_1-/USB_D-)
    (add_net Board_1-Board_1-/USB_ID)
    (add_net Board_1-Board_1-/VBUS)
    (add_net Board_1-Board_1-/VDD_SPI)
    (add_net Board_1-Board_1-/VPP)
    (add_net Board_1-Board_1-/xPSRAM_CS)
    (add_net Board_1-Board_1-/~BOOT)
    (add_net Board_1-Board_1-/~CAN_EN)
    (add_net Board_1-Board_1-/~DFU)
    (add_net Board_1-Board_1-/~RST)
    (add_net Board_1-Board_1-/~SW_L)
    (add_net Board_1-Board_1-/~SW_R)
    (add_net Board_1-Board_1-/~SW_S)
    (add_net Board_1-Board_1-GND)
    (add_net Board_1-Board_1-GNDPWR)
    (add_net "Board_1-Board_1-Net-(D2-Pad1)")
    (add_net "Board_1-Board_1-Net-(D3-Pad1)")
    (add_net "Board_1-Board_1-Net-(JP2-Pad1)")
    (add_net "Board_1-Board_1-Net-(PS1-Pad4)")
    (add_net "Board_1-Board_1-Net-(PS1-Pad6)")
    (add_net "Board_1-Board_1-Net-(U1-Pad10)")
    (add_net "Board_1-Board_1-Net-(U1-Pad11)")
    (add_net "Board_1-Board_1-Net-(U1-Pad12)")
    (add_net "Board_1-Board_1-Net-(U1-Pad13)")
    (add_net "Board_1-Board_1-Net-(U1-Pad14)")
    (add_net "Board_1-Board_1-Net-(U1-Pad15)")
    (add_net "Board_1-Board_1-Net-(U1-Pad16)")
    (add_net "Board_1-Board_1-Net-(U1-Pad17)")
    (add_net "Board_1-Board_1-Net-(U1-Pad24)")
    (add_net "Board_1-Board_1-Net-(U1-Pad27)")
    (add_net "Board_1-Board_1-Net-(U1-Pad28)")
    (add_net "Board_1-Board_1-Net-(U1-Pad6)")
    (add_net "Board_1-Board_1-Net-(U1-Pad9)")
    (add_net "Board_1-Board_1-Net-(U3-Pad4)")
    (add_net Board_2-Board_1-+3V3)
    (add_net Board_2-Board_1-+48V)
    (add_net Board_2-Board_1-/CAN+)
    (add_net Board_2-Board_1-/CAN-)
    (add_net Board_2-Board_1-/CAN_RX)
    (add_net Board_2-Board_1-/CAN_TX)
    (add_net Board_2-Board_1-/LED_D)
    (add_net Board_2-Board_1-/MTCK)
    (add_net Board_2-Board_1-/MTDI)
    (add_net Board_2-Board_1-/MTDO)
    (add_net Board_2-Board_1-/MTMS)
    (add_net Board_2-Board_1-/OLED_SCL)
    (add_net Board_2-Board_1-/OLED_SDA)
    (add_net Board_2-Board_1-/QW_SCL)
    (add_net Board_2-Board_1-/QW_SDA)
    (add_net Board_2-Board_1-/U0RXD)
    (add_net Board_2-Board_1-/U0TXD)
    (add_net Board_2-Board_1-/U1RX0)
    (add_net Board_2-Board_1-/USB_D+)
    (add_net Board_2-Board_1-/USB_D-)
    (add_net Board_2-Board_1-/USB_ID)
    (add_net Board_2-Board_1-/VBUS)
    (add_net Board_2-Board_1-/VDD_SPI)
    (add_net Board_2-Board_1-/VPP)
    (add_net Board_2-Board_1-/xPSRAM_CS)
    (add_net Board_2-Board_1-/~BOOT)
    (add_net Board_2-Board_1-/~CAN_EN)
    (add_net Board_2-Board_1-/~DFU)
    (add_net Board_2-Board_1-/~RST)
    (add_net Board_2-Board_1-/~SW_L)
    (add_net Board_2-Board_1-/~SW_R)
    (add_net Board_2-Board_1-/~SW_S)
    (add_net Board_2-Board_1-GND)
    (add_net Board_2-Board_1-GNDPWR)
    (add_net "Board_2-Board_1-Net-(D2-Pad1)")
    (add_net "Board_2-Board_1-Net-(D3-Pad1)")
    (add_net "Board_2-Board_1-Net-(JP2-Pad1)")
    (add_net "Board_2-Board_1-Net-(PS1-Pad4)")
    (add_net "Board_2-Board_1-Net-(PS1-Pad6)")
    (add_net "Board_2-Board_1-Net-(U1-Pad10)")
    (add_net "Board_2-Board_1-Net-(U1-Pad11)")
    (add_net "Board_2-Board_1-Net-(U1-Pad12)")
    (add_net "Board_2-Board_1-Net-(U1-Pad13)")
    (add_net "Board_2-Board_1-Net-(U1-Pad14)")
    (add_net "Board_2-Board_1-Net-(U1-Pad15)")
    (add_net "Board_2-Board_1-Net-(U1-Pad16)")
    (add_net "Board_2-Board_1-Net-(U1-Pad17)")
    (add_net "Board_2-Board_1-Net-(U1-Pad24)")
    (add_net "Board_2-Board_1-Net-(U1-Pad27)")
    (add_net "Board_2-Board_1-Net-(U1-Pad28)")
    (add_net "Board_2-Board_1-Net-(U1-Pad6)")
    (add_net "Board_2-Board_1-Net-(U1-Pad9)")
    (add_net "Board_2-Board_1-Net-(U3-Pad4)")
  )
  (net_class USB_D ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class VCC ""
    (clearance 0.127)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class VIN ""
    (clearance 0.254)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.127)
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 111.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 110.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 109.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 108.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 107.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 106.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 106.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 107.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 108.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 109.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 110.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 111.753028)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 71.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 70.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 69.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 68.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 67.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 109.753 66.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 66.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 67.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 68.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 69.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 70.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.249 71.251009)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.834752 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.834752 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 92.834752 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 93.834752 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.834752 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 95.834752 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.167376 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.167376 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.167376 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.167376 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 73.167376 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 74.167376 127.755)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 95.834752 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.834752 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 93.834752 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 92.834752 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.834752 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.834752 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 74.167376 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 73.167376 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.167376 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.167376 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.167376 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.167376 90.751)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.834752 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.834752 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 92.834752 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 93.834752 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.834752 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 95.834752 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.167376 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.167376 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.167376 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.167376 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 73.167376 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 74.167376 87.253)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 95.834752 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.834752 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 93.834752 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 92.834752 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 91.834752 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 90.834752 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 74.167376 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 73.167376 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 72.167376 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 71.167376 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 70.167376 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 69.167376 50.249)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.001065 131.502019)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 115.001064 46.502019)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 50.001065 46.502019)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu))
  )
  (module Fiducial (layer B.Cu) (tedit 5EA93A7C)
    (at 55.001065 131.502019)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value Fiducial (at 0 -1.5) (layer B.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer F.Cu) (tedit 5EA93A7C)
    (at 55.001065 131.502019)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 1.5) (layer F.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer B.Cu) (tedit 5EA93A7C)
    (at 110.001064 46.502019)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value Fiducial (at 0 -1.5) (layer B.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer F.Cu) (tedit 5EA93A7C)
    (at 110.001064 46.502019)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 1.5) (layer F.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer B.Cu) (tedit 5EA93A7C)
    (at 55.001065 46.502019)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value Fiducial (at 0 -1.5) (layer B.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer F.Cu) (tedit 5EA93A7C)
    (at 55.001065 46.502019)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 1.5) (layer F.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module 41-EasyEDA-Edits:MICRO-USB-SMD_U254-051T-4BH83-F1S_C397452 (layer F.Cu) (tedit 6045F2E8)
    (at 78.751001 92.50302 180)
    (attr smd)
    (fp_text reference USB1 (at 0 -3) (layer F.SilkS))
    (fp_text value USB (at 0 5.252001) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.375) (layer Dwgs.User))
    (pad 1 smd rect (at -1.3 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 75 Board_2-Board_1-/VBUS))
    (pad 2 smd rect (at -0.65 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 73 Board_2-Board_1-/USB_D-))
    (pad 3 smd rect (at 0 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 72 Board_2-Board_1-/USB_D+))
    (pad 4 smd rect (at 0.65 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 74 Board_2-Board_1-/USB_ID))
    (pad 5 smd rect (at 1.3 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 6 smd rect (at 3.1 -2.225 270) (size 1.6 2.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 6 smd rect (at -3.1 -2.225 270) (size 1.6 2.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 6 thru_hole oval (at -2.83 0.325) (size 1.5 2) (drill oval 0.9 1.4) (layers *.Cu *.Paste *.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 6 thru_hole oval (at 2.83 0.325 180) (size 1.5 2) (drill oval 0.9 1.4) (layers *.Cu *.Paste *.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad "" np_thru_hole circle (at 2 -2.025 180) (size 0.5 0.5) (drill 0.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2 -2.025 180) (size 0.45 0.45) (drill 0.45) (layers *.Cu *.Mask))
    (model ${EASY_EDA_3D}/EasyEDA.3dshapes/MICRO-USB-SMD_U254-051T-4BH83-F1S.wrl
      (offset (xyz 0 0 1.25))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module 11-My-Edits:Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_Horizontal_3D (layer F.Cu) (tedit 6045D355)
    (at 62.501001 103.50302)
    (descr "Molex Nano-Fit Power Connectors, 105313-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053131208_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit top entry")
    (fp_text reference J1 (at -6.875 0 180) (layer F.SilkS))
    (fp_text value CANBUS (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 4.77 -6.15 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 3.75 -7.18 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.75 -7.18 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 3.75 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 87 Board_2-Board_1-GNDPWR))
    (pad 3 thru_hole oval (at 1.25 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 57 Board_2-Board_1-/CAN-))
    (pad 2 thru_hole oval (at -1.25 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 56 Board_2-Board_1-/CAN+))
    (pad 1 thru_hole roundrect (at -3.75 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 55 Board_2-Board_1-+48V))
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_PTH_Clips_Horz.step
      (offset (xyz 0 6.15 2.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module NetTie:NetTie-2_SMD_Pad0.5mm (layer F.Cu) (tedit 6045BC89)
    (at 67.151001 103.50302)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 1.95 0 90) (layer F.Fab) hide)
    (fp_text value GND_TIE (at 0 1.2) (layer F.Fab))
    (pad 2 smd circle (at 0.5 0) (size 0.5 0.5) (layers F.Cu)
      (net 86 Board_2-Board_1-GND) (clearance 0.001) (zone_connect 2))
    (pad 1 smd circle (at -0.5 0) (size 0.5 0.5) (layers F.Cu)
      (net 87 Board_2-Board_1-GNDPWR))
  )
  (module 11-My-Edits:Gecko-G125_PlusTC2030_IDCBox_2x03_P1.25mm_Vertical_3D (layer F.Cu) (tedit 6045B3A6)
    (at 80.116001 117.13302 90)
    (descr "Harwin Gecko Connector, 6 pins, dual row male, vertical entry, no latches, PN:G125-MVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at -2.75 3.375 90) (layer F.SilkS))
    (fp_text value ESP-PROG (at 0 -3.675 90) (layer F.Fab))
    (fp_text user KEEPOUT (at 0 0.025 90) (layer Cmts.User))
    (pad 3 thru_hole oval (at 0 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 70 Board_2-Board_1-/U0TXD))
    (pad 1 thru_hole rect (at -1.27 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 82 Board_2-Board_1-/~RST))
    (pad 4 thru_hole oval (at 0 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 5 thru_hole oval (at 1.27 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 69 Board_2-Board_1-/U0RXD))
    (pad 6 thru_hole oval (at 1.27 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 79 Board_2-Board_1-/~BOOT))
    (pad 2 thru_hole oval (at -1.27 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 77 Board_2-Board_1-/VPP))
    (pad "" np_thru_hole circle (at -2.54 0 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/shapes3D/g125-mv10605l0_asm.stp
      (offset (xyz 0 0 1.925))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 78.751001 109.37802 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.65 90) (layer F.Fab))
    (fp_text value VPP_EN (at 0.025 -1.85 90) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 77 Board_2-Board_1-/VPP) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 54 Board_2-Board_1-+3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module 10-My-Footprints:OLED_SSD1315_128x64_1.3_I2C_New_Silhouette_Big3D locked (layer F.Cu) (tedit 603CB3FF)
    (at 95.696001 106.87802)
    (fp_text reference I2C1 (at 0 -0.75) (layer F.Fab))
    (fp_text value OLED (at 0 0.75) (layer F.Fab))
    (fp_text user "VCC/GND switchable via 0R jumpers on rear" (at 0 -11.25) (layer Cmts.User))
    (fp_text user "GND VCC SCL SDA" (at 0 -12.75) (layer Cmts.User))
    (fp_text user "Visible Area" (at 0 -1.75) (layer Cmts.User))
    (pad 3 thru_hole oval (at 1.28 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 Board_2-Board_1-/OLED_SCL))
    (pad 1 thru_hole rect (at -3.8 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 4 thru_hole oval (at 3.82 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 Board_2-Board_1-/OLED_SDA))
    (pad 2 thru_hole oval (at -1.26 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 Board_2-Board_1-+3V3))
    (model "${KIPRJMOD}/shapes3D/Oled SH1106.wrl"
      (offset (xyz 0 0.3 8.800000000000001))
      (scale (xyz 0.36 0.36 0.36))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal_3D locked (layer F.Cu) (tedit 6045B770)
    (at 104.876001 93.80302 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J3 (at 3 -2.625) (layer F.SilkS))
    (fp_text value Qwiic (at 0 3.98) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad MP smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208)
      (net 86 Board_2-Board_1-GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.2))
    (pad MP smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208)
      (net 86 Board_2-Board_1-GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.2))
    (pad 4 smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (pad 3 smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (pad 2 smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 68 Board_2-Board_1-/QW_SDA))
    (pad 1 smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 67 Board_2-Board_1-/QW_SCL))
    (model ${KIPRJMOD}/shapes3D/SM04B-SRSS-TB.STEP
      (offset (xyz 0 1.325 -0.32))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 95.751001 125.50302)
    (attr smd)
    (fp_text reference SW4 (at 0.025 -0.025 180) (layer F.SilkS))
    (fp_text value SEL (at 0 2.05) (layer F.Fab) hide)
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 85 Board_2-Board_1-/~SW_S))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 85 Board_2-Board_1-/~SW_S))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 110.001001 96.75302 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.25) (layer F.SilkS))
    (fp_text value 22uF (at -1.85 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm_3D (layer F.Cu) (tedit 603F44B0)
    (at 112.501001 120.25302 270)
    (descr https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf)
    (tags "LED RGB NeoPixel Mini")
    (attr smd)
    (fp_text reference D3 (at 0 2.625 270) (layer F.SilkS))
    (fp_text value SK6812MINI (at 0 2.625 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.75 -0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 89 "Board_2-Board_1-Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1.75 0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 4 smd rect (at 1.75 -0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 54 Board_2-Board_1-+3V3))
    (pad 3 smd rect (at 1.75 0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 60 Board_2-Board_1-/LED_D))
    (model "${KIPRJMOD}/shapes3D/SMD3535 RGB.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:Converter_DCDC_TDK-Lambda_CC3-xxxxxF-E locked (layer F.Cu) (tedit 6045D39C)
    (at 63.751001 114.00302)
    (fp_text reference PS1 (at -12.5 -1.5 270) (layer F.SilkS))
    (fp_text value CC3-4803SF-E (at 0 6) (layer F.Fab))
    (pad MP2 thru_hole oval (at 8.89 -8) (size 2.5 1.75) (drill oval 1.5 0.75) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad MP thru_hole oval (at -8.89 8) (size 2.5 1.75) (drill oval 1.5 0.75) (layers *.Cu *.Mask)
      (net 87 Board_2-Board_1-GNDPWR))
    (pad 4 thru_hole circle (at 11.43 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 91 "Board_2-Board_1-Net-(PS1-Pad4)"))
    (pad 5 thru_hole circle (at 11.43 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 6 thru_hole circle (at 11.43 -2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 92 "Board_2-Board_1-Net-(PS1-Pad6)"))
    (pad 7 thru_hole circle (at 11.43 -5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 54 Board_2-Board_1-+3V3))
    (pad 3 thru_hole circle (at -11.43 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 Board_2-Board_1-GNDPWR))
    (pad 2 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 87 Board_2-Board_1-GNDPWR))
    (pad 1 thru_hole circle (at -11.43 -5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 55 Board_2-Board_1-+48V))
    (model ${KIPRJMOD}/shapes3D/cc3-f-e_outline.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 92.126001 126.12302 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.925 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 85 Board_2-Board_1-/~SW_S))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 89.376001 94.00302 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.925 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.376001 93.98302 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.93 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 Board_2-Board_1-/VBUS))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 86.876001 94.37802 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -2.5 0) (layer F.SilkS))
    (fp_text value XC6220B331MR (at 2.325 0 180) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 54 Board_2-Board_1-+3V3))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 106 "Board_2-Board_1-Net-(U3-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 Board_2-Board_1-/VBUS))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 75 Board_2-Board_1-/VBUS))
    (model ${KIPRJMOD}/shapes3D/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 61.501001 125.50302)
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.SilkS))
    (fp_text value BOOT (at 0 -2.375) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 79 Board_2-Board_1-/~BOOT))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 79 Board_2-Board_1-/~BOOT))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 85.751001 125.50302)
    (attr smd)
    (fp_text reference SW3 (at 0 0) (layer F.SilkS))
    (fp_text value LEFT (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 83 Board_2-Board_1-/~SW_L))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 83 Board_2-Board_1-/~SW_L))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 70.501001 125.50302)
    (attr smd)
    (fp_text reference SW1 (at 0 0 180) (layer F.SilkS))
    (fp_text value RST (at 0 -2.375) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 82 Board_2-Board_1-/~RST))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 82 Board_2-Board_1-/~RST))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 105.751001 125.50302)
    (attr smd)
    (fp_text reference SW5 (at 0 0) (layer F.SilkS))
    (fp_text value RIGHT (at 0 -2) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 84 Board_2-Board_1-/~SW_R))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 84 Board_2-Board_1-/~SW_R))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.126001 126.12302 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 84 Board_2-Board_1-/~SW_R))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 82.126001 126.12302 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 83 Board_2-Board_1-/~SW_L))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.321001 103.50302)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.51 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 1) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 53.126001 101.12802 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.625 180) (layer F.SilkS))
    (fp_text value 120R (at 0 -1.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 90 "Board_2-Board_1-Net-(JP2-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 56 Board_2-Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 53.126001 98.25302 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.85 270) (layer F.SilkS) hide)
    (fp_text value CAN_T (at 0 -1.9 270) (layer F.SilkS))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 90 "Board_2-Board_1-Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 57 Board_2-Board_1-/CAN-) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 112.501001 125.50302 180)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H4 (at 0 -3.25) (layer F.Fab) hide)
    (fp_text value MP (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 112.501001 93.00302 180)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H3 (at 0 -0.55) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 52.501001 125.50302)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H2 (at 0 -0.75) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 52.501001 93.00302)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H1 (at 0 -0.55) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 86 Board_2-Board_1-GND) (zone_connect 2))
  )
  (module 10-My-Footprints:LED_0603_1608Metric_SnapModel (layer F.Cu) (tedit 5FFD7569)
    (at 71.876001 93.62802)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer F.Fab) hide)
    (fp_text value PWR (at 0 -1.425 180) (layer F.SilkS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Board_2-Board_1-Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/LTST-C193TBKT-5A.step
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "10-My-Footprints:ESP32-S2-WROVER_and_WROOM(PCB,-I(IPEX))-Universal" (layer F.Cu) (tedit 6034B573)
    (at 100.001001 107.74302 270)
    (fp_text reference U1 (at -8.5 17 270) (layer F.SilkS))
    (fp_text value ESP32-S2-WROVER (at 0 11.25 90) (layer F.Fab))
    (fp_text user "!!! Keepout Area !!!" (at 0.01 -10.5 90) (layer Dwgs.User))
    (fp_text user 17 (at -6.49 13 315 unlocked) (layer F.SilkS))
    (fp_text user o (at -9.779 -8.8646 270) (layer F.SilkS))
    (fp_text user 26 (at 6.51 13 225 unlocked) (layer F.SilkS))
    (fp_text user "!!! Keepout Area !!!" (at 0.01 -14.5 90) (layer Dwgs.User))
    (fp_text user 42 (at 6.75 -8 315 unlocked) (layer F.SilkS))
    (fp_text user ANTENNA (at 0.01 -12.5 90) (layer F.SilkS))
    (fp_text user 1 (at -6.75 -8.001 225 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -8.75 -8 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 3 smd rect (at -8.75 -5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 79 Board_2-Board_1-/~BOOT))
    (pad 43 thru_hole rect (at -1.19 0.05 270) (size 1.4 1.4) (drill 1.2) (layers *.Cu *.Mask F.Paste)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 2 smd rect (at -8.75 -6.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 Board_2-Board_1-+3V3))
    (pad 43 smd rect (at -1.19 0.05 270) (size 4.1 4.1) (layers F.Cu F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 34 smd rect (at 8.75 4 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 Board_2-Board_1-/MTDO))
    (pad 25 smd rect (at 5.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 78 Board_2-Board_1-/xPSRAM_CS))
    (pad 42 smd rect (at 8.75 -8 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 39 smd rect (at 8.75 -3.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 Board_2-Board_1-/VDD_SPI))
    (pad 14 smd rect (at -8.75 11.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 97 "Board_2-Board_1-Net-(U1-Pad14)"))
    (pad 35 smd rect (at 8.75 2.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 Board_2-Board_1-/MTDI))
    (pad 40 smd rect (at 8.75 -5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 81 Board_2-Board_1-/~DFU))
    (pad 11 smd rect (at -8.75 7 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 94 "Board_2-Board_1-Net-(U1-Pad11)"))
    (pad 20 smd rect (at -2.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 80 Board_2-Board_1-/~CAN_EN))
    (pad 24 smd rect (at 3.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 101 "Board_2-Board_1-Net-(U1-Pad24)"))
    (pad 26 smd rect (at 6.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND))
    (pad 43 smd rect (at -2.69 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 smd rect (at -2.69 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 19 smd rect (at -3.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 58 Board_2-Board_1-/CAN_RX))
    (pad 43 thru_hole circle (at -1.94 -1.45 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 23 smd rect (at 2.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 72 Board_2-Board_1-/USB_D+))
    (pad 43 thru_hole circle (at -0.44 -1.45 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 43 thru_hole circle (at -2.69 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 9 smd rect (at -8.75 4 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 105 "Board_2-Board_1-Net-(U1-Pad9)"))
    (pad 43 thru_hole circle (at 0.31 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 41 smd rect (at 8.75 -6.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 82 Board_2-Board_1-/~RST))
    (pad 16 smd rect (at -8.75 14.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 99 "Board_2-Board_1-Net-(U1-Pad16)"))
    (pad 43 thru_hole circle (at 0.31 0.8 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 30 smd rect (at 8.75 10 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 85 Board_2-Board_1-/~SW_S))
    (pad 12 smd rect (at -8.75 8.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 95 "Board_2-Board_1-Net-(U1-Pad12)"))
    (pad 36 smd rect (at 8.75 1 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 64 Board_2-Board_1-/MTMS))
    (pad 10 smd rect (at -8.75 5.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 93 "Board_2-Board_1-Net-(U1-Pad10)"))
    (pad 15 smd rect (at -8.75 13 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 98 "Board_2-Board_1-Net-(U1-Pad15)"))
    (pad 21 smd rect (at -0.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 71 Board_2-Board_1-/U1RX0))
    (pad 43 smd rect (at -2.69 0.05 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 smd rect (at 0.31 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 38 smd rect (at 8.75 -2 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 Board_2-Board_1-/U0RXD))
    (pad 4 smd rect (at -8.75 -3.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 Board_2-Board_1-/QW_SCL))
    (pad 43 smd rect (at 0.31 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 thru_hole circle (at -2.69 0.8 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 22 smd rect (at 0.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 73 Board_2-Board_1-/USB_D-))
    (pad 6 smd rect (at -8.75 -0.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 104 "Board_2-Board_1-Net-(U1-Pad6)"))
    (pad 31 smd rect (at 8.75 8.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 84 Board_2-Board_1-/~SW_R))
    (pad 43 smd rect (at -1.19 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 27 smd rect (at 8.75 14.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 102 "Board_2-Board_1-Net-(U1-Pad27)"))
    (pad 18 smd rect (at -5.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 59 Board_2-Board_1-/CAN_TX))
    (pad 13 smd rect (at -8.75 10 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 96 "Board_2-Board_1-Net-(U1-Pad13)"))
    (pad 43 smd rect (at -1.19 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 37 smd rect (at 8.75 -0.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 Board_2-Board_1-/U0TXD))
    (pad 8 smd rect (at -8.75 2.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 Board_2-Board_1-/OLED_SCL))
    (pad 43 thru_hole circle (at -0.44 1.55 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 5 smd rect (at -8.75 -2 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 Board_2-Board_1-/QW_SDA))
    (pad 28 smd rect (at 8.75 13 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 103 "Board_2-Board_1-Net-(U1-Pad28)"))
    (pad 43 smd rect (at 0.31 0.05 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 86 Board_2-Board_1-GND) (solder_paste_margin -0.001))
    (pad 17 smd rect (at -6.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 100 "Board_2-Board_1-Net-(U1-Pad17)"))
    (pad 7 smd rect (at -8.75 1 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 Board_2-Board_1-/OLED_SDA))
    (pad 29 smd rect (at 8.75 11.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 83 Board_2-Board_1-/~SW_L))
    (pad 33 smd rect (at 8.75 5.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 61 Board_2-Board_1-/MTCK))
    (pad 43 thru_hole circle (at -1.94 1.55 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 86 Board_2-Board_1-GND))
    (pad 32 smd rect (at 8.75 7 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 60 Board_2-Board_1-/LED_D))
    (model ${KIPRJMOD}/shapes3D/ESP32-S2-WROVER-I.STEP
      (offset (xyz -9 -15.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:neggle-logo-0.12 (layer B.Cu) (tedit 602F09FF)
    (at 65.926001 118.00302 180)
    (fp_text reference LOGO1 (at 0 -0.5 180) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0 0.5 180) (layer B.Fab) hide)
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 73.751001 100.00302 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0 3.3) (layer F.SilkS))
    (fp_text value MAX3051ESA (at 0 -1.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (pad 7 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 Board_2-Board_1-/CAN+))
    (pad 6 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 Board_2-Board_1-/CAN-))
    (pad 5 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 80 Board_2-Board_1-/~CAN_EN))
    (pad 4 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 Board_2-Board_1-/CAN_RX))
    (pad 3 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (pad 2 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (pad 1 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 59 Board_2-Board_1-/CAN_TX))
    (model ${KIPRJMOD}/shapes3D/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.601001 95.07802 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1.55 0) (layer F.SilkS))
    (fp_text value 1K (at 0 -0.875) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 88 "Board_2-Board_1-Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.251001 119.12802)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.375) (layer F.SilkS))
    (fp_text value 10uF (at 0 -1.125) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 Board_2-Board_1-/~RST))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.876001 126.12302 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at -0.005 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 79 Board_2-Board_1-/~BOOT))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 86 Board_2-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 66.876001 126.12302 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.945 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0.875 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 82 Board_2-Board_1-/~RST))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 Board_2-Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 41-EasyEDA-Edits:MICRO-USB-SMD_U254-051T-4BH83-F1S_C397452 (layer F.Cu) (tedit 6045F2E8)
    (at 78.751001 52.001001 180)
    (attr smd)
    (fp_text reference USB1 (at 0 -3) (layer F.SilkS))
    (fp_text value USB (at 0 5.252001) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.375) (layer Dwgs.User))
    (pad 1 smd rect (at -1.3 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 22 Board_1-Board_1-/VBUS))
    (pad 2 smd rect (at -0.65 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 20 Board_1-Board_1-/USB_D-))
    (pad 3 smd rect (at 0 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 Board_1-Board_1-/USB_D+))
    (pad 4 smd rect (at 0.65 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 21 Board_1-Board_1-/USB_ID))
    (pad 5 smd rect (at 1.3 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 6 smd rect (at 3.1 -2.225 270) (size 1.6 2.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 6 smd rect (at -3.1 -2.225 270) (size 1.6 2.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 6 thru_hole oval (at -2.83 0.325) (size 1.5 2) (drill oval 0.9 1.4) (layers *.Cu *.Paste *.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 6 thru_hole oval (at 2.83 0.325 180) (size 1.5 2) (drill oval 0.9 1.4) (layers *.Cu *.Paste *.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad "" np_thru_hole circle (at 2 -2.025 180) (size 0.5 0.5) (drill 0.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2 -2.025 180) (size 0.45 0.45) (drill 0.45) (layers *.Cu *.Mask))
    (model ${EASY_EDA_3D}/EasyEDA.3dshapes/MICRO-USB-SMD_U254-051T-4BH83-F1S.wrl
      (offset (xyz 0 0 1.25))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module 11-My-Edits:Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_Horizontal_3D (layer F.Cu) (tedit 6045D355)
    (at 62.501001 63.001001)
    (descr "Molex Nano-Fit Power Connectors, 105313-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053131208_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit top entry")
    (fp_text reference J1 (at -6.875 0 180) (layer F.SilkS))
    (fp_text value CANBUS (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 4.77 -6.15 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 3.75 -7.18 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -3.75 -7.18 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 3.75 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 Board_1-Board_1-GNDPWR))
    (pad 3 thru_hole oval (at 1.25 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 Board_1-Board_1-/CAN-))
    (pad 2 thru_hole oval (at -1.25 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 Board_1-Board_1-/CAN+))
    (pad 1 thru_hole roundrect (at -3.75 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 Board_1-Board_1-+48V))
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_PTH_Clips_Horz.step
      (offset (xyz 0 6.15 2.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module NetTie:NetTie-2_SMD_Pad0.5mm (layer F.Cu) (tedit 6045BC89)
    (at 67.151001 63.001001)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 1.95 0 90) (layer F.Fab) hide)
    (fp_text value GND_TIE (at 0 1.2) (layer F.Fab))
    (pad 2 smd circle (at 0.5 0) (size 0.5 0.5) (layers F.Cu)
      (net 33 Board_1-Board_1-GND) (clearance 0.001) (zone_connect 2))
    (pad 1 smd circle (at -0.5 0) (size 0.5 0.5) (layers F.Cu)
      (net 34 Board_1-Board_1-GNDPWR))
  )
  (module 11-My-Edits:Gecko-G125_PlusTC2030_IDCBox_2x03_P1.25mm_Vertical_3D (layer F.Cu) (tedit 6045B3A6)
    (at 80.116001 76.631001 90)
    (descr "Harwin Gecko Connector, 6 pins, dual row male, vertical entry, no latches, PN:G125-MVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at -2.75 3.375 90) (layer F.SilkS))
    (fp_text value ESP-PROG (at 0 -3.675 90) (layer F.Fab))
    (fp_text user KEEPOUT (at 0 0.025 90) (layer Cmts.User))
    (pad 3 thru_hole oval (at 0 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 Board_1-Board_1-/U0TXD))
    (pad 1 thru_hole rect (at -1.27 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 Board_1-Board_1-/~RST))
    (pad 4 thru_hole oval (at 0 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 5 thru_hole oval (at 1.27 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 Board_1-Board_1-/U0RXD))
    (pad 6 thru_hole oval (at 1.27 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 Board_1-Board_1-/~BOOT))
    (pad 2 thru_hole oval (at -1.27 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 Board_1-Board_1-/VPP))
    (pad "" np_thru_hole circle (at -2.54 0 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 1.016 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/shapes3D/g125-mv10605l0_asm.stp
      (offset (xyz 0 0 1.925))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 78.751001 68.876001 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.65 90) (layer F.Fab))
    (fp_text value VPP_EN (at 0.025 -1.85 90) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 24 Board_1-Board_1-/VPP) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 Board_1-Board_1-+3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module 10-My-Footprints:OLED_SSD1315_128x64_1.3_I2C_New_Silhouette_Big3D locked (layer F.Cu) (tedit 603CB3FF)
    (at 95.696001 66.376001)
    (fp_text reference I2C1 (at 0 -0.75) (layer F.Fab))
    (fp_text value OLED (at 0 0.75) (layer F.Fab))
    (fp_text user "VCC/GND switchable via 0R jumpers on rear" (at 0 -11.25) (layer Cmts.User))
    (fp_text user "GND VCC SCL SDA" (at 0 -12.75) (layer Cmts.User))
    (fp_text user "Visible Area" (at 0 -1.75) (layer Cmts.User))
    (pad 3 thru_hole oval (at 1.28 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 Board_1-Board_1-/OLED_SCL))
    (pad 1 thru_hole rect (at -3.8 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 4 thru_hole oval (at 3.82 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 Board_1-Board_1-/OLED_SDA))
    (pad 2 thru_hole oval (at -1.26 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Board_1-Board_1-+3V3))
    (model "${KIPRJMOD}/shapes3D/Oled SH1106.wrl"
      (offset (xyz 0 0.3 8.800000000000001))
      (scale (xyz 0.36 0.36 0.36))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal_3D locked (layer F.Cu) (tedit 6045B770)
    (at 104.876001 53.301001 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J3 (at 3 -2.625) (layer F.SilkS))
    (fp_text value Qwiic (at 0 3.98) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad MP smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208)
      (net 33 Board_1-Board_1-GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.2))
    (pad MP smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208)
      (net 33 Board_1-Board_1-GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.2))
    (pad 4 smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (pad 3 smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (pad 2 smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 Board_1-Board_1-/QW_SDA))
    (pad 1 smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-Board_1-/QW_SCL))
    (model ${KIPRJMOD}/shapes3D/SM04B-SRSS-TB.STEP
      (offset (xyz 0 1.325 -0.32))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 95.751001 85.001001)
    (attr smd)
    (fp_text reference SW4 (at 0.025 -0.025 180) (layer F.SilkS))
    (fp_text value SEL (at 0 2.05) (layer F.Fab) hide)
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_1-Board_1-/~SW_S))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_1-Board_1-/~SW_S))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 110.001001 56.251001 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.25) (layer F.SilkS))
    (fp_text value 22uF (at -1.85 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm_3D (layer F.Cu) (tedit 603F44B0)
    (at 112.501001 79.751001 270)
    (descr https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf)
    (tags "LED RGB NeoPixel Mini")
    (attr smd)
    (fp_text reference D3 (at 0 2.625 270) (layer F.SilkS))
    (fp_text value SK6812MINI (at 0 2.625 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.75 -0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 36 "Board_1-Board_1-Net-(D3-Pad1)"))
    (pad 2 smd rect (at -1.75 0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 4 smd rect (at 1.75 -0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-Board_1-+3V3))
    (pad 3 smd rect (at 1.75 0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-Board_1-/LED_D))
    (model "${KIPRJMOD}/shapes3D/SMD3535 RGB.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:Converter_DCDC_TDK-Lambda_CC3-xxxxxF-E locked (layer F.Cu) (tedit 6045D39C)
    (at 63.751001 73.501001)
    (fp_text reference PS1 (at -12.5 -1.5 270) (layer F.SilkS))
    (fp_text value CC3-4803SF-E (at 0 6) (layer F.Fab))
    (pad MP2 thru_hole oval (at 8.89 -8) (size 2.5 1.75) (drill oval 1.5 0.75) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad MP thru_hole oval (at -8.89 8) (size 2.5 1.75) (drill oval 1.5 0.75) (layers *.Cu *.Mask)
      (net 34 Board_1-Board_1-GNDPWR))
    (pad 4 thru_hole circle (at 11.43 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Board_1-Board_1-Net-(PS1-Pad4)"))
    (pad 5 thru_hole circle (at 11.43 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 6 thru_hole circle (at 11.43 -2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Board_1-Board_1-Net-(PS1-Pad6)"))
    (pad 7 thru_hole circle (at 11.43 -5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 Board_1-Board_1-+3V3))
    (pad 3 thru_hole circle (at -11.43 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 34 Board_1-Board_1-GNDPWR))
    (pad 2 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 34 Board_1-Board_1-GNDPWR))
    (pad 1 thru_hole circle (at -11.43 -5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 Board_1-Board_1-+48V))
    (model ${KIPRJMOD}/shapes3D/cc3-f-e_outline.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 92.126001 85.621001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.925 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 Board_1-Board_1-/~SW_S))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 89.376001 53.501001 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.925 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 84.376001 53.481001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.93 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 Board_1-Board_1-/VBUS))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 86.876001 53.876001 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -2.5 0) (layer F.SilkS))
    (fp_text value XC6220B331MR (at 2.325 0 180) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-Board_1-+3V3))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 "Board_1-Board_1-Net-(U3-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 Board_1-Board_1-/VBUS))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 Board_1-Board_1-/VBUS))
    (model ${KIPRJMOD}/shapes3D/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 61.501001 85.001001)
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.SilkS))
    (fp_text value BOOT (at 0 -2.375) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 Board_1-Board_1-/~BOOT))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 Board_1-Board_1-/~BOOT))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 85.751001 85.001001)
    (attr smd)
    (fp_text reference SW3 (at 0 0) (layer F.SilkS))
    (fp_text value LEFT (at 0 -2) (layer F.Fab))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 Board_1-Board_1-/~SW_L))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 Board_1-Board_1-/~SW_L))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 70.501001 85.001001)
    (attr smd)
    (fp_text reference SW1 (at 0 0 180) (layer F.SilkS))
    (fp_text value RST (at 0 -2.375) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 Board_1-Board_1-/~RST))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 Board_1-Board_1-/~RST))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 105.751001 85.001001)
    (attr smd)
    (fp_text reference SW5 (at 0 0) (layer F.SilkS))
    (fp_text value RIGHT (at 0 -2) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 Board_1-Board_1-/~SW_R))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 Board_1-Board_1-/~SW_R))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 102.126001 85.621001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 Board_1-Board_1-/~SW_R))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 82.126001 85.621001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 Board_1-Board_1-/~SW_L))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 74.321001 63.001001)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.51 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 1) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 53.126001 60.626001 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.625 180) (layer F.SilkS))
    (fp_text value 120R (at 0 -1.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 "Board_1-Board_1-Net-(JP2-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Board_1-Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 53.126001 57.751001 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.85 270) (layer F.SilkS) hide)
    (fp_text value CAN_T (at 0 -1.9 270) (layer F.SilkS))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 37 "Board_1-Board_1-Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 4 Board_1-Board_1-/CAN-) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 112.501001 85.001001 180)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H4 (at 0 -3.25) (layer F.Fab) hide)
    (fp_text value MP (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 112.501001 52.501001 180)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H3 (at 0 -0.55) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 52.501001 85.001001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H2 (at 0 -0.75) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 52.501001 52.501001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H1 (at 0 -0.55) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-Board_1-GND) (zone_connect 2))
  )
  (module 10-My-Footprints:LED_0603_1608Metric_SnapModel (layer F.Cu) (tedit 5FFD7569)
    (at 71.876001 53.126001)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer F.Fab) hide)
    (fp_text value PWR (at 0 -1.425 180) (layer F.SilkS))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Board_1-Board_1-Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/LTST-C193TBKT-5A.step
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "10-My-Footprints:ESP32-S2-WROVER_and_WROOM(PCB,-I(IPEX))-Universal" (layer F.Cu) (tedit 6034B573)
    (at 100.001001 67.241001 270)
    (fp_text reference U1 (at -8.5 17 270) (layer F.SilkS))
    (fp_text value ESP32-S2-WROVER (at 0 11.25 90) (layer F.Fab))
    (fp_text user "!!! Keepout Area !!!" (at 0.01 -10.5 90) (layer Dwgs.User))
    (fp_text user 17 (at -6.49 13 315 unlocked) (layer F.SilkS))
    (fp_text user o (at -9.779 -8.8646 270) (layer F.SilkS))
    (fp_text user 26 (at 6.51 13 225 unlocked) (layer F.SilkS))
    (fp_text user "!!! Keepout Area !!!" (at 0.01 -14.5 90) (layer Dwgs.User))
    (fp_text user 42 (at 6.75 -8 315 unlocked) (layer F.SilkS))
    (fp_text user ANTENNA (at 0.01 -12.5 90) (layer F.SilkS))
    (fp_text user 1 (at -6.75 -8.001 225 unlocked) (layer F.SilkS))
    (pad 1 smd rect (at -8.75 -8 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 3 smd rect (at -8.75 -5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 Board_1-Board_1-/~BOOT))
    (pad 43 thru_hole rect (at -1.19 0.05 270) (size 1.4 1.4) (drill 1.2) (layers *.Cu *.Mask F.Paste)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 2 smd rect (at -8.75 -6.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-Board_1-+3V3))
    (pad 43 smd rect (at -1.19 0.05 270) (size 4.1 4.1) (layers F.Cu F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 34 smd rect (at 8.75 4 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 Board_1-Board_1-/MTDO))
    (pad 25 smd rect (at 5.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 25 Board_1-Board_1-/xPSRAM_CS))
    (pad 42 smd rect (at 8.75 -8 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 39 smd rect (at 8.75 -3.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 Board_1-Board_1-/VDD_SPI))
    (pad 14 smd rect (at -8.75 11.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Board_1-Board_1-Net-(U1-Pad14)"))
    (pad 35 smd rect (at 8.75 2.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 Board_1-Board_1-/MTDI))
    (pad 40 smd rect (at 8.75 -5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 Board_1-Board_1-/~DFU))
    (pad 11 smd rect (at -8.75 7 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Board_1-Board_1-Net-(U1-Pad11)"))
    (pad 20 smd rect (at -2.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 Board_1-Board_1-/~CAN_EN))
    (pad 24 smd rect (at 3.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Board_1-Board_1-Net-(U1-Pad24)"))
    (pad 26 smd rect (at 6.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND))
    (pad 43 smd rect (at -2.69 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 smd rect (at -2.69 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 19 smd rect (at -3.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 Board_1-Board_1-/CAN_RX))
    (pad 43 thru_hole circle (at -1.94 -1.45 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 23 smd rect (at 2.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 Board_1-Board_1-/USB_D+))
    (pad 43 thru_hole circle (at -0.44 -1.45 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 43 thru_hole circle (at -2.69 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 9 smd rect (at -8.75 4 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Board_1-Board_1-Net-(U1-Pad9)"))
    (pad 43 thru_hole circle (at 0.31 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 41 smd rect (at 8.75 -6.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 Board_1-Board_1-/~RST))
    (pad 16 smd rect (at -8.75 14.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Board_1-Board_1-Net-(U1-Pad16)"))
    (pad 43 thru_hole circle (at 0.31 0.8 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 30 smd rect (at 8.75 10 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_1-Board_1-/~SW_S))
    (pad 12 smd rect (at -8.75 8.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Board_1-Board_1-Net-(U1-Pad12)"))
    (pad 36 smd rect (at 8.75 1 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 Board_1-Board_1-/MTMS))
    (pad 10 smd rect (at -8.75 5.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Board_1-Board_1-Net-(U1-Pad10)"))
    (pad 15 smd rect (at -8.75 13 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Board_1-Board_1-Net-(U1-Pad15)"))
    (pad 21 smd rect (at -0.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-Board_1-/U1RX0))
    (pad 43 smd rect (at -2.69 0.05 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 smd rect (at 0.31 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 38 smd rect (at 8.75 -2 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 Board_1-Board_1-/U0RXD))
    (pad 4 smd rect (at -8.75 -3.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-Board_1-/QW_SCL))
    (pad 43 smd rect (at 0.31 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 thru_hole circle (at -2.69 0.8 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 22 smd rect (at 0.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 Board_1-Board_1-/USB_D-))
    (pad 6 smd rect (at -8.75 -0.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Board_1-Board_1-Net-(U1-Pad6)"))
    (pad 31 smd rect (at 8.75 8.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 Board_1-Board_1-/~SW_R))
    (pad 43 smd rect (at -1.19 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 27 smd rect (at 8.75 14.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Board_1-Board_1-Net-(U1-Pad27)"))
    (pad 18 smd rect (at -5.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 Board_1-Board_1-/CAN_TX))
    (pad 13 smd rect (at -8.75 10 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Board_1-Board_1-Net-(U1-Pad13)"))
    (pad 43 smd rect (at -1.19 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 37 smd rect (at 8.75 -0.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-Board_1-/U0TXD))
    (pad 8 smd rect (at -8.75 2.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 Board_1-Board_1-/OLED_SCL))
    (pad 43 thru_hole circle (at -0.44 1.55 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 5 smd rect (at -8.75 -2 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 Board_1-Board_1-/QW_SDA))
    (pad 28 smd rect (at 8.75 13 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Board_1-Board_1-Net-(U1-Pad28)"))
    (pad 43 smd rect (at 0.31 0.05 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-Board_1-GND) (solder_paste_margin -0.001))
    (pad 17 smd rect (at -6.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Board_1-Board_1-Net-(U1-Pad17)"))
    (pad 7 smd rect (at -8.75 1 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 Board_1-Board_1-/OLED_SDA))
    (pad 29 smd rect (at 8.75 11.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 Board_1-Board_1-/~SW_L))
    (pad 33 smd rect (at 8.75 5.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 Board_1-Board_1-/MTCK))
    (pad 43 thru_hole circle (at -1.94 1.55 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-Board_1-GND))
    (pad 32 smd rect (at 8.75 7 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-Board_1-/LED_D))
    (model ${KIPRJMOD}/shapes3D/ESP32-S2-WROVER-I.STEP
      (offset (xyz -9 -15.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:neggle-logo-0.12 (layer B.Cu) (tedit 602F09FF)
    (at 65.926001 77.501001 180)
    (fp_text reference LOGO1 (at 0 -0.5 180) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0 0.5 180) (layer B.Fab) hide)
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 73.751001 59.501001 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0 3.3) (layer F.SilkS))
    (fp_text value MAX3051ESA (at 0 -1.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (pad 7 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Board_1-Board_1-/CAN+))
    (pad 6 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Board_1-Board_1-/CAN-))
    (pad 5 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 Board_1-Board_1-/~CAN_EN))
    (pad 4 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Board_1-Board_1-/CAN_RX))
    (pad 3 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (pad 2 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (pad 1 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-Board_1-/CAN_TX))
    (model ${KIPRJMOD}/shapes3D/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 71.601001 54.576001 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1.55 0) (layer F.SilkS))
    (fp_text value 1K (at 0 -0.875) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Board_1-Board_1-Net-(D2-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 107.251001 78.626001)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.375) (layer F.SilkS))
    (fp_text value 10uF (at 0 -1.125) (layer F.Fab))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 Board_1-Board_1-/~RST))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 57.876001 85.621001 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at -0.005 -0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 Board_1-Board_1-/~BOOT))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 66.876001 85.621001 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.945 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0.875 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 Board_1-Board_1-/~RST))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 69.1616 128.898) (end 69.1664 129.0148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1473 128.8019) (end 69.1616 128.898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1237 128.7076) (end 69.1473 128.8019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.091 128.6161) (end 69.1237 128.7076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0495 128.5283) (end 69.091 128.6161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9995 128.445) (end 69.0495 128.5283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9416 128.367) (end 68.9995 128.445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8764 128.295) (end 68.9416 128.367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8044 128.2297) (end 68.8764 128.295) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7264 128.1719) (end 68.8044 128.2297) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6431 128.1219) (end 68.7264 128.1719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5552 128.0804) (end 68.6431 128.1219) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4638 128.0476) (end 68.5552 128.0804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3695 128.024) (end 68.4638 128.0476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2734 128.0098) (end 68.3695 128.024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1761 128.005) (end 68.2734 128.0098) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.5008 128.0049) (end 68.1761 128.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.2397 127.991) (end 52.5008 128.0049) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9938 127.9523) (end 52.2397 127.991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9681 127.9469) (end 51.9938 127.9523) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.7277 127.8821) (end 51.9681 127.9469) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4837 127.7885) (end 51.7277 127.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2618 127.6759) (end 51.4837 127.7885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2389 127.6627) (end 51.2618 127.6759) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0413 127.5343) (end 51.2389 127.6627) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0201 127.5189) (end 51.0413 127.5343) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8268 127.3619) (end 51.0201 127.5189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.6417 127.1767) (end 50.8268 127.3619) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.477 126.9733) (end 50.6417 127.1767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3344 126.7536) (end 50.477 126.9733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2155 126.5202) (end 50.3344 126.7536) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1217 126.2757) (end 50.2155 126.5202) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.054 126.0229) (end 50.1217 126.2757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0148 125.7776) (end 50.054 126.0229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.012 125.7517) (end 50.0148 125.7776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 125.4965) (end 50.012 125.7517) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 112.7443) (end 49.999 125.4965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9942 112.647) (end 49.999 112.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.98 112.5509) (end 49.9942 112.647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9564 112.4566) (end 49.98 112.5509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9236 112.3652) (end 49.9564 112.4566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8821 112.2774) (end 49.9236 112.3652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8321 112.194) (end 49.8821 112.2774) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7743 112.116) (end 49.8321 112.194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.709 112.044) (end 49.7743 112.116) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.637 111.9788) (end 49.709 112.044) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.559 111.9209) (end 49.637 111.9788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4757 111.8709) (end 49.559 111.9209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.3879 111.8294) (end 49.4757 111.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2964 111.7967) (end 49.3879 111.8294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2021 111.7731) (end 49.2964 111.7967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.106 111.7588) (end 49.2021 111.7731) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9892 111.754) (end 49.106 111.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.892 111.7588) (end 48.9892 111.754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7959 111.7731) (end 48.892 111.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7016 111.7967) (end 48.7959 111.7731) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6101 111.8294) (end 48.7016 111.7967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5223 111.8709) (end 48.6101 111.8294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.439 111.9209) (end 48.5223 111.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.361 111.9788) (end 48.439 111.9209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.289 112.044) (end 48.361 111.9788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2237 112.116) (end 48.289 112.044) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1659 112.194) (end 48.2237 112.116) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1159 112.2774) (end 48.1659 112.194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0744 112.3652) (end 48.1159 112.2774) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0416 112.4566) (end 48.0744 112.3652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.018 112.5509) (end 48.0416 112.4566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0038 112.647) (end 48.018 112.5509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 112.7443) (end 48.0038 112.647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 125.4965) (end 47.999 112.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0021 125.6142) (end 47.999 125.4965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0148 125.8562) (end 48.0021 125.6142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0216 125.9478) (end 48.0148 125.8562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0395 126.0909) (end 48.0216 125.9478) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0764 126.3236) (end 48.0395 126.0909) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0927 126.4135) (end 48.0764 126.3236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1252 126.5532) (end 48.0927 126.4135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1861 126.7808) (end 48.1252 126.5532) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2119 126.8689) (end 48.1861 126.7808) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2589 127.005) (end 48.2119 126.8689) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3434 127.225) (end 48.2589 127.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3782 127.31) (end 48.3434 127.225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.4393 127.4404) (end 48.3782 127.31) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5464 127.6505) (end 48.4393 127.4404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5898 127.7312) (end 48.5464 127.6505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.664 127.8542) (end 48.5898 127.7312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7924 128.0519) (end 48.664 127.8542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.844 128.1277) (end 48.7924 128.0519) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9308 128.2425) (end 48.844 128.1277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.0791 128.4256) (end 48.9308 128.2425) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.1384 128.4956) (end 49.0791 128.4256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2367 128.6006) (end 49.1384 128.4956) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4034 128.7673) (end 49.2367 128.6006) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4697 128.8307) (end 49.4034 128.7673) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5784 128.9249) (end 49.4697 128.8307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7616 129.0732) (end 49.5784 128.9249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8759 129.1597) (end 49.7616 129.0732) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9515 129.2112) (end 49.8759 129.1597) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1714 129.3537) (end 49.9515 129.2112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2729 129.4144) (end 50.1714 129.3537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.331 129.4459) (end 50.2729 129.4144) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.5642 129.565) (end 50.331 129.4459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.6942 129.6259) (end 50.5642 129.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.779 129.6606) (end 50.6942 129.6259) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.999 129.7451) (end 50.779 129.6606) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0854 129.776) (end 50.999 129.7451) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2232 129.8179) (end 51.0854 129.776) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4508 129.8788) (end 51.2232 129.8179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.5396 129.9005) (end 51.4508 129.8788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.6548 129.9232) (end 51.5396 129.9005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9132 129.9646) (end 51.6548 129.9232) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.0042 129.9769) (end 51.9132 129.9646) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.1479 129.9892) (end 52.0042 129.9769) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.3898 130.0019) (end 52.1479 129.9892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.5075 130.005) (end 52.3898 130.0019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1761 130.005) (end 52.5075 130.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2734 130.0002) (end 68.1761 130.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3695 129.986) (end 68.2734 130.0002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4638 129.9624) (end 68.3695 129.986) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5552 129.9296) (end 68.4638 129.9624) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6431 129.8881) (end 68.5552 129.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7264 129.8381) (end 68.6431 129.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8044 129.7803) (end 68.7264 129.8381) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8764 129.715) (end 68.8044 129.7803) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9416 129.643) (end 68.8764 129.715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9995 129.565) (end 68.9416 129.643) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0495 129.4817) (end 68.9995 129.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.091 129.3939) (end 69.0495 129.4817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1237 129.3024) (end 69.091 129.3939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1473 129.2081) (end 69.1237 129.3024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1616 129.112) (end 69.1473 129.2081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1664 129.0148) (end 69.1616 129.112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.5075 47.999) (end 68.1761 47.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.4028 48.0015) (end 52.5075 47.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.1478 48.0148) (end 52.4028 48.0015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.0043 48.0271) (end 52.1478 48.0148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9131 48.0395) (end 52.0043 48.0271) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.6548 48.0808) (end 51.9131 48.0395) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.5397 48.1035) (end 51.6548 48.0808) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.476 48.1188) (end 51.5397 48.1035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2232 48.1861) (end 51.476 48.1188) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0855 48.228) (end 51.2232 48.1861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.999 48.2589) (end 51.0855 48.228) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.779 48.3434) (end 50.999 48.2589) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.694 48.3782) (end 50.779 48.3434) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.5636 48.4393) (end 50.694 48.3782) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3535 48.5464) (end 50.5636 48.4393) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2278 48.6158) (end 50.3535 48.5464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1498 48.664) (end 50.2278 48.6158) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9521 48.7924) (end 50.1498 48.664) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8342 48.8746) (end 49.9521 48.7924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7615 48.9308) (end 49.8342 48.8746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5784 49.0791) (end 49.7615 48.9308) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5084 49.1384) (end 49.5784 49.0791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4034 49.2367) (end 49.5084 49.1384) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2367 49.4034) (end 49.4034 49.2367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.1733 49.4697) (end 49.2367 49.4034) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.0791 49.5784) (end 49.1733 49.4697) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9308 49.7616) (end 49.0791 49.5784) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.8748 49.8339) (end 48.9308 49.7616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7928 49.9515) (end 48.8748 49.8339) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6643 50.1492) (end 48.7928 49.9515) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6158 50.2276) (end 48.6643 50.1492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5896 50.2729) (end 48.6158 50.2276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5459 50.3542) (end 48.5896 50.2729) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.439 50.5642) (end 48.5459 50.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3993 50.6467) (end 48.439 50.5642) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.353 50.7548) (end 48.3993 50.6467) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2589 50.999) (end 48.353 50.7548) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2119 51.135) (end 48.2589 50.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1861 51.2232) (end 48.2119 51.135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1252 51.4508) (end 48.1861 51.2232) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0927 51.5904) (end 48.1252 51.4508) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0764 51.6804) (end 48.0927 51.5904) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0357 51.939) (end 48.0764 51.6804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0216 52.0561) (end 48.0357 51.939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0165 52.1218) (end 48.0216 52.0561) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0015 52.4028) (end 48.0165 52.1218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 52.5075) (end 48.0015 52.4028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 65.2598) (end 47.999 52.5075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0038 65.357) (end 47.999 65.2598) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.018 65.4531) (end 48.0038 65.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0416 65.5474) (end 48.018 65.4531) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0744 65.6389) (end 48.0416 65.5474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1159 65.7267) (end 48.0744 65.6389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1659 65.81) (end 48.1159 65.7267) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2237 65.8881) (end 48.1659 65.81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.289 65.96) (end 48.2237 65.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.361 66.0253) (end 48.289 65.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.439 66.0832) (end 48.361 66.0253) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5223 66.1331) (end 48.439 66.0832) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6101 66.1746) (end 48.5223 66.1331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7016 66.2074) (end 48.6101 66.1746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7959 66.231) (end 48.7016 66.2074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.892 66.2452) (end 48.7959 66.231) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9892 66.25) (end 48.892 66.2452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.106 66.2452) (end 48.9892 66.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2021 66.231) (end 49.106 66.2452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2964 66.2074) (end 49.2021 66.231) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.3879 66.1746) (end 49.2964 66.2074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4757 66.1331) (end 49.3879 66.1746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.559 66.0832) (end 49.4757 66.1331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.637 66.0253) (end 49.559 66.0832) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.709 65.96) (end 49.637 66.0253) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7743 65.8881) (end 49.709 65.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8321 65.81) (end 49.7743 65.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8821 65.7267) (end 49.8321 65.81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9236 65.6389) (end 49.8821 65.7267) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9564 65.5474) (end 49.9236 65.6389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.98 65.4531) (end 49.9564 65.5474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9942 65.357) (end 49.98 65.4531) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 65.2598) (end 49.9942 65.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 52.5076) (end 49.999 65.2598) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.012 52.2526) (end 49.999 52.5076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0148 52.2264) (end 50.012 52.2526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.054 51.9811) (end 50.0148 52.2264) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.118 51.7406) (end 50.054 51.9811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1262 51.7156) (end 50.118 51.7406) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2106 51.4957) (end 50.1262 51.7156) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2212 51.4717) (end 50.2106 51.4957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3346 51.2499) (end 50.2212 51.4717) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4773 51.0303) (end 50.3346 51.2499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.6421 50.8268) (end 50.4773 51.0303) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8273 50.6417) (end 50.6421 50.8268) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0303 50.4773) (end 50.8273 50.6417) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.239 50.3414) (end 51.0303 50.4773) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2617 50.3283) (end 51.239 50.3414) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4716 50.2213) (end 51.2617 50.3283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4957 50.2106) (end 51.4716 50.2213) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.7283 50.1217) (end 51.4957 50.2106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9811 50.054) (end 51.7283 50.1217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.2392 50.0131) (end 51.9811 50.054) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.5009 49.9991) (end 52.2392 50.0131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1761 49.999) (end 52.5009 49.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2734 49.9942) (end 68.1761 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3695 49.98) (end 68.2734 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4638 49.9564) (end 68.3695 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5552 49.9236) (end 68.4638 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6431 49.8821) (end 68.5552 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7264 49.8321) (end 68.6431 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8044 49.7743) (end 68.7264 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8764 49.709) (end 68.8044 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9416 49.637) (end 68.8764 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9995 49.559) (end 68.9416 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0495 49.4757) (end 68.9995 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.091 49.3879) (end 69.0495 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1237 49.2964) (end 69.091 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1473 49.2021) (end 69.1237 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1616 49.106) (end 69.1473 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1664 49.0088) (end 69.1616 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1616 48.892) (end 69.1664 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1473 48.7959) (end 69.1616 48.892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1237 48.7016) (end 69.1473 48.7959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.091 48.6101) (end 69.1237 48.7016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0495 48.5223) (end 69.091 48.6101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9995 48.439) (end 69.0495 48.5223) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9416 48.361) (end 68.9995 48.439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8764 48.289) (end 68.9416 48.361) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8044 48.2237) (end 68.8764 48.289) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7264 48.1659) (end 68.8044 48.2237) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6431 48.1159) (end 68.7264 48.1659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5552 48.0744) (end 68.6431 48.1159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4638 48.0416) (end 68.5552 48.0744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3695 48.018) (end 68.4638 48.0416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2734 48.0038) (end 68.3695 48.018) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1761 47.999) (end 68.2734 48.0038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 84.9945) (end 47.999 72.2423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0015 85.0992) (end 47.999 84.9945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0148 85.3542) (end 48.0015 85.0992) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0216 85.4458) (end 48.0148 85.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0357 85.563) (end 48.0216 85.4458) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0808 85.8472) (end 48.0357 85.563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1035 85.9623) (end 48.0808 85.8472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1252 86.0512) (end 48.1035 85.9623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1861 86.2788) (end 48.1252 86.0512) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.228 86.4165) (end 48.1861 86.2788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2589 86.503) (end 48.228 86.4165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3434 86.723) (end 48.2589 86.503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3782 86.808) (end 48.3434 86.723) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.4278 86.915) (end 48.3782 86.808) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5464 87.1485) (end 48.4278 86.915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5898 87.2292) (end 48.5464 87.1485) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.664 87.3522) (end 48.5898 87.2292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7924 87.5499) (end 48.664 87.3522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.844 87.6257) (end 48.7924 87.5499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9308 87.7405) (end 48.844 87.6257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.0791 87.9236) (end 48.9308 87.7405) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.1732 88.0323) (end 49.0791 87.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2367 88.0986) (end 49.1732 88.0323) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4034 88.2653) (end 49.2367 88.0986) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5084 88.3635) (end 49.4034 88.2653) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5784 88.4229) (end 49.5084 88.3635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7616 88.5712) (end 49.5784 88.4229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8759 88.6577) (end 49.7616 88.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9515 88.7092) (end 49.8759 88.6577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1714 88.8517) (end 49.9515 88.7092) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2729 88.9124) (end 50.1714 88.8517) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4268 88.9934) (end 50.2729 88.9124) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4304 88.9968) (end 50.4268 88.9934) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4318 89.0015) (end 50.4304 88.9968) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4309 89.0064) (end 50.4318 89.0015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4268 89.0107) (end 50.4309 89.0064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2728 89.0918) (end 50.4268 89.0107) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1718 89.1521) (end 50.2728 89.0918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9521 89.2944) (end 50.1718 89.1521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8763 89.346) (end 49.9521 89.2944) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7615 89.4328) (end 49.8763 89.346) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5784 89.5811) (end 49.7615 89.4328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.5084 89.6404) (end 49.5784 89.5811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4034 89.7387) (end 49.5084 89.6404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2367 89.9054) (end 49.4034 89.7387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.1385 90.0104) (end 49.2367 89.9054) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.0791 90.0804) (end 49.1385 90.0104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.9147 90.284) (end 49.0791 90.0804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.8443 90.3779) (end 48.9147 90.284) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.8072 90.4319) (end 48.8443 90.3779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6503 90.6734) (end 48.8072 90.4319) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5896 90.7749) (end 48.6503 90.6734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5459 90.8562) (end 48.5896 90.7749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.439 91.0662) (end 48.5459 90.8562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3781 91.1962) (end 48.439 91.0662) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.3434 91.281) (end 48.3781 91.1962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2589 91.501) (end 48.3434 91.281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.228 91.5874) (end 48.2589 91.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1932 91.7001) (end 48.228 91.5874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1252 91.9528) (end 48.1932 91.7001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1035 92.0416) (end 48.1252 91.9528) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0764 92.1824) (end 48.1035 92.0416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0394 92.4152) (end 48.0764 92.1824) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0216 92.5581) (end 48.0394 92.4152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0148 92.6499) (end 48.0216 92.5581) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0021 92.8918) (end 48.0148 92.6499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 93.0095) (end 48.0021 92.8918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 105.7618) (end 47.999 93.0095) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0038 105.8591) (end 47.999 105.7618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.018 105.9552) (end 48.0038 105.8591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0416 106.0494) (end 48.018 105.9552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0744 106.1409) (end 48.0416 106.0494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1159 106.2287) (end 48.0744 106.1409) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1659 106.312) (end 48.1159 106.2287) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2237 106.3901) (end 48.1659 106.312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.289 106.4621) (end 48.2237 106.3901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.361 106.5273) (end 48.289 106.4621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.439 106.5852) (end 48.361 106.5273) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5223 106.6351) (end 48.439 106.5852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6101 106.6767) (end 48.5223 106.6351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7016 106.7094) (end 48.6101 106.6767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7959 106.733) (end 48.7016 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.892 106.7472) (end 48.7959 106.733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.0088 106.752) (end 48.892 106.7472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.106 106.7472) (end 49.0088 106.752) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2021 106.733) (end 49.106 106.7472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2964 106.7094) (end 49.2021 106.733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.3879 106.6767) (end 49.2964 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4757 106.6351) (end 49.3879 106.6767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.559 106.5852) (end 49.4757 106.6351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.637 106.5273) (end 49.559 106.5852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.709 106.4621) (end 49.637 106.5273) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7743 106.3901) (end 49.709 106.4621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8321 106.312) (end 49.7743 106.3901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8821 106.2287) (end 49.8321 106.312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9236 106.1409) (end 49.8821 106.2287) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9564 106.0494) (end 49.9236 106.1409) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.98 105.9552) (end 49.9564 106.0494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9942 105.8591) (end 49.98 105.9552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 105.7618) (end 49.9942 105.8591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 93.0096) (end 49.999 105.7618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.012 92.7546) (end 49.999 93.0096) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0148 92.7284) (end 50.012 92.7546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.054 92.4831) (end 50.0148 92.7284) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.118 92.2426) (end 50.054 92.4831) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1262 92.2176) (end 50.118 92.2426) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2106 91.9977) (end 50.1262 92.2176) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2212 91.9737) (end 50.2106 91.9977) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3346 91.7519) (end 50.2212 91.9737) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4773 91.5323) (end 50.3346 91.7519) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.6418 91.3292) (end 50.4773 91.5323) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8269 91.1441) (end 50.6418 91.3292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0303 90.9793) (end 50.8269 91.1441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.239 90.8434) (end 51.0303 90.9793) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2617 90.8303) (end 51.239 90.8434) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4716 90.7233) (end 51.2617 90.8303) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4957 90.7126) (end 51.4716 90.7233) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.7283 90.6237) (end 51.4957 90.7126) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9811 90.556) (end 51.7283 90.6237) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.2392 90.5151) (end 51.9811 90.556) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.5009 90.5011) (end 52.2392 90.5151) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1761 90.501) (end 52.5009 90.5011) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2734 90.4962) (end 68.1761 90.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3695 90.482) (end 68.2734 90.4962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4638 90.4584) (end 68.3695 90.482) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5552 90.4256) (end 68.4638 90.4584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6431 90.3841) (end 68.5552 90.4256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7264 90.3341) (end 68.6431 90.3841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8044 90.2763) (end 68.7264 90.3341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8764 90.211) (end 68.8044 90.2763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9416 90.139) (end 68.8764 90.211) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9995 90.061) (end 68.9416 90.139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0495 89.9777) (end 68.9995 90.061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.091 89.8899) (end 69.0495 89.9777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1237 89.7984) (end 69.091 89.8899) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1473 89.7041) (end 69.1237 89.7984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1616 89.608) (end 69.1473 89.7041) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1664 89.5108) (end 69.1616 89.608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1664 88.4932) (end 69.1664 89.5108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1616 88.396) (end 69.1664 88.4932) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1473 88.2999) (end 69.1616 88.396) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1237 88.2056) (end 69.1473 88.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.091 88.1141) (end 69.1237 88.2056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0495 88.0263) (end 69.091 88.1141) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9995 87.943) (end 69.0495 88.0263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.9416 87.865) (end 68.9995 87.943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8764 87.793) (end 68.9416 87.865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8044 87.7277) (end 68.8764 87.793) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7264 87.6699) (end 68.8044 87.7277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6431 87.6199) (end 68.7264 87.6699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5552 87.5784) (end 68.6431 87.6199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4638 87.5456) (end 68.5552 87.5784) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3695 87.522) (end 68.4638 87.5456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2734 87.5078) (end 68.3695 87.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1761 87.503) (end 68.2734 87.5078) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.5008 87.5029) (end 68.1761 87.503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.2397 87.489) (end 52.5008 87.5029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9938 87.4503) (end 52.2397 87.489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.9681 87.4449) (end 51.9938 87.4503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.7277 87.3801) (end 51.9681 87.4449) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.4837 87.2865) (end 51.7277 87.3801) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2618 87.1739) (end 51.4837 87.2865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.2389 87.1607) (end 51.2618 87.1739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0413 87.0323) (end 51.2389 87.1607) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 51.0203 87.017) (end 51.0413 87.0323) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.8268 86.8599) (end 51.0203 87.017) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.6417 86.6747) (end 50.8268 86.8599) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.477 86.4713) (end 50.6417 86.6747) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3344 86.2516) (end 50.477 86.4713) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2155 86.0182) (end 50.3344 86.2516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1217 85.7737) (end 50.2155 86.0182) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.054 85.5209) (end 50.1217 85.7737) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0148 85.2756) (end 50.054 85.5209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.012 85.2497) (end 50.0148 85.2756) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 84.9945) (end 50.012 85.2497) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 72.2423) (end 49.999 84.9945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9942 72.145) (end 49.999 72.2423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.98 72.0489) (end 49.9942 72.145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9564 71.9546) (end 49.98 72.0489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9236 71.8632) (end 49.9564 71.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8821 71.7753) (end 49.9236 71.8632) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.8321 71.692) (end 49.8821 71.7753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.7743 71.614) (end 49.8321 71.692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.709 71.542) (end 49.7743 71.614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.637 71.4767) (end 49.709 71.542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.559 71.4189) (end 49.637 71.4767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.4757 71.3689) (end 49.559 71.4189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.3879 71.3274) (end 49.4757 71.3689) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2964 71.2946) (end 49.3879 71.3274) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.2021 71.271) (end 49.2964 71.2946) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.106 71.2568) (end 49.2021 71.271) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.0088 71.252) (end 49.106 71.2568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.892 71.2568) (end 49.0088 71.252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7959 71.271) (end 48.892 71.2568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.7016 71.2946) (end 48.7959 71.271) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.6101 71.3274) (end 48.7016 71.2946) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.5223 71.3689) (end 48.6101 71.3274) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.439 71.4189) (end 48.5223 71.3689) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.361 71.4767) (end 48.439 71.4189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.289 71.542) (end 48.361 71.4767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.2237 71.614) (end 48.289 71.542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1659 71.692) (end 48.2237 71.614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.1159 71.7753) (end 48.1659 71.692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0744 71.8632) (end 48.1159 71.7753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0416 71.9546) (end 48.0744 71.8632) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.018 72.0489) (end 48.0416 71.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 48.0038 72.145) (end 48.018 72.0489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 47.999 72.2423) (end 48.0038 72.145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.829 128.898) (end 90.8338 129.0148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8147 128.8019) (end 90.829 128.898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7911 128.7076) (end 90.8147 128.8019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7584 128.6161) (end 90.7911 128.7076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7168 128.5283) (end 90.7584 128.6161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.6669 128.445) (end 90.7168 128.5283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.609 128.367) (end 90.6669 128.445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5438 128.295) (end 90.609 128.367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.4718 128.2297) (end 90.5438 128.295) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3938 128.1719) (end 90.4718 128.2297) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3104 128.1219) (end 90.3938 128.1719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.2226 128.0804) (end 90.3104 128.1219) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.1311 128.0476) (end 90.2226 128.0804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.0369 128.024) (end 90.1311 128.0476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9408 128.0098) (end 90.0369 128.024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.8435 128.005) (end 89.9408 128.0098) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1586 128.005) (end 89.8435 128.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.0613 128.0098) (end 75.1586 128.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.9652 128.024) (end 75.0613 128.0098) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.871 128.0476) (end 74.9652 128.024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.7795 128.0804) (end 74.871 128.0476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6917 128.1219) (end 74.7795 128.0804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6084 128.1719) (end 74.6917 128.1219) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.5303 128.2297) (end 74.6084 128.1719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.4583 128.295) (end 74.5303 128.2297) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3931 128.367) (end 74.4583 128.295) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3352 128.445) (end 74.3931 128.367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2853 128.5283) (end 74.3352 128.445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2437 128.6161) (end 74.2853 128.5283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.211 128.7076) (end 74.2437 128.6161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1874 128.8019) (end 74.211 128.7076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1732 128.898) (end 74.1874 128.8019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1684 128.9952) (end 74.1732 128.898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1732 129.112) (end 74.1684 128.9952) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1874 129.2081) (end 74.1732 129.112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.211 129.3024) (end 74.1874 129.2081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2437 129.3939) (end 74.211 129.3024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2853 129.4817) (end 74.2437 129.3939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3352 129.565) (end 74.2853 129.4817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3931 129.643) (end 74.3352 129.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.4583 129.715) (end 74.3931 129.643) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.5303 129.7803) (end 74.4583 129.715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6084 129.8381) (end 74.5303 129.7803) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6917 129.8881) (end 74.6084 129.8381) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.7795 129.9296) (end 74.6917 129.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.871 129.9624) (end 74.7795 129.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.9652 129.986) (end 74.871 129.9624) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.0613 130.0002) (end 74.9652 129.986) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1586 130.005) (end 75.0613 130.0002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.8435 130.005) (end 75.1586 130.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9408 130.0002) (end 89.8435 130.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.0369 129.986) (end 89.9408 130.0002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.1311 129.9624) (end 90.0369 129.986) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.2226 129.9296) (end 90.1311 129.9624) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3104 129.8881) (end 90.2226 129.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3938 129.8381) (end 90.3104 129.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.4718 129.7803) (end 90.3938 129.8381) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5438 129.715) (end 90.4718 129.7803) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.609 129.643) (end 90.5438 129.715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.6669 129.565) (end 90.609 129.643) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7168 129.4817) (end 90.6669 129.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7584 129.3939) (end 90.7168 129.4817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7911 129.3024) (end 90.7584 129.3939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8147 129.2081) (end 90.7911 129.3024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.829 129.112) (end 90.8147 129.2081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8338 129.0148) (end 90.829 129.112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.8435 90.501) (end 75.1586 90.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9408 90.4962) (end 89.8435 90.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.0369 90.482) (end 89.9408 90.4962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.1311 90.4584) (end 90.0369 90.482) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.2226 90.4256) (end 90.1311 90.4584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3104 90.3841) (end 90.2226 90.4256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3938 90.3341) (end 90.3104 90.3841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.4718 90.2763) (end 90.3938 90.3341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5438 90.211) (end 90.4718 90.2763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.609 90.139) (end 90.5438 90.211) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.6669 90.061) (end 90.609 90.139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7168 89.9777) (end 90.6669 90.061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7584 89.8899) (end 90.7168 89.9777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7911 89.7984) (end 90.7584 89.8899) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8147 89.7041) (end 90.7911 89.7984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.829 89.608) (end 90.8147 89.7041) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8338 89.5108) (end 90.829 89.608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8338 88.4932) (end 90.8338 89.5108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.829 88.396) (end 90.8338 88.4932) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8147 88.2999) (end 90.829 88.396) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7911 88.2056) (end 90.8147 88.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7584 88.1141) (end 90.7911 88.2056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7168 88.0263) (end 90.7584 88.1141) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.6669 87.943) (end 90.7168 88.0263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.609 87.865) (end 90.6669 87.943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5438 87.793) (end 90.609 87.865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.4718 87.7277) (end 90.5438 87.793) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3938 87.6699) (end 90.4718 87.7277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3104 87.6199) (end 90.3938 87.6699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.2226 87.5784) (end 90.3104 87.6199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.1311 87.5456) (end 90.2226 87.5784) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.0369 87.522) (end 90.1311 87.5456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9408 87.5078) (end 90.0369 87.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.8435 87.503) (end 89.9408 87.5078) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1586 87.503) (end 89.8435 87.503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.0613 87.5078) (end 75.1586 87.503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.9652 87.522) (end 75.0613 87.5078) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.871 87.5456) (end 74.9652 87.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.7795 87.5784) (end 74.871 87.5456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6917 87.6199) (end 74.7795 87.5784) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6084 87.6699) (end 74.6917 87.6199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.5303 87.7277) (end 74.6084 87.6699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.4583 87.793) (end 74.5303 87.7277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3931 87.865) (end 74.4583 87.793) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3352 87.943) (end 74.3931 87.865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2853 88.0263) (end 74.3352 87.943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2437 88.1141) (end 74.2853 88.0263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.211 88.2056) (end 74.2437 88.1141) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1874 88.2999) (end 74.211 88.2056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1732 88.396) (end 74.1874 88.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1684 88.4932) (end 74.1732 88.396) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1684 89.5108) (end 74.1684 88.4932) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1732 89.608) (end 74.1684 89.5108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1874 89.7041) (end 74.1732 89.608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.211 89.7984) (end 74.1874 89.7041) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2437 89.8899) (end 74.211 89.7984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2853 89.9777) (end 74.2437 89.8899) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3352 90.061) (end 74.2853 89.9777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3931 90.139) (end 74.3352 90.061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.4583 90.211) (end 74.3931 90.139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.5303 90.2763) (end 74.4583 90.211) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6084 90.3341) (end 74.5303 90.2763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6917 90.3841) (end 74.6084 90.3341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.7795 90.4256) (end 74.6917 90.3841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.871 90.4584) (end 74.7795 90.4256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.9652 90.482) (end 74.871 90.4584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.0613 90.4962) (end 74.9652 90.482) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1586 90.501) (end 75.0613 90.4962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.8435 49.999) (end 75.1586 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9408 49.9942) (end 89.8435 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.0369 49.98) (end 89.9408 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.1311 49.9564) (end 90.0369 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.2226 49.9236) (end 90.1311 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3104 49.8821) (end 90.2226 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3938 49.8321) (end 90.3104 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.4718 49.7743) (end 90.3938 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5438 49.709) (end 90.4718 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.609 49.637) (end 90.5438 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.6669 49.559) (end 90.609 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7168 49.4757) (end 90.6669 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7584 49.3879) (end 90.7168 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7911 49.2964) (end 90.7584 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8147 49.2021) (end 90.7911 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.829 49.106) (end 90.8147 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8338 48.9892) (end 90.829 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.829 48.892) (end 90.8338 48.9892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.8147 48.7959) (end 90.829 48.892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7911 48.7016) (end 90.8147 48.7959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7584 48.6101) (end 90.7911 48.7016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.7168 48.5223) (end 90.7584 48.6101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.6669 48.439) (end 90.7168 48.5223) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.609 48.361) (end 90.6669 48.439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.5438 48.289) (end 90.609 48.361) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.4718 48.2237) (end 90.5438 48.289) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3938 48.1659) (end 90.4718 48.2237) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.3104 48.1159) (end 90.3938 48.1659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.2226 48.0744) (end 90.3104 48.1159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.1311 48.0416) (end 90.2226 48.0744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 90.0369 48.018) (end 90.1311 48.0416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.9408 48.0038) (end 90.0369 48.018) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.8435 47.999) (end 89.9408 48.0038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1586 47.999) (end 89.8435 47.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.0613 48.0038) (end 75.1586 47.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.9652 48.018) (end 75.0613 48.0038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.871 48.0416) (end 74.9652 48.018) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.7795 48.0744) (end 74.871 48.0416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6917 48.1159) (end 74.7795 48.0744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6084 48.1659) (end 74.6917 48.1159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.5303 48.2237) (end 74.6084 48.1659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.4583 48.289) (end 74.5303 48.2237) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3931 48.361) (end 74.4583 48.289) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3352 48.439) (end 74.3931 48.361) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2853 48.5223) (end 74.3352 48.439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2437 48.6101) (end 74.2853 48.5223) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.211 48.7016) (end 74.2437 48.6101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1874 48.7959) (end 74.211 48.7016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1732 48.892) (end 74.1874 48.7959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1684 49.0088) (end 74.1732 48.892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1732 49.106) (end 74.1684 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.1874 49.2021) (end 74.1732 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.211 49.2964) (end 74.1874 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2437 49.3879) (end 74.211 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.2853 49.4757) (end 74.2437 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3352 49.559) (end 74.2853 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.3931 49.637) (end 74.3352 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.4583 49.709) (end 74.3931 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.5303 49.7743) (end 74.4583 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6084 49.8321) (end 74.5303 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.6917 49.8821) (end 74.6084 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.7795 49.9236) (end 74.6917 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.871 49.9564) (end 74.7795 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 74.9652 49.98) (end 74.871 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.0613 49.9942) (end 74.9652 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 75.1586 49.999) (end 75.0613 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.896 111.7588) (end 111.0128 111.754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7999 111.7731) (end 110.896 111.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7056 111.7967) (end 110.7999 111.7731) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6141 111.8294) (end 110.7056 111.7967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5263 111.8709) (end 110.6141 111.8294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.443 111.9209) (end 110.5263 111.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.365 111.9788) (end 110.443 111.9209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.293 112.044) (end 110.365 111.9788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2277 112.116) (end 110.293 112.044) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1699 112.194) (end 110.2277 112.116) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1199 112.2774) (end 110.1699 112.194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0784 112.3652) (end 110.1199 112.2774) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0456 112.4566) (end 110.0784 112.3652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.022 112.5509) (end 110.0456 112.4566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0078 112.647) (end 110.022 112.5509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 112.7443) (end 110.0078 112.647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 115.9771) (end 110.003 112.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0043 116.0288) (end 110.003 115.9771) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0071 116.0811) (end 110.0043 116.0288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.018 116.1854) (end 110.0071 116.0811) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0222 116.2113) (end 110.018 116.1854) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0437 116.3125) (end 110.0222 116.2113) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0505 116.3379) (end 110.0437 116.3125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0829 116.4377) (end 110.0505 116.3379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0924 116.4623) (end 110.0829 116.4377) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1344 116.5567) (end 110.0924 116.4623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1464 116.5803) (end 110.1344 116.5567) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1987 116.671) (end 110.1464 116.5803) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2129 116.6928) (end 110.1987 116.671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2741 116.777) (end 110.2129 116.6928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2908 116.7976) (end 110.2741 116.777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3604 116.8748) (end 110.2908 116.7976) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3792 116.8936) (end 110.3604 116.8748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.4564 116.9632) (end 110.3792 116.8936) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.477 116.9799) (end 110.4564 116.9632) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5612 117.0411) (end 110.477 116.9799) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.583 117.0553) (end 110.5612 117.0411) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6737 117.1076) (end 110.583 117.0553) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6973 117.1196) (end 110.6737 117.1076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7917 117.1616) (end 110.6973 117.1196) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.8163 117.1711) (end 110.7917 117.1616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9161 117.2035) (end 110.8163 117.1711) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9415 117.2103) (end 110.9161 117.2035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0427 117.2318) (end 110.9415 117.2103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0686 117.236) (end 111.0427 117.2318) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.1729 117.2469) (end 111.0686 117.236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2769 117.251) (end 111.1729 117.2469) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2446 117.251) (end 111.2769 117.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.33 117.2555) (end 114.2446 117.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3943 117.2653) (end 114.33 117.2555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4199 117.2708) (end 114.3943 117.2653) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4831 117.2881) (end 114.4199 117.2708) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5445 117.3113) (end 114.4831 117.2881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5685 117.322) (end 114.5445 117.3113) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6271 117.3522) (end 114.5685 117.322) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6819 117.3874) (end 114.6271 117.3522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7032 117.4029) (end 114.6819 117.3874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7538 117.4443) (end 114.7032 117.4029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8006 117.4905) (end 114.7538 117.4443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8181 117.51) (end 114.8006 117.4905) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8593 117.5614) (end 114.8181 117.51) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8951 117.6159) (end 114.8593 117.5614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9082 117.6387) (end 114.8951 117.6159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9376 117.6971) (end 114.9082 117.6387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9615 117.7584) (end 114.9376 117.6971) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9695 117.7831) (end 114.9615 117.7584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9862 117.8464) (end 114.9695 117.7831) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9986 117.9246) (end 114.9862 117.8464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.003 118.0095) (end 114.9986 117.9246) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.003 125.4964) (end 115.003 118.0095) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.99 125.7516) (end 115.003 125.4964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9872 125.7775) (end 114.99 125.7516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9504 126.0101) (end 114.9872 125.7775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.945 126.0358) (end 114.9504 126.0101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8801 126.2763) (end 114.945 126.0358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7865 126.5202) (end 114.8801 126.2763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6737 126.7423) (end 114.7865 126.5202) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6606 126.765) (end 114.6737 126.7423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.525 126.9733) (end 114.6606 126.765) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3686 127.1669) (end 114.525 126.9733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.351 127.1865) (end 114.3686 127.1669) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.1751 127.3619) (end 114.351 127.1865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.9716 127.5268) (end 114.1751 127.3619) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.752 127.6694) (end 113.9716 127.5268) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.5187 127.7883) (end 113.752 127.6694) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.2742 127.8821) (end 113.5187 127.7883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.0214 127.9499) (end 113.2742 127.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.7628 127.9909) (end 113.0214 127.9499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.5077 128.0047) (end 112.7628 127.9909) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.826 128.005) (end 112.5077 128.0047) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.7287 128.0098) (end 96.826 128.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.6326 128.024) (end 96.7287 128.0098) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.5384 128.0476) (end 96.6326 128.024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.4469 128.0804) (end 96.5384 128.0476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.3591 128.1219) (end 96.4469 128.0804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.2757 128.1719) (end 96.3591 128.1219) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1977 128.2297) (end 96.2757 128.1719) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1257 128.295) (end 96.1977 128.2297) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0605 128.367) (end 96.1257 128.295) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0026 128.445) (end 96.0605 128.367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9527 128.5283) (end 96.0026 128.445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9111 128.6161) (end 95.9527 128.5283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8784 128.7076) (end 95.9111 128.6161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8548 128.8019) (end 95.8784 128.7076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8405 128.898) (end 95.8548 128.8019) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8358 129.0148) (end 95.8405 128.898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8405 129.112) (end 95.8358 129.0148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8548 129.2081) (end 95.8405 129.112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8784 129.3024) (end 95.8548 129.2081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9111 129.3939) (end 95.8784 129.3024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9527 129.4817) (end 95.9111 129.3939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0026 129.565) (end 95.9527 129.4817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0605 129.643) (end 96.0026 129.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1257 129.715) (end 96.0605 129.643) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1977 129.7803) (end 96.1257 129.715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.2757 129.8381) (end 96.1977 129.7803) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.3591 129.8881) (end 96.2757 129.8381) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.4469 129.9296) (end 96.3591 129.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.5384 129.9624) (end 96.4469 129.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.6326 129.986) (end 96.5384 129.9624) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.7287 130.0002) (end 96.6326 129.986) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.826 130.005) (end 96.7287 130.0002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.4946 130.005) (end 96.826 130.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.5993 130.0025) (end 112.4946 130.005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.8802 129.9875) (end 112.5993 130.0025) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.9977 129.9769) (end 112.8802 129.9875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.063 129.9683) (end 112.9977 129.9769) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.3216 129.9276) (end 113.063 129.9683) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.4115 129.9113) (end 113.3216 129.9276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.5512 129.8788) (end 113.4115 129.9113) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.7788 129.8179) (end 113.5512 129.8788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.8669 129.7921) (end 113.7788 129.8179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.003 129.7451) (end 113.8669 129.7921) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.223 129.6606) (end 114.003 129.7451) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3077 129.6259) (end 114.223 129.6606) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4378 129.565) (end 114.3077 129.6259) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6478 129.4581) (end 114.4378 129.565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7289 129.4144) (end 114.6478 129.4581) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7742 129.3883) (end 114.7289 129.4144) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8526 129.3399) (end 114.7742 129.3883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0718 129.197) (end 114.8526 129.3399) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.1679 129.1293) (end 115.0718 129.197) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2404 129.0732) (end 115.1679 129.1293) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4437 128.9082) (end 115.2404 129.0732) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5323 128.8307) (end 115.4437 128.9082) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.58 128.7855) (end 115.5323 128.8307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7835 128.582) (end 115.58 128.7855) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8635 128.4956) (end 115.7835 128.582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9229 128.4256) (end 115.8635 128.4956) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0712 128.2424) (end 115.9229 128.4256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1579 128.1278) (end 116.0712 128.2424) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2096 128.0519) (end 116.1579 128.1278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3519 127.8322) (end 116.2096 128.0519) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4122 127.7312) (end 116.3519 127.8322) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4556 127.6505) (end 116.4122 127.7312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5627 127.4404) (end 116.4556 127.6505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6237 127.3101) (end 116.5627 127.4404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6586 127.225) (end 116.6237 127.3101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7431 127.0049) (end 116.6586 127.225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7739 126.9188) (end 116.7431 127.0049) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8157 126.7814) (end 116.7739 126.9188) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8768 126.5537) (end 116.8157 126.7814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9094 126.4133) (end 116.8768 126.5537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9259 126.3227) (end 116.9094 126.4133) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9627 126.09) (end 116.9259 126.3227) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9804 125.9475) (end 116.9627 126.09) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9872 125.8561) (end 116.9804 125.9475) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9999 125.6142) (end 116.9872 125.8561) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.003 125.4965) (end 116.9999 125.6142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0029 117.9965) (end 117.003 125.4965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0005 117.9052) (end 117.0029 117.9965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9952 117.8071) (end 117.0005 117.9052) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9845 117.6895) (end 116.9952 117.8071) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9759 117.6241) (end 116.9845 117.6895) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.964 117.5465) (end 116.9759 117.6241) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9475 117.4557) (end 116.964 117.5465) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9211 117.3402) (end 116.9475 117.4557) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.894 117.2392) (end 116.9211 117.3402) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8596 117.128) (end 116.894 117.2392) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8379 117.0668) (end 116.8596 117.128) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8102 116.9935) (end 116.8379 117.0668) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7754 116.9085) (end 116.8102 116.9935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7143 116.7779) (end 116.7754 116.9085) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6469 116.6501) (end 116.7143 116.7779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5724 116.5266) (end 116.6469 116.6501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4921 116.4068) (end 116.5724 116.5266) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4052 116.2918) (end 116.4921 116.4068) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3554 116.231) (end 116.4052 116.2918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2781 116.1426) (end 116.3554 116.231) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1776 116.0392) (end 116.2781 116.1426) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0729 115.9412) (end 116.1776 116.0392) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9621 115.8488) (end 116.0729 115.9412) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8473 115.762) (end 115.9621 115.8488) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7273 115.6816) (end 115.8473 115.762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.604 115.6072) (end 115.7273 115.6816) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5229 115.5636) (end 115.604 115.6072) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4527 115.5282) (end 115.5229 115.5636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.3456 115.4787) (end 115.4527 115.5282) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2847 115.4535) (end 115.3456 115.4787) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.1872 115.4161) (end 115.2847 115.4535) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0771 115.3785) (end 115.1872 115.4161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9392 115.3394) (end 115.0771 115.3785) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8496 115.3175) (end 114.9392 115.3394) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7334 115.2945) (end 114.8496 115.3175) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6299 115.2781) (end 114.7334 115.2945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5126 115.264) (end 114.6299 115.2781) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4208 115.2571) (end 114.5126 115.264) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3161 115.2522) (end 114.4208 115.2571) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2445 115.251) (end 114.3161 115.2522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0275 115.251) (end 114.2445 115.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0122 115.2502) (end 112.0275 115.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.007 115.2477) (end 112.0122 115.2502) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0038 115.2418) (end 112.007 115.2477) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 115.2265) (end 112.0038 115.2418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 112.7443) (end 112.003 115.2265) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9982 112.647) (end 112.003 112.7443) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.984 112.5509) (end 111.9982 112.647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9604 112.4566) (end 111.984 112.5509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9276 112.3652) (end 111.9604 112.4566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8861 112.2774) (end 111.9276 112.3652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8361 112.194) (end 111.8861 112.2774) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.7783 112.116) (end 111.8361 112.194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.713 112.044) (end 111.7783 112.116) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.641 111.9788) (end 111.713 112.044) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.563 111.9209) (end 111.641 111.9788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.4797 111.8709) (end 111.563 111.9209) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3919 111.8294) (end 111.4797 111.8709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3004 111.7967) (end 111.3919 111.8294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2061 111.7731) (end 111.3004 111.7967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.11 111.7588) (end 111.2061 111.7731) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0128 111.754) (end 111.11 111.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.11 66.2452) (end 110.9932 66.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2061 66.231) (end 111.11 66.2452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3004 66.2074) (end 111.2061 66.231) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3919 66.1746) (end 111.3004 66.2074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.4797 66.1331) (end 111.3919 66.1746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.563 66.0832) (end 111.4797 66.1331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.641 66.0253) (end 111.563 66.0832) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.713 65.96) (end 111.641 66.0253) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.7783 65.8881) (end 111.713 65.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8361 65.81) (end 111.7783 65.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8861 65.7267) (end 111.8361 65.81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9276 65.6389) (end 111.8861 65.7267) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9604 65.5474) (end 111.9276 65.6389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.984 65.4531) (end 111.9604 65.5474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9982 65.357) (end 111.984 65.4531) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 65.2598) (end 111.9982 65.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 59.7775) (end 112.003 65.2598) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0038 59.7622) (end 112.003 59.7775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0056 59.7577) (end 112.0038 59.7622) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0113 59.754) (end 112.0056 59.7577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0275 59.753) (end 112.0113 59.754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2445 59.753) (end 112.0275 59.753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3161 59.7518) (end 114.2445 59.753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4208 59.7469) (end 114.3161 59.7518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5125 59.74) (end 114.4208 59.7469) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6299 59.7259) (end 114.5125 59.74) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7332 59.7096) (end 114.6299 59.7259) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8484 59.6868) (end 114.7332 59.7096) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.988 59.6516) (end 114.8484 59.6868) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0764 59.6258) (end 114.988 59.6516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.1883 59.5876) (end 115.0764 59.6258) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.286 59.55) (end 115.1883 59.5876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.3937 59.5039) (end 115.286 59.55) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4528 59.4758) (end 115.3937 59.5039) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5229 59.4404) (end 115.4528 59.4758) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.6041 59.3967) (end 115.5229 59.4404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.6495 59.3705) (end 115.6041 59.3967) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.728 59.322) (end 115.6495 59.3705) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8476 59.2418) (end 115.728 59.322) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9619 59.1554) (end 115.8476 59.2418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0226 59.1057) (end 115.9619 59.1554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1105 59.029) (end 116.0226 59.1057) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2134 58.9291) (end 116.1105 59.029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2778 58.8618) (end 116.2134 58.9291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3132 58.8225) (end 116.2778 58.8618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4064 58.7106) (end 116.3132 58.8225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4921 58.5972) (end 116.4064 58.7106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.572 58.478) (end 116.4921 58.5972) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6205 58.3996) (end 116.572 58.478) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6467 58.3542) (end 116.6205 58.3996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7143 58.226) (end 116.6467 58.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.775 58.0965) (end 116.7143 58.226) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8096 58.0119) (end 116.775 58.0965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8376 57.9383) (end 116.8096 58.0119) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8758 57.8261) (end 116.8376 57.9383) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8946 57.7626) (end 116.8758 57.8261) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9153 57.6866) (end 116.8946 57.7626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9369 57.5979) (end 116.9153 57.6866) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9596 57.4827) (end 116.9369 57.5979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9723 57.4051) (end 116.9596 57.4827) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.99 57.2625) (end 116.9723 57.4051) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9969 57.1709) (end 116.99 57.2625) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0025 57.0403) (end 116.9969 57.1709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.003 52.5075) (end 117.0025 57.0403) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0005 52.4028) (end 117.003 52.5075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9872 52.1479) (end 117.0005 52.4028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.975 52.0049) (end 116.9872 52.1479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9627 51.914) (end 116.975 52.0049) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9214 51.6555) (end 116.9627 51.914) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8986 51.5398) (end 116.9214 51.6555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8768 51.4503) (end 116.8986 51.5398) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8157 51.2226) (end 116.8768 51.4503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.774 51.0853) (end 116.8157 51.2226) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7431 50.9991) (end 116.774 51.0853) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6586 50.779) (end 116.7431 50.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6239 50.6943) (end 116.6586 50.779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.563 50.5642) (end 116.6239 50.6943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4561 50.3542) (end 116.563 50.5642) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4124 50.2731) (end 116.4561 50.3542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3518 50.1715) (end 116.4124 50.2731) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2095 49.9518) (end 116.3518 50.1715) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1579 49.8761) (end 116.2095 49.9518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0712 49.7616) (end 116.1579 49.8761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9228 49.5783) (end 116.0712 49.7616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8636 49.5084) (end 115.9228 49.5783) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7835 49.422) (end 115.8636 49.5084) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5986 49.2367) (end 115.7835 49.422) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5324 49.1733) (end 115.5986 49.2367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4237 49.0792) (end 115.5324 49.1733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2404 48.9307) (end 115.4237 49.0792) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.168 48.8747) (end 115.2404 48.9307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0718 48.807) (end 115.168 48.8747) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8526 48.6641) (end 115.0718 48.807) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7743 48.6157) (end 114.8526 48.6641) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.729 48.5896) (end 114.7743 48.6157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6478 48.5459) (end 114.729 48.5896) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4378 48.439) (end 114.6478 48.5459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3078 48.3781) (end 114.4378 48.439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.223 48.3434) (end 114.3078 48.3781) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.003 48.2589) (end 114.223 48.3434) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.867 48.2119) (end 114.003 48.2589) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.7788 48.1861) (end 113.867 48.2119) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.5512 48.1252) (end 113.7788 48.1861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.4116 48.0927) (end 113.5512 48.1252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.3216 48.0764) (end 113.4116 48.0927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.063 48.0357) (end 113.3216 48.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.9459 48.0216) (end 113.063 48.0357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.8802 48.0165) (end 112.9459 48.0216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.5992 48.0015) (end 112.8802 48.0165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.4945 47.999) (end 112.5992 48.0015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.826 47.999) (end 112.4945 47.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.7287 48.0038) (end 96.826 47.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.6326 48.018) (end 96.7287 48.0038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.5384 48.0416) (end 96.6326 48.018) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.4469 48.0744) (end 96.5384 48.0416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.3591 48.1159) (end 96.4469 48.0744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.2757 48.1659) (end 96.3591 48.1159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1977 48.2237) (end 96.2757 48.1659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1257 48.289) (end 96.1977 48.2237) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0605 48.361) (end 96.1257 48.289) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0026 48.439) (end 96.0605 48.361) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9527 48.5223) (end 96.0026 48.439) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9111 48.6101) (end 95.9527 48.5223) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8784 48.7016) (end 95.9111 48.6101) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8548 48.7959) (end 95.8784 48.7016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8405 48.892) (end 95.8548 48.7959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8358 49.0088) (end 95.8405 48.892) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8405 49.106) (end 95.8358 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8548 49.2021) (end 95.8405 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8784 49.2964) (end 95.8548 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9111 49.3879) (end 95.8784 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9527 49.4757) (end 95.9111 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0026 49.559) (end 95.9527 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0605 49.637) (end 96.0026 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1257 49.709) (end 96.0605 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1977 49.7743) (end 96.1257 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.2757 49.8321) (end 96.1977 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.3591 49.8821) (end 96.2757 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.4469 49.9236) (end 96.3591 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.5384 49.9564) (end 96.4469 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.6326 49.98) (end 96.5384 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.7287 49.9942) (end 96.6326 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.826 49.999) (end 96.7287 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.5076 49.9993) (end 96.826 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.7629 50.0131) (end 112.5076 49.9993) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.0214 50.0541) (end 112.7629 50.0131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.2743 50.1219) (end 113.0214 50.0541) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.5187 50.2157) (end 113.2743 50.1219) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.7521 50.3346) (end 113.5187 50.2157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.9716 50.4772) (end 113.7521 50.3346) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.1752 50.6421) (end 113.9716 50.4772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.351 50.8175) (end 114.1752 50.6421) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3686 50.837) (end 114.351 50.8175) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5248 51.0304) (end 114.3686 50.837) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6607 51.2389) (end 114.5248 51.0304) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6739 51.2618) (end 114.6607 51.2389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7865 51.4838) (end 114.6739 51.2618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8801 51.7278) (end 114.7865 51.4838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.945 51.9681) (end 114.8801 51.7278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9504 51.9939) (end 114.945 51.9681) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.989 52.2398) (end 114.9504 51.9939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.003 52.5075) (end 114.989 52.2398) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0029 57.0009) (end 115.003 52.5075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9996 57.0666) (end 115.0029 57.0009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9968 57.0925) (end 114.9996 57.0666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9863 57.157) (end 114.9968 57.0925) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9697 57.2205) (end 114.9863 57.157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9615 57.2457) (end 114.9697 57.2205) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9378 57.3065) (end 114.9615 57.2457) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9021 57.3766) (end 114.9378 57.3065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8589 57.4431) (end 114.9021 57.3766) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8183 57.4939) (end 114.8589 57.4431) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8004 57.5137) (end 114.8183 57.4939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7537 57.5598) (end 114.8004 57.5137) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7033 57.6011) (end 114.7537 57.5598) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6381 57.645) (end 114.7033 57.6011) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6152 57.6583) (end 114.6381 57.645) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5569 57.6876) (end 114.6152 57.6583) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4834 57.7158) (end 114.5569 57.6876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4076 57.7362) (end 114.4834 57.7158) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3299 57.7485) (end 114.4076 57.7362) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2445 57.753) (end 114.3299 57.7485) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2769 57.753) (end 114.2445 57.753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.1729 57.7571) (end 111.2769 57.753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0686 57.768) (end 111.1729 57.7571) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0427 57.7722) (end 111.0686 57.768) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9415 57.7937) (end 111.0427 57.7722) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9161 57.8005) (end 110.9415 57.7937) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.8163 57.8329) (end 110.9161 57.8005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7917 57.8424) (end 110.8163 57.8329) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6973 57.8844) (end 110.7917 57.8424) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6737 57.8964) (end 110.6973 57.8844) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.583 57.9487) (end 110.6737 57.8964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5612 57.9629) (end 110.583 57.9487) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.477 58.0241) (end 110.5612 57.9629) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.4564 58.0408) (end 110.477 58.0241) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3792 58.1104) (end 110.4564 58.0408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3604 58.1292) (end 110.3792 58.1104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2908 58.2064) (end 110.3604 58.1292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2741 58.227) (end 110.2908 58.2064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2129 58.3112) (end 110.2741 58.227) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1987 58.333) (end 110.2129 58.3112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1464 58.4237) (end 110.1987 58.333) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1344 58.4473) (end 110.1464 58.4237) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0924 58.5417) (end 110.1344 58.4473) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0829 58.5663) (end 110.0924 58.5417) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0505 58.6661) (end 110.0829 58.5663) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0437 58.6915) (end 110.0505 58.6661) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0222 58.7927) (end 110.0437 58.6915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.018 58.8186) (end 110.0222 58.7927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0071 58.9229) (end 110.018 58.8186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 59.0269) (end 110.0071 58.9229) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 65.2598) (end 110.003 59.0269) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0078 65.357) (end 110.003 65.2598) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.022 65.4531) (end 110.0078 65.357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0456 65.5474) (end 110.022 65.4531) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0784 65.6389) (end 110.0456 65.5474) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1199 65.7267) (end 110.0784 65.6389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1699 65.81) (end 110.1199 65.7267) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2277 65.8881) (end 110.1699 65.81) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.293 65.96) (end 110.2277 65.8881) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.365 66.0253) (end 110.293 65.96) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.443 66.0832) (end 110.365 66.0253) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5263 66.1331) (end 110.443 66.0832) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6141 66.1746) (end 110.5263 66.1331) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7056 66.2074) (end 110.6141 66.1746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7999 66.231) (end 110.7056 66.2074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.896 66.2452) (end 110.7999 66.231) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9932 66.25) (end 110.896 66.2452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.5076 90.5013) (end 96.826 90.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.7629 90.5151) (end 112.5076 90.5013) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.0214 90.5561) (end 112.7629 90.5151) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.2743 90.6239) (end 113.0214 90.5561) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.5187 90.7177) (end 113.2743 90.6239) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.7516 90.8363) (end 113.5187 90.7177) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.9712 90.9789) (end 113.7516 90.8363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.1748 91.1438) (end 113.9712 90.9789) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3599 91.3289) (end 114.1748 91.1438) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5248 91.5324) (end 114.3599 91.3289) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6607 91.7409) (end 114.5248 91.5324) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6739 91.7638) (end 114.6607 91.7409) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7863 91.9853) (end 114.6739 91.7638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8801 92.2298) (end 114.7863 91.9853) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.945 92.4701) (end 114.8801 92.2298) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9504 92.4959) (end 114.945 92.4701) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.989 92.7418) (end 114.9504 92.4959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.003 93.0095) (end 114.989 92.7418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0029 97.5029) (end 115.003 93.0095) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9996 97.5686) (end 115.0029 97.5029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9968 97.5945) (end 114.9996 97.5686) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9863 97.659) (end 114.9968 97.5945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9697 97.7225) (end 114.9863 97.659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9615 97.7477) (end 114.9697 97.7225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9378 97.8085) (end 114.9615 97.7477) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9021 97.8786) (end 114.9378 97.8085) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8589 97.9451) (end 114.9021 97.8786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8183 97.9959) (end 114.8589 97.9451) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8004 98.0157) (end 114.8183 97.9959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7537 98.0618) (end 114.8004 98.0157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7033 98.1031) (end 114.7537 98.0618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6381 98.147) (end 114.7033 98.1031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6152 98.1603) (end 114.6381 98.147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5569 98.1896) (end 114.6152 98.1603) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4834 98.2178) (end 114.5569 98.1896) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4076 98.2382) (end 114.4834 98.2178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3299 98.2505) (end 114.4076 98.2382) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2445 98.255) (end 114.3299 98.2505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2769 98.255) (end 114.2445 98.255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.1729 98.2591) (end 111.2769 98.255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0686 98.27) (end 111.1729 98.2591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0427 98.2742) (end 111.0686 98.27) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9415 98.2957) (end 111.0427 98.2742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9161 98.3025) (end 110.9415 98.2957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.8163 98.3349) (end 110.9161 98.3025) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7917 98.3444) (end 110.8163 98.3349) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6973 98.3864) (end 110.7917 98.3444) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6737 98.3984) (end 110.6973 98.3864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.583 98.4507) (end 110.6737 98.3984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5612 98.4649) (end 110.583 98.4507) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.477 98.5261) (end 110.5612 98.4649) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.4564 98.5428) (end 110.477 98.5261) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3792 98.6124) (end 110.4564 98.5428) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3604 98.6312) (end 110.3792 98.6124) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2908 98.7084) (end 110.3604 98.6312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2741 98.729) (end 110.2908 98.7084) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2129 98.8132) (end 110.2741 98.729) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1987 98.835) (end 110.2129 98.8132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1464 98.9257) (end 110.1987 98.835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1344 98.9493) (end 110.1464 98.9257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0924 99.0437) (end 110.1344 98.9493) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0829 99.0683) (end 110.0924 99.0437) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0505 99.1681) (end 110.0829 99.0683) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0437 99.1935) (end 110.0505 99.1681) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0222 99.2947) (end 110.0437 99.1935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.018 99.3206) (end 110.0222 99.2947) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0071 99.4249) (end 110.018 99.3206) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 99.5289) (end 110.0071 99.4249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 105.7618) (end 110.003 99.5289) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0078 105.8591) (end 110.003 105.7618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.022 105.9552) (end 110.0078 105.8591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0456 106.0494) (end 110.022 105.9552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0784 106.1409) (end 110.0456 106.0494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1199 106.2287) (end 110.0784 106.1409) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1699 106.312) (end 110.1199 106.2287) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2277 106.3901) (end 110.1699 106.312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.293 106.4621) (end 110.2277 106.3901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.365 106.5273) (end 110.293 106.4621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.443 106.5852) (end 110.365 106.5273) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5263 106.6351) (end 110.443 106.5852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6141 106.6767) (end 110.5263 106.6351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7056 106.7094) (end 110.6141 106.6767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7999 106.733) (end 110.7056 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.896 106.7472) (end 110.7999 106.733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9932 106.752) (end 110.896 106.7472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.11 106.7472) (end 110.9932 106.752) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2061 106.733) (end 111.11 106.7472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3004 106.7094) (end 111.2061 106.733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3919 106.6767) (end 111.3004 106.7094) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.4797 106.6351) (end 111.3919 106.6767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.563 106.5852) (end 111.4797 106.6351) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.641 106.5273) (end 111.563 106.5852) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.713 106.4621) (end 111.641 106.5273) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.7783 106.3901) (end 111.713 106.4621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8361 106.312) (end 111.7783 106.3901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8861 106.2287) (end 111.8361 106.312) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9276 106.1409) (end 111.8861 106.2287) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9604 106.0494) (end 111.9276 106.1409) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.984 105.9552) (end 111.9604 106.0494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9982 105.8591) (end 111.984 105.9552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 105.7618) (end 111.9982 105.8591) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 100.2795) (end 112.003 105.7618) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0051 100.2605) (end 112.003 100.2795) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0113 100.256) (end 112.0051 100.2605) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0275 100.255) (end 112.0113 100.256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2445 100.255) (end 112.0275 100.255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3161 100.2538) (end 114.2445 100.255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4469 100.2472) (end 114.3161 100.2538) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5645 100.2365) (end 114.4469 100.2472) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7076 100.216) (end 114.5645 100.2365) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8484 100.1888) (end 114.7076 100.216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9374 100.1671) (end 114.8484 100.1888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0132 100.1465) (end 114.9374 100.1671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.1261 100.1116) (end 115.0132 100.1465) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2619 100.0616) (end 115.1261 100.1116) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.3937 100.0059) (end 115.2619 100.0616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.476 99.9663) (end 115.3937 100.0059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5461 99.9302) (end 115.476 99.9663) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.6495 99.8725) (end 115.5461 99.9302) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7058 99.838) (end 115.6495 99.8725) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7721 99.7953) (end 115.7058 99.838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8476 99.7438) (end 115.7721 99.7953) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9415 99.6734) (end 115.8476 99.7438) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0028 99.6243) (end 115.9415 99.6734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1105 99.531) (end 116.0028 99.6243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2134 99.4311) (end 116.1105 99.531) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2778 99.3638) (end 116.2134 99.4311) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3132 99.3245) (end 116.2778 99.3638) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3735 99.2534) (end 116.3132 99.3245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4619 99.1408) (end 116.3735 99.2534) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5289 99.0456) (end 116.4619 99.1408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.572 98.98) (end 116.5289 99.0456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6205 98.9016) (end 116.572 98.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6467 98.8562) (end 116.6205 98.9016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6904 98.7749) (end 116.6467 98.8562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7258 98.7048) (end 116.6904 98.7749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.775 98.5985) (end 116.7258 98.7048) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8 98.538) (end 116.775 98.5985) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8285 98.4649) (end 116.8 98.538) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8596 98.378) (end 116.8285 98.4649) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8758 98.3281) (end 116.8596 98.378) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9017 98.2393) (end 116.8758 98.3281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9217 98.1635) (end 116.9017 98.2393) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9477 98.0491) (end 116.9217 98.1635) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9723 97.9071) (end 116.9477 98.0491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9846 97.8162) (end 116.9723 97.9071) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9951 97.6989) (end 116.9846 97.8162) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0018 97.5683) (end 116.9951 97.6989) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.003 97.4965) (end 117.0018 97.5683) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0025 92.9637) (end 117.003 97.4965) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9999 92.8918) (end 117.0025 92.9637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9855 92.6239) (end 116.9999 92.8918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.975 92.5069) (end 116.9855 92.6239) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9627 92.416) (end 116.975 92.5069) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9259 92.1833) (end 116.9627 92.416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8986 92.0418) (end 116.9259 92.1833) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8768 91.9523) (end 116.8986 92.0418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8157 91.7246) (end 116.8768 91.9523) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.79 91.6368) (end 116.8157 91.7246) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7521 91.5255) (end 116.79 91.6368) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6586 91.281) (end 116.7521 91.5255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6239 91.1963) (end 116.6586 91.281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.563 91.0662) (end 116.6239 91.1963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4561 90.8562) (end 116.563 91.0662) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4124 90.7751) (end 116.4561 90.8562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3863 90.7298) (end 116.4124 90.7751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3379 90.6514) (end 116.3863 90.7298) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2095 90.4538) (end 116.3379 90.6514) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1579 90.3781) (end 116.2095 90.4538) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0712 90.2636) (end 116.1579 90.3781) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9228 90.0803) (end 116.0712 90.2636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8636 90.0104) (end 115.9228 90.0803) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7835 89.924) (end 115.8636 90.0104) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5986 89.7387) (end 115.7835 89.924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5324 89.6753) (end 115.5986 89.7387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4237 89.5812) (end 115.5324 89.6753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2404 89.4327) (end 115.4237 89.5812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.168 89.3767) (end 115.2404 89.4327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0718 89.309) (end 115.168 89.3767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8526 89.1661) (end 115.0718 89.309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7743 89.1177) (end 114.8526 89.1661) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.729 89.0916) (end 114.7743 89.1177) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5752 89.0107) (end 114.729 89.0916) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5717 89.0072) (end 114.5752 89.0107) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5702 89.0025) (end 114.5717 89.0072) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5712 88.9977) (end 114.5702 89.0025) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5752 88.9933) (end 114.5712 88.9977) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7289 88.9124) (end 114.5752 88.9933) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8305 88.8518) (end 114.7289 88.9124) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0502 88.7095) (end 114.8305 88.8518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.1259 88.6579) (end 115.0502 88.7095) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2404 88.5712) (end 115.1259 88.6579) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4237 88.4228) (end 115.2404 88.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4936 88.3636) (end 115.4237 88.4228) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.5986 88.2653) (end 115.4936 88.3636) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7653 88.0986) (end 115.5986 88.2653) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8635 87.9936) (end 115.7653 88.0986) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9229 87.9236) (end 115.8635 87.9936) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.0712 87.7404) (end 115.9229 87.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1579 87.6258) (end 116.0712 87.7404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2096 87.5499) (end 116.1579 87.6258) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.338 87.3522) (end 116.2096 87.5499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4122 87.2292) (end 116.338 87.3522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4556 87.1485) (end 116.4122 87.2292) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5742 86.915) (end 116.4556 87.1485) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6237 86.8081) (end 116.5742 86.915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6586 86.723) (end 116.6237 86.8081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7431 86.5029) (end 116.6586 86.723) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.79 86.3673) (end 116.7431 86.5029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8157 86.2794) (end 116.79 86.3673) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8768 86.0517) (end 116.8157 86.2794) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8986 85.9623) (end 116.8768 86.0517) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9214 85.8465) (end 116.8986 85.9623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9664 85.5622) (end 116.9214 85.8465) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9804 85.4455) (end 116.9664 85.5622) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9872 85.3541) (end 116.9804 85.4455) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0005 85.0992) (end 116.9872 85.3541) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.003 84.9945) (end 117.0005 85.0992) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.003 77.5075) (end 117.003 84.9945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9999 77.3903) (end 117.003 77.5075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9952 77.3051) (end 116.9999 77.3903) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9845 77.1875) (end 116.9952 77.3051) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9722 77.0962) (end 116.9845 77.1875) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9595 77.0187) (end 116.9722 77.0962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9366 76.9025) (end 116.9595 77.0187) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9211 76.8382) (end 116.9366 76.9025) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.894 76.7372) (end 116.9211 76.8382) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8596 76.626) (end 116.894 76.7372) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8102 76.4915) (end 116.8596 76.626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7754 76.4065) (end 116.8102 76.4915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7258 76.2993) (end 116.7754 76.4065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6904 76.2291) (end 116.7258 76.2993) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6469 76.1481) (end 116.6904 76.2291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5864 76.0467) (end 116.6469 76.1481) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5293 75.959) (end 116.5864 76.0467) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4614 75.8626) (end 116.5293 75.959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4052 75.7898) (end 116.4614 75.8626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3129 75.6792) (end 116.4052 75.7898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2148 75.5744) (end 116.3129 75.6792) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.1115 75.4739) (end 116.2148 75.5744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.023 75.3966) (end 116.1115 75.4739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.9417 75.3307) (end 116.023 75.3966) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.8473 75.26) (end 115.9417 75.3307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7713 75.2082) (end 115.8473 75.26) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.7053 75.1656) (end 115.7713 75.2082) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.604 75.1052) (end 115.7053 75.1656) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.4761 75.0377) (end 115.604 75.1052) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.3456 74.9767) (end 115.4761 75.0377) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.2605 74.9418) (end 115.3456 74.9767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.1261 74.8924) (end 115.2605 74.9418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.0148 74.858) (end 115.1261 74.8924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9138 74.8309) (end 115.0148 74.858) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7984 74.8045) (end 114.9138 74.8309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7075 74.788) (end 114.7984 74.8045) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6299 74.7761) (end 114.7075 74.788) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5126 74.762) (end 114.6299 74.7761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4208 74.7551) (end 114.5126 74.762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3161 74.7502) (end 114.4208 74.7551) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2445 74.749) (end 114.3161 74.7502) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0275 74.749) (end 114.2445 74.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.0085 74.7469) (end 112.0275 74.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.004 74.7407) (end 112.0085 74.7469) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 74.7245) (end 112.004 74.7407) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.003 72.2423) (end 112.003 74.7245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9982 72.145) (end 112.003 72.2423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.984 72.0489) (end 111.9982 72.145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9604 71.9546) (end 111.984 72.0489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.9276 71.8632) (end 111.9604 71.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8861 71.7753) (end 111.9276 71.8632) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.8361 71.692) (end 111.8861 71.7753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.7783 71.614) (end 111.8361 71.692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.713 71.542) (end 111.7783 71.614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.641 71.4767) (end 111.713 71.542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.563 71.4189) (end 111.641 71.4767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.4797 71.3689) (end 111.563 71.4189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3919 71.3274) (end 111.4797 71.3689) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.3004 71.2946) (end 111.3919 71.3274) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2061 71.271) (end 111.3004 71.2946) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.11 71.2568) (end 111.2061 71.271) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9932 71.252) (end 111.11 71.2568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.896 71.2568) (end 110.9932 71.252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7999 71.271) (end 110.896 71.2568) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7056 71.2946) (end 110.7999 71.271) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6141 71.3274) (end 110.7056 71.2946) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5263 71.3689) (end 110.6141 71.3274) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.443 71.4189) (end 110.5263 71.3689) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.365 71.4767) (end 110.443 71.4189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.293 71.542) (end 110.365 71.4767) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2277 71.614) (end 110.293 71.542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1699 71.692) (end 110.2277 71.614) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1199 71.7753) (end 110.1699 71.692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0784 71.8632) (end 110.1199 71.7753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0456 71.9546) (end 110.0784 71.8632) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.022 72.0489) (end 110.0456 71.9546) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0078 72.145) (end 110.022 72.0489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 72.2423) (end 110.0078 72.145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.003 75.4751) (end 110.003 72.2423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0043 75.5268) (end 110.003 75.4751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0071 75.5791) (end 110.0043 75.5268) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.018 75.6834) (end 110.0071 75.5791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0222 75.7093) (end 110.018 75.6834) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0437 75.8105) (end 110.0222 75.7093) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0505 75.8359) (end 110.0437 75.8105) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0829 75.9357) (end 110.0505 75.8359) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0924 75.9603) (end 110.0829 75.9357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1344 76.0547) (end 110.0924 75.9603) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1464 76.0783) (end 110.1344 76.0547) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1987 76.169) (end 110.1464 76.0783) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2129 76.1908) (end 110.1987 76.169) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2741 76.275) (end 110.2129 76.1908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2908 76.2956) (end 110.2741 76.275) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3604 76.3728) (end 110.2908 76.2956) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.3792 76.3916) (end 110.3604 76.3728) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.4564 76.4612) (end 110.3792 76.3916) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.477 76.4779) (end 110.4564 76.4612) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.5612 76.5391) (end 110.477 76.4779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.583 76.5533) (end 110.5612 76.5391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6737 76.6056) (end 110.583 76.5533) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.6973 76.6176) (end 110.6737 76.6056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.7917 76.6596) (end 110.6973 76.6176) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.8163 76.6691) (end 110.7917 76.6596) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9161 76.7015) (end 110.8163 76.6691) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.9415 76.7083) (end 110.9161 76.7015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0427 76.7298) (end 110.9415 76.7083) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.0686 76.734) (end 111.0427 76.7298) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.1729 76.7449) (end 111.0686 76.734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 111.2769 76.749) (end 111.1729 76.7449) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.2446 76.749) (end 111.2769 76.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3294 76.7534) (end 114.2446 76.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4076 76.7658) (end 114.3294 76.7534) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4708 76.7825) (end 114.4076 76.7658) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.4955 76.7905) (end 114.4708 76.7825) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.5564 76.8142) (end 114.4955 76.7905) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6152 76.8437) (end 114.5564 76.8142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.638 76.8569) (end 114.6152 76.8437) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6926 76.8927) (end 114.638 76.8569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.744 76.9339) (end 114.6926 76.8927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7634 76.9514) (end 114.744 76.9339) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8094 76.9979) (end 114.7634 76.9514) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8511 77.0488) (end 114.8094 76.9979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8666 77.0701) (end 114.8511 77.0488) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9018 77.125) (end 114.8666 77.0701) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.932 77.1834) (end 114.9018 77.125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9427 77.2075) (end 114.932 77.1834) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9659 77.269) (end 114.9427 77.2075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9832 77.332) (end 114.9659 77.269) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9886 77.3577) (end 114.9832 77.332) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9985 77.4221) (end 114.9886 77.3577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.003 77.5075) (end 114.9985 77.4221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.003 84.9944) (end 115.003 77.5075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.989 85.2622) (end 115.003 84.9944) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.9481 85.5208) (end 114.989 85.2622) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8803 85.7738) (end 114.9481 85.5208) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.7865 86.0182) (end 114.8803 85.7738) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.6676 86.2516) (end 114.7865 86.0182) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.525 86.4713) (end 114.6676 86.2516) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3602 86.6748) (end 114.525 86.4713) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.1751 86.8599) (end 114.3602 86.6748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.9716 87.0248) (end 114.1751 86.8599) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.7631 87.1607) (end 113.9716 87.0248) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.7402 87.1739) (end 113.7631 87.1607) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.5182 87.2865) (end 113.7402 87.1739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.2742 87.3801) (end 113.5182 87.2865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.0339 87.4449) (end 113.2742 87.3801) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.0083 87.4503) (end 113.0339 87.4449) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.7623 87.489) (end 113.0083 87.4503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 112.5012 87.5029) (end 112.7623 87.489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.826 87.503) (end 112.5012 87.5029) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.7287 87.5078) (end 96.826 87.503) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.6326 87.522) (end 96.7287 87.5078) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.5384 87.5456) (end 96.6326 87.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.4469 87.5784) (end 96.5384 87.5456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.3591 87.6199) (end 96.4469 87.5784) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.2757 87.6699) (end 96.3591 87.6199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1977 87.7277) (end 96.2757 87.6699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1257 87.793) (end 96.1977 87.7277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0605 87.865) (end 96.1257 87.793) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0026 87.943) (end 96.0605 87.865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9527 88.0263) (end 96.0026 87.943) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9111 88.1141) (end 95.9527 88.0263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8784 88.2056) (end 95.9111 88.1141) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8548 88.2999) (end 95.8784 88.2056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8405 88.396) (end 95.8548 88.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8358 88.4932) (end 95.8405 88.396) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8358 89.5108) (end 95.8358 88.4932) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8405 89.608) (end 95.8358 89.5108) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8548 89.7041) (end 95.8405 89.608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.8784 89.7984) (end 95.8548 89.7041) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9111 89.8899) (end 95.8784 89.7984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.9527 89.9777) (end 95.9111 89.8899) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0026 90.061) (end 95.9527 89.9777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.0605 90.139) (end 96.0026 90.061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1257 90.211) (end 96.0605 90.139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.1977 90.2763) (end 96.1257 90.211) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.2757 90.3341) (end 96.1977 90.2763) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.3591 90.3841) (end 96.2757 90.3341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.4469 90.4256) (end 96.3591 90.3841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.5384 90.4584) (end 96.4469 90.4256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.6326 90.482) (end 96.5384 90.4584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.7287 90.4962) (end 96.6326 90.482) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 96.826 90.501) (end 96.7287 90.4962) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0019 44.0112) (end 45.0011 44.0261) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.005 44.0053) (end 45.0019 44.0112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0103 44.0028) (end 45.005 44.0053) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0256 44.002) (end 45.0103 44.0028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.9765 44.002) (end 45.0256 44.002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.9919 44.0028) (end 119.9765 44.002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.9978 44.006) (end 119.9919 44.0028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.0003 44.0112) (end 119.9978 44.006) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.0011 44.0266) (end 120.0003 44.0112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.0011 133.9775) (end 120.0011 44.0266) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.0003 133.9928) (end 120.0011 133.9775) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.9971 133.9987) (end 120.0003 133.9928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.9919 134.0012) (end 119.9971 133.9987) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.9765 134.002) (end 119.9919 134.0012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0256 134.002) (end 119.9765 134.002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0103 134.0012) (end 45.0256 134.002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0043 133.9981) (end 45.0103 134.0012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0019 133.9928) (end 45.0043 133.9981) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0011 133.9775) (end 45.0019 133.9928) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 45.0011 44.0261) (end 45.0011 133.9775) (layer Edge.Cuts) (width 0.1))
  (zone (net 33) (net_name Board_1-Board_1-GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.308) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 115.251001 88.001001) (xy 49.501001 88.001001) (xy 49.501001 49.501001) (xy 69.501001 49.501001) (xy 115.251001 49.501001)
      )
    )
  )
  (zone (net 33) (net_name Board_1-Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.308) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 115.251001 88.001001) (xy 49.501001 88.001001) (xy 49.501001 49.501001) (xy 69.501001 49.501001) (xy 115.251001 49.501001)
      )
    )
  )
  (zone (net 34) (net_name Board_1-Board_1-GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.152))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 56.101001 75.576001) (xy 56.101001 82.376001) (xy 54.076001 82.376001) (xy 51.301001 78.926001) (xy 51.301001 75.051001)
        (xy 55.576001 75.051001) (xy 56.401001 74.226001) (xy 56.951001 74.726001)
      )
    )
  )
  (zone (net 1) (net_name Board_1-Board_1-+3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.318) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 89.686001 54.421001) (xy 89.686001 55.501001) (xy 88.301001 55.501001) (xy 87.666001 55.501001) (xy 87.666001 55.131001)
        (xy 87.666001 53.821001) (xy 89.686001 53.821001)
      )
    )
  )
  (zone (net 34) (net_name Board_1-Board_1-GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.152))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 56.101001 75.576001) (xy 56.101001 82.376001) (xy 54.076001 82.376001) (xy 51.301001 78.926001) (xy 51.301001 75.051001)
        (xy 55.576001 75.051001) (xy 56.401001 74.226001) (xy 56.951001 74.726001)
      )
    )
  )
  (zone (net 86) (net_name Board_2-Board_1-GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.308) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 115.251001 128.50302) (xy 49.501001 128.50302) (xy 49.501001 90.00302) (xy 69.501001 90.00302) (xy 115.251001 90.00302)
      )
    )
  )
  (zone (net 86) (net_name Board_2-Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.308) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 115.251001 128.50302) (xy 49.501001 128.50302) (xy 49.501001 90.00302) (xy 69.501001 90.00302) (xy 115.251001 90.00302)
      )
    )
  )
  (zone (net 87) (net_name Board_2-Board_1-GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.152))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 56.101001 116.07802) (xy 56.101001 122.87802) (xy 54.076001 122.87802) (xy 51.301001 119.42802) (xy 51.301001 115.55302)
        (xy 55.576001 115.55302) (xy 56.401001 114.72802) (xy 56.951001 115.22802)
      )
    )
  )
  (zone (net 54) (net_name Board_2-Board_1-+3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.318) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 89.686001 94.92302) (xy 89.686001 96.00302) (xy 88.301001 96.00302) (xy 87.666001 96.00302) (xy 87.666001 95.63302)
        (xy 87.666001 94.32302) (xy 89.686001 94.32302)
      )
    )
  )
  (zone (net 87) (net_name Board_2-Board_1-GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.152))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 56.101001 116.07802) (xy 56.101001 122.87802) (xy 54.076001 122.87802) (xy 51.301001 119.42802) (xy 51.301001 115.55302)
        (xy 55.576001 115.55302) (xy 56.401001 114.72802) (xy 56.951001 115.22802)
      )
    )
  )
)
