(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6002)
    (drawings 131)
    (tracks 334)
    (zones 0)
    (modules 36)
    (nets 54)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3175)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 0.762)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 0.9 0.4)
    (user_via 1 0.6)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.254)
    (pcb_text_width 0.254)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.127)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.1524)
    (pad_size 2.5 1.75)
    (pad_drill 1.5)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 0 0)
    (grid_origin 100 77)
    (visible_elements 7FFFBFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-+3V3)
  (net 2 Board_1-+48V)
  (net 3 Board_1-/CAN+)
  (net 4 Board_1-/CAN-)
  (net 5 Board_1-/CAN_RX)
  (net 6 Board_1-/CAN_TX)
  (net 7 Board_1-/LED_D)
  (net 8 Board_1-/MTCK)
  (net 9 Board_1-/MTDI)
  (net 10 Board_1-/MTDO)
  (net 11 Board_1-/MTMS)
  (net 12 Board_1-/OLED_SCL)
  (net 13 Board_1-/OLED_SDA)
  (net 14 Board_1-/QW_SCL)
  (net 15 Board_1-/QW_SDA)
  (net 16 Board_1-/U0RXD)
  (net 17 Board_1-/U0TXD)
  (net 18 Board_1-/U1RX0)
  (net 19 Board_1-/USB_D+)
  (net 20 Board_1-/USB_D-)
  (net 21 Board_1-/USB_ID)
  (net 22 Board_1-/VBUS)
  (net 23 Board_1-/VDD_SPI)
  (net 24 Board_1-/VPP)
  (net 25 Board_1-/xPSRAM_CS)
  (net 26 Board_1-/~BOOT)
  (net 27 Board_1-/~CAN_EN)
  (net 28 Board_1-/~DFU)
  (net 29 Board_1-/~RST)
  (net 30 Board_1-/~SW_L)
  (net 31 Board_1-/~SW_R)
  (net 32 Board_1-/~SW_S)
  (net 33 Board_1-GND)
  (net 34 Board_1-GNDPWR)
  (net 35 "Board_1-Net-(D2-Pad1)")
  (net 36 "Board_1-Net-(D3-Pad1)")
  (net 37 "Board_1-Net-(JP2-Pad1)")
  (net 38 "Board_1-Net-(PS1-Pad4)")
  (net 39 "Board_1-Net-(PS1-Pad6)")
  (net 40 "Board_1-Net-(U1-Pad10)")
  (net 41 "Board_1-Net-(U1-Pad11)")
  (net 42 "Board_1-Net-(U1-Pad12)")
  (net 43 "Board_1-Net-(U1-Pad13)")
  (net 44 "Board_1-Net-(U1-Pad14)")
  (net 45 "Board_1-Net-(U1-Pad15)")
  (net 46 "Board_1-Net-(U1-Pad16)")
  (net 47 "Board_1-Net-(U1-Pad17)")
  (net 48 "Board_1-Net-(U1-Pad24)")
  (net 49 "Board_1-Net-(U1-Pad27)")
  (net 50 "Board_1-Net-(U1-Pad28)")
  (net 51 "Board_1-Net-(U1-Pad6)")
  (net 52 "Board_1-Net-(U1-Pad9)")
  (net 53 "Board_1-Net-(U3-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-+3V3)
    (add_net Board_1-+48V)
    (add_net Board_1-/CAN+)
    (add_net Board_1-/CAN-)
    (add_net Board_1-/CAN_RX)
    (add_net Board_1-/CAN_TX)
    (add_net Board_1-/LED_D)
    (add_net Board_1-/MTCK)
    (add_net Board_1-/MTDI)
    (add_net Board_1-/MTDO)
    (add_net Board_1-/MTMS)
    (add_net Board_1-/OLED_SCL)
    (add_net Board_1-/OLED_SDA)
    (add_net Board_1-/QW_SCL)
    (add_net Board_1-/QW_SDA)
    (add_net Board_1-/U0RXD)
    (add_net Board_1-/U0TXD)
    (add_net Board_1-/U1RX0)
    (add_net Board_1-/USB_D+)
    (add_net Board_1-/USB_D-)
    (add_net Board_1-/USB_ID)
    (add_net Board_1-/VBUS)
    (add_net Board_1-/VDD_SPI)
    (add_net Board_1-/VPP)
    (add_net Board_1-/xPSRAM_CS)
    (add_net Board_1-/~BOOT)
    (add_net Board_1-/~CAN_EN)
    (add_net Board_1-/~DFU)
    (add_net Board_1-/~RST)
    (add_net Board_1-/~SW_L)
    (add_net Board_1-/~SW_R)
    (add_net Board_1-/~SW_S)
    (add_net Board_1-GND)
    (add_net Board_1-GNDPWR)
    (add_net "Board_1-Net-(D2-Pad1)")
    (add_net "Board_1-Net-(D3-Pad1)")
    (add_net "Board_1-Net-(JP2-Pad1)")
    (add_net "Board_1-Net-(PS1-Pad4)")
    (add_net "Board_1-Net-(PS1-Pad6)")
    (add_net "Board_1-Net-(U1-Pad10)")
    (add_net "Board_1-Net-(U1-Pad11)")
    (add_net "Board_1-Net-(U1-Pad12)")
    (add_net "Board_1-Net-(U1-Pad13)")
    (add_net "Board_1-Net-(U1-Pad14)")
    (add_net "Board_1-Net-(U1-Pad15)")
    (add_net "Board_1-Net-(U1-Pad16)")
    (add_net "Board_1-Net-(U1-Pad17)")
    (add_net "Board_1-Net-(U1-Pad24)")
    (add_net "Board_1-Net-(U1-Pad27)")
    (add_net "Board_1-Net-(U1-Pad28)")
    (add_net "Board_1-Net-(U1-Pad6)")
    (add_net "Board_1-Net-(U1-Pad9)")
    (add_net "Board_1-Net-(U3-Pad4)")
  )
  (net_class USB_D ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.1524)
  )
  (net_class VCC ""
    (clearance 0.127)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class VIN ""
    (clearance 0.254)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.127)
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 134.375 116.87 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.945 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0.875 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 1 smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 Board_1-/~RST))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 125.375 116.87 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at -0.005 -0.875 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 Board_1-/~BOOT))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 174.75 109.875)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0 1.375) (layer F.SilkS))
    (fp_text value 10uF (at 0 -1.125) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 Board_1-/~RST))
    (pad 2 smd roundrect (at 0.775 0) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 139.1 85.825 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -1.55 0) (layer F.SilkS))
    (fp_text value 1K (at 0 -0.875) (layer F.Fab))
    (pad 2 smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Board_1-Net-(D2-Pad1)"))
    (pad 1 smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 141.25 90.75 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U2 (at 0 3.3) (layer F.SilkS))
    (fp_text value MAX3051ESA (at 0 -1.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-/CAN_TX))
    (pad 2 smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 3 smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 4 smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Board_1-/CAN_RX))
    (pad 5 smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 Board_1-/~CAN_EN))
    (pad 6 smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Board_1-/CAN-))
    (pad 7 smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Board_1-/CAN+))
    (pad 8 smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:neggle-logo-0.12 (layer B.Cu) (tedit 602F09FF)
    (at 133.425 108.75 180)
    (fp_text reference LOGO1 (at 0 -0.5 180) (layer B.SilkS) hide)
    (fp_text value Logo_Open_Hardware_Small (at 0 0.5 180) (layer B.Fab) hide)
  )
  (module "10-My-Footprints:ESP32-S2-WROVER_and_WROOM(PCB,-I(IPEX))-Universal" (layer F.Cu) (tedit 6034B573)
    (at 167.5 98.49 270)
    (fp_text reference U1 (at -8.5 17 270) (layer F.SilkS))
    (fp_text value ESP32-S2-WROVER (at 0 11.25 90) (layer F.Fab))
    (fp_text user 1 (at -6.75 -8.001 225 unlocked) (layer F.SilkS))
    (fp_text user ANTENNA (at 0.01 -12.5 90) (layer F.SilkS))
    (fp_text user 42 (at 6.75 -8 315 unlocked) (layer F.SilkS))
    (fp_text user "!!! Keepout Area !!!" (at 0.01 -14.5 90) (layer Dwgs.User))
    (fp_text user 26 (at 6.51 13 225 unlocked) (layer F.SilkS))
    (fp_text user o (at -9.779 -8.8646 270) (layer F.SilkS))
    (fp_text user 17 (at -6.49 13 315 unlocked) (layer F.SilkS))
    (fp_text user "!!! Keepout Area !!!" (at 0.01 -10.5 90) (layer Dwgs.User))
    (pad 32 smd rect (at 8.75 7 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-/LED_D))
    (pad 43 thru_hole circle (at -1.94 1.55 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 33 smd rect (at 8.75 5.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 Board_1-/MTCK))
    (pad 29 smd rect (at 8.75 11.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 Board_1-/~SW_L))
    (pad 7 smd rect (at -8.75 1 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 Board_1-/OLED_SDA))
    (pad 17 smd rect (at -6.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 47 "Board_1-Net-(U1-Pad17)"))
    (pad 43 smd rect (at 0.31 0.05 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 28 smd rect (at 8.75 13 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 "Board_1-Net-(U1-Pad28)"))
    (pad 5 smd rect (at -8.75 -2 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 Board_1-/QW_SDA))
    (pad 43 thru_hole circle (at -0.44 1.55 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 8 smd rect (at -8.75 2.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 Board_1-/OLED_SCL))
    (pad 37 smd rect (at 8.75 -0.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-/U0TXD))
    (pad 43 smd rect (at -1.19 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 13 smd rect (at -8.75 10 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Board_1-Net-(U1-Pad13)"))
    (pad 18 smd rect (at -5.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 Board_1-/CAN_TX))
    (pad 27 smd rect (at 8.75 14.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 "Board_1-Net-(U1-Pad27)"))
    (pad 43 smd rect (at -1.19 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 31 smd rect (at 8.75 8.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 Board_1-/~SW_R))
    (pad 6 smd rect (at -8.75 -0.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Board_1-Net-(U1-Pad6)"))
    (pad 22 smd rect (at 0.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 Board_1-/USB_D-))
    (pad 43 thru_hole circle (at -2.69 0.8 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 43 smd rect (at 0.31 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 4 smd rect (at -8.75 -3.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-/QW_SCL))
    (pad 38 smd rect (at 8.75 -2 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 Board_1-/U0RXD))
    (pad 43 smd rect (at 0.31 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 smd rect (at -2.69 0.05 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 21 smd rect (at -0.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 Board_1-/U1RX0))
    (pad 15 smd rect (at -8.75 13 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Board_1-Net-(U1-Pad15)"))
    (pad 10 smd rect (at -8.75 5.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Board_1-Net-(U1-Pad10)"))
    (pad 36 smd rect (at 8.75 1 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 Board_1-/MTMS))
    (pad 12 smd rect (at -8.75 8.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 "Board_1-Net-(U1-Pad12)"))
    (pad 30 smd rect (at 8.75 10 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_1-/~SW_S))
    (pad 43 thru_hole circle (at 0.31 0.8 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 16 smd rect (at -8.75 14.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 "Board_1-Net-(U1-Pad16)"))
    (pad 41 smd rect (at 8.75 -6.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 Board_1-/~RST))
    (pad 43 thru_hole circle (at 0.31 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 9 smd rect (at -8.75 4 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Board_1-Net-(U1-Pad9)"))
    (pad 43 thru_hole circle (at -2.69 -0.7 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 43 thru_hole circle (at -0.44 -1.45 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 23 smd rect (at 2.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 19 Board_1-/USB_D+))
    (pad 43 thru_hole circle (at -1.94 -1.45 270) (size 0.5 0.5) (drill 0.3) (layers *.Cu)
      (net 33 Board_1-GND))
    (pad 19 smd rect (at -3.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 Board_1-/CAN_RX))
    (pad 43 smd rect (at -2.69 1.55 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 43 smd rect (at -2.69 -1.45 270) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 26 smd rect (at 6.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 24 smd rect (at 3.75 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 48 "Board_1-Net-(U1-Pad24)"))
    (pad 20 smd rect (at -2.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 27 Board_1-/~CAN_EN))
    (pad 11 smd rect (at -8.75 7 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Board_1-Net-(U1-Pad11)"))
    (pad 40 smd rect (at 8.75 -5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 Board_1-/~DFU))
    (pad 35 smd rect (at 8.75 2.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 Board_1-/MTDI))
    (pad 14 smd rect (at -8.75 11.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Board_1-Net-(U1-Pad14)"))
    (pad 39 smd rect (at 8.75 -3.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 Board_1-/VDD_SPI))
    (pad 42 smd rect (at 8.75 -8 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 25 smd rect (at 5.25 15.25 270) (size 0.9 1.5) (layers F.Cu F.Paste F.Mask)
      (net 25 Board_1-/xPSRAM_CS))
    (pad 34 smd rect (at 8.75 4 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 Board_1-/MTDO))
    (pad 43 smd rect (at -1.19 0.05 270) (size 4.1 4.1) (layers F.Cu F.Mask)
      (net 33 Board_1-GND))
    (pad 2 smd rect (at -8.75 -6.5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3V3))
    (pad 43 thru_hole rect (at -1.19 0.05 270) (size 1.4 1.4) (drill 1.2) (layers *.Cu *.Mask F.Paste)
      (net 33 Board_1-GND) (solder_paste_margin -0.001))
    (pad 3 smd rect (at -8.75 -5 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 Board_1-/~BOOT))
    (pad 1 smd rect (at -8.75 -8 270) (size 1.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/ESP32-S2-WROVER-I.STEP
      (offset (xyz -9 -15.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:LED_0603_1608Metric_SnapModel (layer F.Cu) (tedit 5FFD7569)
    (at 139.375 84.375)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer F.Fab) hide)
    (fp_text value PWR (at 0 -1.425 180) (layer F.SilkS))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Board_1-Net-(D2-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/LTST-C193TBKT-5A.step
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 120 83.75)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H1 (at 0 -0.55) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.65) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 120 116.25)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H2 (at 0 -0.75) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 180 83.75 180)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H3 (at 0 -0.55) (layer F.Fab) hide)
    (fp_text value MP (at 0 0.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 180 116.25 180)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H4 (at 0 -3.25) (layer F.Fab) hide)
    (fp_text value MP (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
    (pad 1 connect circle (at 0 0 180) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 33 Board_1-GND) (zone_connect 2))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 120.625 89 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP2 (at 0 1.85 270) (layer F.SilkS) hide)
    (fp_text value CAN_T (at 0 -1.9 270) (layer F.SilkS))
    (pad 2 smd custom (at 0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 4 Board_1-/CAN-) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 1 smd custom (at -0.65 0 90) (size 1 0.5) (layers F.Cu F.Mask)
      (net 37 "Board_1-Net-(JP2-Pad1)") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 120.625 91.875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.625 180) (layer F.SilkS))
    (fp_text value 120R (at 0 -1.35) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 3 Board_1-/CAN+))
    (pad 2 smd roundrect (at 1.025 0 180) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 37 "Board_1-Net-(JP2-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 141.82 94.25)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.51 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 1) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 149.625 116.87 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 Board_1-/~SW_L))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 169.625 116.87 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 0.92 0 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 Board_1-/~SW_R))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 173.25 116.25)
    (attr smd)
    (fp_text reference SW5 (at 0 0) (layer F.SilkS))
    (fp_text value RIGHT (at 0 -2) (layer F.Fab) hide)
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 Board_1-/~SW_R))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 Board_1-/~SW_R))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 138 116.25)
    (attr smd)
    (fp_text reference SW1 (at 0 0 180) (layer F.SilkS))
    (fp_text value RST (at 0 -2.375) (layer F.SilkS))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 Board_1-/~RST))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 Board_1-/~RST))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 153.25 116.25)
    (attr smd)
    (fp_text reference SW3 (at 0 0) (layer F.SilkS))
    (fp_text value LEFT (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 Board_1-/~SW_L))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 Board_1-/~SW_L))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 129 116.25)
    (attr smd)
    (fp_text reference SW2 (at 0 0) (layer F.SilkS))
    (fp_text value BOOT (at 0 -2.375) (layer F.SilkS))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 Board_1-/~BOOT))
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 26 Board_1-/~BOOT))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 154.375 85.125 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -2.5 0) (layer F.SilkS))
    (fp_text value XC6220B331MR (at 2.325 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 Board_1-/VBUS))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 Board_1-/VBUS))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 53 "Board_1-Net-(U3-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 151.875 84.73 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.93 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.875 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 Board_1-/VBUS))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 156.875 84.75 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at -0.925 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 -0.875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 159.625 116.87 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 0.925 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 -0.875 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 Board_1-/~SW_S))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:Converter_DCDC_TDK-Lambda_CC3-xxxxxF-E locked (layer F.Cu) (tedit 6045D39C)
    (at 131.25 104.75)
    (fp_text reference PS1 (at -12.5 -1.5 270) (layer F.SilkS))
    (fp_text value CC3-4803SF-E (at 0 6) (layer F.Fab))
    (pad 1 thru_hole circle (at -11.43 -5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 Board_1-+48V))
    (pad 2 thru_hole circle (at -11.43 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 34 Board_1-GNDPWR))
    (pad 3 thru_hole circle (at -11.43 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 34 Board_1-GNDPWR))
    (pad 7 thru_hole circle (at 11.43 -5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 Board_1-+3V3))
    (pad 6 thru_hole circle (at 11.43 -2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Board_1-Net-(PS1-Pad6)"))
    (pad 5 thru_hole circle (at 11.43 2.54) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 33 Board_1-GND))
    (pad 4 thru_hole circle (at 11.43 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Board_1-Net-(PS1-Pad4)"))
    (pad MP thru_hole oval (at -8.89 8) (size 2.5 1.75) (drill oval 1.5 0.75) (layers *.Cu *.Mask)
      (net 34 Board_1-GNDPWR))
    (pad MP2 thru_hole oval (at 8.89 -8) (size 2.5 1.75) (drill oval 1.5 0.75) (layers *.Cu *.Mask)
      (net 33 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/cc3-f-e_outline.STEP
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 10-My-Footprints:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm_3D (layer F.Cu) (tedit 603F44B0)
    (at 180 111 270)
    (descr https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf)
    (tags "LED RGB NeoPixel Mini")
    (attr smd)
    (fp_text reference D3 (at 0 2.625 270) (layer F.SilkS))
    (fp_text value SK6812MINI (at 0 2.625 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.75 0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-/LED_D))
    (pad 4 smd rect (at 1.75 -0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3V3))
    (pad 2 smd rect (at -1.75 0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 1 smd rect (at -1.75 -0.875 270) (size 1 0.85) (layers F.Cu F.Paste F.Mask)
      (net 36 "Board_1-Net-(D3-Pad1)"))
    (model "${KIPRJMOD}/shapes3D/SMD3535 RGB.stp"
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5F68FEEE)
    (at 177.5 87.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 1.25) (layer F.SilkS))
    (fp_text value 22uF (at -1.85 0 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad 2 smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 10-My-Footprints:KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL (layer F.Cu) (tedit 6040DDF0)
    (at 163.25 116.25)
    (attr smd)
    (fp_text reference SW4 (at 0.025 -0.025 180) (layer F.SilkS))
    (fp_text value SEL (at 0 2.05) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_1-/~SW_S))
    (pad 1 smd rect (at 2.2 -1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 32 Board_1-/~SW_S))
    (pad 2 smd rect (at -2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 2 smd rect (at 2.2 1.1) (size 1.2 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/KEY-SMD_4P-L4.2-W3.2-P2.20-LS5.1-TL.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937007874015748 0.3937007874015748 0.3937007874015748))
      (rotate (xyz 0 0 180))
    )
  )
  (module 10-My-Footprints:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal_3D locked (layer F.Cu) (tedit 6045B770)
    (at 172.375 84.55 180)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J3 (at 3 -2.625) (layer F.SilkS))
    (fp_text value Qwiic (at 0 3.98) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-/QW_SCL))
    (pad 2 smd roundrect (at -0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 Board_1-/QW_SDA))
    (pad 3 smd roundrect (at 0.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3V3))
    (pad 4 smd roundrect (at 1.5 -2 180) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 Board_1-GND))
    (pad MP smd roundrect (at -2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208)
      (net 33 Board_1-GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.2))
    (pad MP smd roundrect (at 2.8 1.875 180) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208)
      (net 33 Board_1-GND) (zone_connect 1) (thermal_width 0.254) (thermal_gap 0.2))
    (model ${KIPRJMOD}/shapes3D/SM04B-SRSS-TB.STEP
      (offset (xyz 0 1.325 -0.32))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 10-My-Footprints:OLED_SSD1315_128x64_1.3_I2C_New_Silhouette_Big3D locked (layer F.Cu) (tedit 603CB3FF)
    (at 163.195 97.625)
    (fp_text reference I2C1 (at 0 -0.75) (layer F.Fab))
    (fp_text value OLED (at 0 0.75) (layer F.Fab))
    (fp_text user "Visible Area" (at 0 -1.75) (layer Cmts.User))
    (fp_text user "GND VCC SCL SDA" (at 0 -12.75) (layer Cmts.User))
    (fp_text user "VCC/GND switchable via 0R jumpers on rear" (at 0 -11.25) (layer Cmts.User))
    (pad 2 thru_hole oval (at -1.26 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 Board_1-+3V3))
    (pad 4 thru_hole oval (at 3.82 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 Board_1-/OLED_SDA))
    (pad 1 thru_hole rect (at -3.8 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 Board_1-GND))
    (pad 3 thru_hole oval (at 1.28 -14.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 Board_1-/OLED_SCL))
    (model "${KIPRJMOD}/shapes3D/Oled SH1106.wrl"
      (offset (xyz 0 0.3 8.800000000000001))
      (scale (xyz 0.36 0.36 0.36))
      (rotate (xyz 0 0 180))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 146.25 100.125 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.65 90) (layer F.Fab))
    (fp_text value VPP_EN (at 0.025 -1.85 90) (layer F.SilkS))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 1 Board_1-+3V3) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 24 Board_1-/VPP) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module 11-My-Edits:Gecko-G125_PlusTC2030_IDCBox_2x03_P1.25mm_Vertical_3D (layer F.Cu) (tedit 6045B3A6)
    (at 147.615 107.88 90)
    (descr "Harwin Gecko Connector, 6 pins, dual row male, vertical entry, no latches, PN:G125-MVX0605L0X")
    (tags "connector harwin gecko")
    (fp_text reference J2 (at -2.75 3.375 90) (layer F.SilkS))
    (fp_text value ESP-PROG (at 0 -3.675 90) (layer F.Fab))
    (fp_text user KEEPOUT (at 0 0.025 90) (layer Cmts.User))
    (pad "" np_thru_hole circle (at 2.54 1.016 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 -1.016 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.54 0 90) (size 0.9906 0.9906) (drill 0.9906) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at -1.27 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 Board_1-/VPP))
    (pad 6 thru_hole oval (at 1.27 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 Board_1-/~BOOT))
    (pad 5 thru_hole oval (at 1.27 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 Board_1-/U0RXD))
    (pad 4 thru_hole oval (at 0 -0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 Board_1-GND))
    (pad 1 thru_hole rect (at -1.27 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 Board_1-/~RST))
    (pad 3 thru_hole oval (at 0 0.635 180) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 17 Board_1-/U0TXD))
    (model ${KIPRJMOD}/shapes3D/g125-mv10605l0_asm.stp
      (offset (xyz 0 0 1.925))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module NetTie:NetTie-2_SMD_Pad0.5mm (layer F.Cu) (tedit 6045BC89)
    (at 134.65 94.25)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 1.95 0 90) (layer F.Fab) hide)
    (fp_text value GND_TIE (at 0 1.2) (layer F.Fab))
    (pad 1 smd circle (at -0.5 0) (size 0.5 0.5) (layers F.Cu)
      (net 34 Board_1-GNDPWR))
    (pad 2 smd circle (at 0.5 0) (size 0.5 0.5) (layers F.Cu)
      (net 33 Board_1-GND) (clearance 0.001) (zone_connect 2))
  )
  (module 11-My-Edits:Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_Horizontal_3D (layer F.Cu) (tedit 6045D355)
    (at 130 94.25)
    (descr "Molex Nano-Fit Power Connectors, 105313-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053131208_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit top entry")
    (fp_text reference J1 (at -6.875 0 180) (layer F.SilkS))
    (fp_text value CANBUS (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 4.77 -6.15 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at -3.75 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 2 Board_1-+48V))
    (pad 2 thru_hole oval (at -1.25 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 Board_1-/CAN+))
    (pad 3 thru_hole oval (at 1.25 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 Board_1-/CAN-))
    (pad 4 thru_hole oval (at 3.75 0 90) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 Board_1-GNDPWR))
    (pad "" np_thru_hole circle (at -3.75 -7.18 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 3.75 -7.18 90) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_PTH_Clips_Horz.step
      (offset (xyz 0 6.15 2.05))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module 41-EasyEDA-Edits:MICRO-USB-SMD_U254-051T-4BH83-F1S_C397452 (layer F.Cu) (tedit 6045F2E8)
    (at 146.25 83.25 180)
    (attr smd)
    (fp_text reference USB1 (at 0 -3) (layer F.SilkS))
    (fp_text value USB (at 0 5.252001) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.375) (layer Dwgs.User))
    (pad "" np_thru_hole circle (at -2 -2.025 180) (size 0.45 0.45) (drill 0.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2 -2.025 180) (size 0.5 0.5) (drill 0.45) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2.83 0.325 180) (size 1.5 2) (drill oval 0.9 1.4) (layers *.Cu *.Paste *.Mask)
      (net 33 Board_1-GND))
    (pad 6 thru_hole oval (at -2.83 0.325) (size 1.5 2) (drill oval 0.9 1.4) (layers *.Cu *.Paste *.Mask)
      (net 33 Board_1-GND))
    (pad 6 smd rect (at -3.1 -2.225 270) (size 1.6 2.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 6 smd rect (at 3.1 -2.225 270) (size 1.6 2.1) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 5 smd rect (at 1.3 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 33 Board_1-GND))
    (pad 4 smd rect (at 0.65 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 21 Board_1-/USB_ID))
    (pad 3 smd rect (at 0 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 19 Board_1-/USB_D+))
    (pad 2 smd rect (at -0.65 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 20 Board_1-/USB_D-))
    (pad 1 smd rect (at -1.3 -2.325 180) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 22 Board_1-/VBUS))
    (model ${EASY_EDA_3D}/EasyEDA.3dshapes/MICRO-USB-SMD_U254-051T-4BH83-F1S.wrl
      (offset (xyz 0 0 1.25))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 182.501 108.75) (end 182.501 116.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4969 108.6714) (end 182.501 108.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4846 108.5938) (end 182.4969 108.6714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4642 108.5179) (end 182.4846 108.5938) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4361 108.4446) (end 182.4642 108.5179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4004 108.3745) (end 182.4361 108.4446) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3576 108.3086) (end 182.4004 108.3745) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3081 108.2475) (end 182.3576 108.3086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.2525 108.1919) (end 182.3081 108.2475) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.1914 108.1424) (end 182.2525 108.1919) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.1255 108.0996) (end 182.1914 108.1424) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.0554 108.0639) (end 182.1255 108.0996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.9821 108.0358) (end 182.0554 108.0639) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.9062 108.0154) (end 181.9821 108.0358) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.8286 108.0031) (end 181.9062 108.0154) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.75 107.999) (end 181.8286 108.0031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.75 107.999) (end 181.75 107.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.6194 107.9922) (end 178.75 107.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.4903 107.9717) (end 178.6194 107.9922) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.364 107.9379) (end 178.4903 107.9717) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.242 107.891) (end 178.364 107.9379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.1255 107.8317) (end 178.242 107.891) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.0159 107.7605) (end 178.1255 107.8317) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.9143 107.6782) (end 178.0159 107.7605) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.8218 107.5857) (end 177.9143 107.6782) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.7395 107.4841) (end 177.8218 107.5857) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.6683 107.3745) (end 177.7395 107.4841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.609 107.258) (end 177.6683 107.3745) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.5621 107.136) (end 177.609 107.258) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.5283 107.0097) (end 177.5621 107.136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.5078 106.8806) (end 177.5283 107.0097) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.501 106.75) (end 177.5078 106.8806) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.501 90.25) (end 177.501 106.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.5078 90.1194) (end 177.501 90.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.5283 89.9903) (end 177.5078 90.1194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.5621 89.864) (end 177.5283 89.9903) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.609 89.742) (end 177.5621 89.864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.6683 89.6255) (end 177.609 89.742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.7395 89.5159) (end 177.6683 89.6255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.8218 89.4143) (end 177.7395 89.5159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 177.9143 89.3218) (end 177.8218 89.4143) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.0159 89.2395) (end 177.9143 89.3218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.1255 89.1683) (end 178.0159 89.2395) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.242 89.109) (end 178.1255 89.1683) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.364 89.0621) (end 178.242 89.109) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.4903 89.0283) (end 178.364 89.0621) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.6194 89.0078) (end 178.4903 89.0283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 178.75 89.001) (end 178.6194 89.0078) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.75 89.001) (end 178.75 89.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.8286 88.9969) (end 181.75 89.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.9062 88.9846) (end 181.8286 88.9969) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.982 88.9643) (end 181.9062 88.9846) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.0554 88.9361) (end 181.982 88.9643) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.1255 88.9004) (end 182.0554 88.9361) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.1915 88.8575) (end 182.1255 88.9004) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.2525 88.8081) (end 182.1915 88.8575) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3081 88.7526) (end 182.2525 88.8081) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3575 88.6915) (end 182.3081 88.7526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4004 88.6255) (end 182.3575 88.6915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4361 88.5554) (end 182.4004 88.6255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4643 88.482) (end 182.4361 88.5554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4846 88.4061) (end 182.4643 88.482) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4969 88.3284) (end 182.4846 88.4061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.501 88.25) (end 182.4969 88.3284) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.501 83.75) (end 182.501 88.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4873 83.4886) (end 182.501 83.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4464 83.2301) (end 182.4873 83.4886) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3786 82.9772) (end 182.4464 83.2301) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.2848 82.7328) (end 182.3786 82.9772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.166 82.4995) (end 182.2848 82.7328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.0234 82.28) (end 182.166 82.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.8586 82.0765) (end 182.0234 82.28) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.6735 81.8914) (end 181.8586 82.0765) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.47 81.7266) (end 181.6735 81.8914) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.2505 81.584) (end 181.47 81.7266) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.0172 81.4652) (end 181.2505 81.584) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.7728 81.3714) (end 181.0172 81.4652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.52 81.3037) (end 180.7728 81.3714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.2615 81.2627) (end 180.52 81.3037) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180 81.249) (end 180.2615 81.2627) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120 81.249) (end 180 81.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.7385 81.2627) (end 120 81.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.48 81.3037) (end 119.7385 81.2627) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.2272 81.3714) (end 119.48 81.3037) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.9828 81.4652) (end 119.2272 81.3714) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.7495 81.5841) (end 118.9828 81.4652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.5299 81.7267) (end 118.7495 81.5841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.3265 81.8914) (end 118.5299 81.7267) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.1414 82.0765) (end 118.3265 81.8914) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.9767 82.2799) (end 118.1414 82.0765) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.834 82.4995) (end 117.9767 82.2799) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.7152 82.7328) (end 117.834 82.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.6214 82.9772) (end 117.7152 82.7328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5537 83.23) (end 117.6214 82.9772) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5127 83.4885) (end 117.5537 83.23) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.499 83.75) (end 117.5127 83.4885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.499 116.25) (end 117.499 83.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5127 116.5115) (end 117.499 116.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5537 116.77) (end 117.5127 116.5115) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.6214 117.0228) (end 117.5537 116.77) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.7152 117.2672) (end 117.6214 117.0228) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.8341 117.5005) (end 117.7152 117.2672) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.9767 117.7201) (end 117.8341 117.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.1414 117.9235) (end 117.9767 117.7201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.3265 118.1086) (end 118.1414 117.9235) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.5299 118.2733) (end 118.3265 118.1086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.7495 118.416) (end 118.5299 118.2733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.9828 118.5348) (end 118.7495 118.416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.2272 118.6286) (end 118.9828 118.5348) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.48 118.6963) (end 119.2272 118.6286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.7385 118.7373) (end 119.48 118.6963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120 118.751) (end 119.7385 118.7373) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.0001 118.751) (end 120 118.751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.2615 118.7373) (end 180.0001 118.751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.52 118.6963) (end 180.2615 118.7373) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.7728 118.6286) (end 180.52 118.6963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.0172 118.5348) (end 180.7728 118.6286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.2505 118.416) (end 181.0172 118.5348) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.47 118.2734) (end 181.2505 118.416) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.6735 118.1086) (end 181.47 118.2734) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 181.8586 117.9235) (end 181.6735 118.1086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.0233 117.7201) (end 181.8586 117.9235) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.1659 117.5005) (end 182.0233 117.7201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.2848 117.2672) (end 182.1659 117.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3786 117.0228) (end 182.2848 117.2672) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4464 116.7699) (end 182.3786 117.0228) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.4873 116.5114) (end 182.4464 116.7699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.501 116.25) (end 182.4873 116.5114) (layer Edge.Cuts) (width 0.1))
  (zone (net 33) (net_name Board_1-GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.308) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 182.75 119.25) (xy 117 119.25) (xy 117 80.75) (xy 137 80.75) (xy 182.75 80.75)
      )
    )
  )
  (zone (net 33) (net_name Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.308) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 182.75 119.25) (xy 117 119.25) (xy 117 80.75) (xy 137 80.75) (xy 182.75 80.75)
      )
    )
  )
  (zone (net 34) (net_name Board_1-GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.152))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 123.6 106.825) (xy 123.6 113.625) (xy 121.575 113.625) (xy 118.8 110.175) (xy 118.8 106.3)
        (xy 123.075 106.3) (xy 123.9 105.475) (xy 124.45 105.975)
      )
    )
  )
  (zone (net 1) (net_name Board_1-+3V3) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.1524) (thermal_bridge_width 0.318) (smoothing fillet) (radius 0.25))
    (polygon
      (pts
        (xy 157.185 85.67) (xy 157.185 86.75) (xy 155.8 86.75) (xy 155.165 86.75) (xy 155.165 86.38)
        (xy 155.165 85.07) (xy 157.185 85.07)
      )
    )
  )
  (zone (net 34) (net_name Board_1-GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.152))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 123.6 106.825) (xy 123.6 113.625) (xy 121.575 113.625) (xy 118.8 110.175) (xy 118.8 106.3)
        (xy 123.075 106.3) (xy 123.9 105.475) (xy 124.45 105.975)
      )
    )
  )
)
