(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 862)
    (tracks 284)
    (zones 0)
    (modules 179)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 0.9 0.4)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 0.8128 0.8128)
    (mod_text_width 0.1524)
    (pad_size 2.2 1.7)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-/CAN+)
  (net 2 Board_1-/CAN-)
  (net 3 Board_1-/VBUS+)
  (net 4 Board_1-/VBUS-)
  (net 5 Board_1-/VCCD)
  (net 6 Board_1-Earth)
  (net 7 Board_1-GNDD)
  (net 8 Board_1-LINE)
  (net 9 Board_1-NEUT)
  (net 10 Board_2-/CAN+)
  (net 11 Board_2-/CAN-)
  (net 12 Board_2-/VBUS+)
  (net 13 Board_2-/VBUS-)
  (net 14 Board_2-/VCCD)
  (net 15 Board_2-Earth)
  (net 16 Board_2-GNDD)
  (net 17 Board_2-LINE)
  (net 18 Board_2-NEUT)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-/CAN+)
    (add_net Board_1-/CAN-)
    (add_net Board_1-/VBUS+)
    (add_net Board_1-/VBUS-)
    (add_net Board_1-/VCCD)
    (add_net Board_1-Earth)
    (add_net Board_1-GNDD)
    (add_net Board_1-LINE)
    (add_net Board_1-NEUT)
    (add_net Board_2-/CAN+)
    (add_net Board_2-/CAN-)
    (add_net Board_2-/VBUS+)
    (add_net Board_2-/VBUS-)
    (add_net Board_2-/VCCD)
    (add_net Board_2-Earth)
    (add_net Board_2-GNDD)
    (add_net Board_2-LINE)
    (add_net Board_2-NEUT)
  )
  (net_class CANBUS ""
    (clearance 0.154)
    (trace_width 0.154)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class PWR_AC ""
    (clearance 1)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class PWR_DC ""
    (clearance 0.5)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class PWR_IO ""
    (clearance 0.154)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 73.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 74.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 75.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 76.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 77.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 78.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 79.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 80.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 81.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 82.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.500001 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 88.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 87.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 86.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 85.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 84.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 83.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 82.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 81.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 80.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 79.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 78.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 77.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 76.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 75.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 74.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 73.500001 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 122.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 123.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 124.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 125.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 126.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 127.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 128.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 129.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 130.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 131.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 132.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 133.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 134.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 135.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 136.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 137.250009 49.749)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 137.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 136.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 135.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 134.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 133.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 132.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 131.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 130.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 129.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 128.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 127.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 126.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 125.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 124.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 123.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 122.250009 131.251)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499002 108.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499002 107.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499002 106.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499003 105.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499003 104.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499003 103.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499003 102.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499003 101.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499003 100.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499004 99.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499004 98.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499004 97.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499004 96.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499004 95.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499004 94.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499005 93.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499005 92.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499005 91.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499005 90.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499005 89.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499005 88.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499006 87.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499006 86.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499006 85.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499006 84.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499006 83.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499006 82.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499007 81.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499007 80.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499007 79.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499007 78.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499007 77.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499007 76.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499008 75.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499008 74.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 98.499008 73.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 73.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 74.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 75.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 76.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 77.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 78.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 79.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 80.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 81.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 82.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 83.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 84.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 85.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 86.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 87.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 88.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 89.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 90.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 91.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 92.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 93.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 94.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 95.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 96.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 97.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 98.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 99.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 100.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 101.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 102.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 103.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 104.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 105.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 106.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 107.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 94.001 108.000004)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 54.999 136.250001)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 137.501009 45.000001)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu))
  )
  (module NPTH (layer F.Cu) (tedit 5FA56C77)
    (at 54.999 45.000001)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value NPTH (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu))
  )
  (module Fiducial (layer B.Cu) (tedit 5EA93A7C)
    (at 59.999 136.250001)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value Fiducial (at 0 -1.5) (layer B.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer F.Cu) (tedit 5EA93A7C)
    (at 59.999 136.250001)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 1.5) (layer F.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer B.Cu) (tedit 5EA93A7C)
    (at 132.501009 45.000001)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value Fiducial (at 0 -1.5) (layer B.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer F.Cu) (tedit 5EA93A7C)
    (at 132.501009 45.000001)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 1.5) (layer F.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer B.Cu) (tedit 5EA93A7C)
    (at 59.999 45.000001)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 1.5) (layer B.SilkS) hide)
    (fp_text value Fiducial (at 0 -1.5) (layer B.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers B.Cu B.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Fiducial (layer F.Cu) (tedit 5EA93A7C)
    (at 59.999 45.000001)
    (descr "Circular Fiducial")
    (tags fiducial)
    (attr smd)
    (fp_text reference REF** (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value Fiducial (at 0 1.5) (layer F.Fab) hide)
    (pad "" smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.5) (clearance 0.5))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 115.250009 88.500001 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.55 90) (layer F.SilkS))
    (fp_text value 120R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 11 Board_2-/CAN-))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 10 Board_2-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B784ED0)
    (at 134.250009 94.250001 90)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/3-G-3.5; number of pins: 03; pin pitch: 3.50mm; Angled || order number: 1844223 8A 160V")
    (tags "phoenix_contact connector MC_01x03_G_3.5mm")
    (fp_text reference JB2 (at 3.5 3.4 270) (layer F.SilkS))
    (fp_text value CANBUS (at 3.5 9.2 90) (layer F.Fab))
    (fp_text user %R (at 3.5 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 16 Board_2-GNDD))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 Board_2-/CAN-))
    (pad 3 thru_hole oval (at 7 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 Board_2-/CAN+))
    (model ${KIPRJMOD}/shapes3D/PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 121.250009 82.975001 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.6 90) (layer F.SilkS))
    (fp_text value CTRL_VBUS+ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 12 Board_2-/VBUS+) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 14 Board_2-/VCCD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 120.000009 128.250001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 15 Board_2-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 120.000009 52.750001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 15 Board_2-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 139.750009 52.750001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 15 Board_2-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 139.750009 128.250001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 15 Board_2-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 15 Board_2-Earth))
  )
  (module "1 My Footprints:TerminalBlock_WAGO_236-103_1x03_P5.00mm_PadsOnly" (layer F.Cu) (tedit 601D1331)
    (at 130.000009 119.500001 90)
    (descr "Terminal Block WAGO 236-103, 45Degree (cable under 45degree), 3 pins, pitch 5mm, size 17.3x14mm^2, drill diamater 1.15mm, pad diameter 3mm, see , script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_WAGO")
    (tags "THT Terminal Block WAGO 236-103 45Degree pitch 5mm size 17.3x14mm^2 drill 1.15mm pad 3mm")
    (fp_text reference JB1 (at 5 2.65 90) (layer F.SilkS))
    (fp_text value AC_IN (at 5.15 10.12 90) (layer F.Fab))
    (fp_text user %R (at 5.15 1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 17 Board_2-LINE))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 3 thru_hole oval (at 10 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 18 Board_2-NEUT))
    (model ${KIPRJMOD}/shapes3D/TerminalBlock_WAGO_236-103_1x03_P5.00mm_45Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:1605540000" (layer F.Cu) (tedit 602379B0)
    (at 125.000009 119.580001 90)
    (fp_text reference JA1 (at 5.08 -4.75 90) (layer F.SilkS))
    (fp_text value AC_IN (at 5.05 4.85 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 17 Board_2-LINE))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 Board_2-NEUT))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (model ${KIPRJMOD}/shapes3D/1605540000.stp
      (offset (xyz -3.54 -9.5 -3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EltekFlatpack2:Amass_XT60PW-M_Kombifootprint (layer F.Cu) (tedit 60237AFA)
    (at 131.800009 69.000001 270)
    (fp_text reference JC3 (at 0 0.75 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 1 90) (layer F.Fab) hide)
    (pad 2 thru_hole custom (at 3.6 0 270) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.949 0.127) (xy -2.10902 -3.1877) (xy -1.5045 -4.064) (xy -0.552 -4.064) (xy -0.19894 -3.75158)
           (xy 1.44698 -1.30556)) (width 0.1))
        (gr_poly (pts
           (xy -2.11664 -3.175) (xy -2.11664 -7.4295) (xy -0.2345 -7.4295) (xy -0.2345 -3.175)) (width 0.1))
      ))
    (pad 1 thru_hole custom (at -3.6 0 270) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.861 0) (xy 1.949 0) (xy 2.10394 -3.14706) (xy 1.695 -3.937) (xy 1.441 -4.064)
           (xy 0.1075 -3.6195) (xy -1.734 -0.889)) (width 0.1))
        (gr_poly (pts
           (xy 0.21786 -3.175) (xy 0.21786 -7.4295) (xy 2.1 -7.4295) (xy 2.1 -3.175)) (width 0.1))
      ))
    (pad 2 thru_hole circle (at 2.54 -3.175 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.54 -3.175 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-) (zone_connect 2))
    (pad MP thru_hole oval (at -6.75 -6 270) (size 1.6 2.8) (drill oval 0.8 1.8) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad MP thru_hole oval (at 6.75 -6 270) (size 1.6 2.8) (drill oval 0.8 1.8) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
  )
  (module "1 My Footprints:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Combi_3D-V" (layer F.Cu) (tedit 6023867E)
    (at 121.250009 87.000001)
    (descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference JA2 (at -3 3.75 90) (layer F.SilkS))
    (fp_text value CTRL (at 0 10.42) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 14 Board_2-/VCCD))
    (pad 2 thru_hole oval (at 0 2.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 Board_2-/CAN+))
    (pad 3 thru_hole oval (at 0 5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 Board_2-/CAN-))
    (pad 4 thru_hole oval (at 0 7.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 Board_2-GNDD))
    (pad "" np_thru_hole circle (at -1.34 3.75) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.18 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.18 7.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.step
      (offset (xyz 0 -3.75 4.85))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_Horizontal.step
      (offset (xyz 6.15 -3.75 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module EltekFlatpack2:CON_Edge_Flatpack2_AllContacts locked (layer F.Cu) (tedit 6023AC13)
    (at 98.750009 56.250001)
    (fp_text reference PC1 (at 6 13.75) (layer F.SilkS) hide)
    (fp_text value Flatpack2 (at 6 14.75) (layer F.Fab))
    (fp_text user H (at 12.675 31 90 unlocked) (layer F.SilkS))
    (fp_text user L (at 12.675 33.5 90 unlocked) (layer F.SilkS))
    (pad DC-POS smd roundrect (at 11.5 20) (size 5 8.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 12 Board_2-/VBUS+) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 11.5 5.5) (size 5 8.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 13 Board_2-/VBUS-) (solder_mask_margin 0.1016))
    (pad DC-POS smd roundrect (at 5.05 20) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 12 Board_2-/VBUS+) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 5.05 5.5) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 13 Board_2-/VBUS-) (solder_mask_margin 0.1016))
    (pad AC-N smd roundrect (at 5.05 49) (size 9.9 8) (layers B.Cu B.Mask) (roundrect_rratio 0.062)
      (net 18 Board_2-NEUT) (solder_mask_margin 0.1016))
    (pad AC-L smd roundrect (at 5.05 63.5) (size 9.9 8) (layers B.Cu B.Mask) (roundrect_rratio 0.062)
      (net 17 Board_2-LINE) (solder_mask_margin 0.1016))
    (pad AC-N smd roundrect (at 5.05 49) (size 9.9 8) (layers F.Cu F.Mask) (roundrect_rratio 0.062)
      (net 18 Board_2-NEUT) (solder_mask_margin 0.1016))
    (pad AC-L smd roundrect (at 5.05 63.5) (size 9.9 8) (layers F.Cu F.Mask) (roundrect_rratio 0.062)
      (net 17 Board_2-LINE) (solder_mask_margin 0.1016))
    (pad GNDD smd roundrect (at 5.05 36) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 16 Board_2-GNDD) (solder_mask_margin 0.1016))
    (pad DC-POS smd roundrect (at 7.05 20) (size 13.9 8.5) (layers F.Cu F.Mask) (roundrect_rratio 0.059)
      (net 12 Board_2-/VBUS+) (solder_mask_margin 0.1016))
    (pad AC-E smd roundrect (at 5.05 34.5) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 15 Board_2-Earth) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 7.05 5.5) (size 13.9 8.5) (layers F.Cu F.Mask) (roundrect_rratio 0.059)
      (net 13 Board_2-/VBUS-) (solder_mask_margin 0.1016))
    (pad CAN-H smd roundrect (at 5.05 31) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 10 Board_2-/CAN+) (solder_mask_margin 0.1016))
    (pad CAN-L smd roundrect (at 5.05 33.5) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 11 Board_2-/CAN-) (solder_mask_margin 0.1016))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 115.250009 91.050001 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.92 90) (layer F.SilkS) hide)
    (fp_text value 120R (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 Board_2-/CAN-))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 Board_2-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:Connector_Keystone_4912_Overlaid" locked (layer F.Cu) (tedit 603C8B9E)
    (at 124.200009 77.240001 90)
    (fp_text reference T1 (at -3.175 -2.54 270) (layer F.Fab))
    (fp_text value "Keystone 4912" (at 0 5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
    (pad 1 thru_hole circle (at -2.54 2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
  )
  (module "1 My Footprints:Connector_Keystone_4912_Overlaid" locked (layer F.Cu) (tedit 603C8BCB)
    (at 124.200009 60.750001 90)
    (fp_text reference T2 (at -3.175 -2.54 270) (layer F.Fab))
    (fp_text value "Keystone 4912" (at 0 5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (pad 1 thru_hole circle (at 2.54 2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
  )
  (module SnapEDA-zip:TE_2204535-1 locked (layer F.Cu) (tedit 603C8BDE)
    (at 131.050009 69.000001 90)
    (fp_text reference JB3 (at 3.325 -3.15 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.7 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
    (pad 4 thru_hole circle (at -5.7 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
    (pad 2 thru_hole circle (at 0 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 5 thru_hole circle (at 0 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 3 thru_hole circle (at 5.7 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (pad 6 thru_hole circle (at 5.7 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (pad "" np_thru_hole circle (at -7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -5.7 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
    (pad 2 thru_hole circle (at 0 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 3 thru_hole circle (at 5.7 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (pad 4 thru_hole circle (at -5.7 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
    (pad 5 thru_hole circle (at 0 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 6 thru_hole circle (at 5.7 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (model ${KIPRJMOD}/shapes3D/TE_2204535-1.stp
      (offset (xyz 0 -9.949999999999999 10.7))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:TE_2204529-1" (layer F.Cu) (tedit 603C8C5D)
    (at 125.000009 69.000001 270)
    (fp_text reference JA3 (at -3.4 3.15 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 -0.45 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 5.7 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
    (pad 3 thru_hole circle (at -5.7 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (pad 2 thru_hole circle (at 0 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad 2 thru_hole circle (at 0 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 15 Board_2-Earth))
    (pad "" np_thru_hole circle (at -7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.7 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 13 Board_2-/VBUS-))
    (pad 1 thru_hole circle (at 5.7 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 12 Board_2-/VBUS+))
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 66.500001 88.500001 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.55 90) (layer F.SilkS))
    (fp_text value 120R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 Board_1-/CAN-))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B784ED0)
    (at 85.500001 94.250001 90)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/3-G-3.5; number of pins: 03; pin pitch: 3.50mm; Angled || order number: 1844223 8A 160V")
    (tags "phoenix_contact connector MC_01x03_G_3.5mm")
    (fp_text reference JB2 (at 3.5 3.4 270) (layer F.SilkS))
    (fp_text value CANBUS (at 3.5 9.2 90) (layer F.Fab))
    (fp_text user %R (at 3.5 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 7 Board_1-GNDD))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Board_1-/CAN-))
    (pad 3 thru_hole oval (at 7 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 72.500001 82.975001 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.6 90) (layer F.SilkS))
    (fp_text value CTRL_VBUS+ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 3 Board_1-/VBUS+) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 Board_1-/VCCD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 71.250001 128.250001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 71.250001 52.750001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 91.000001 52.750001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 91.000001 128.250001)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module "1 My Footprints:TerminalBlock_WAGO_236-103_1x03_P5.00mm_PadsOnly" (layer F.Cu) (tedit 601D1331)
    (at 81.250001 119.500001 90)
    (descr "Terminal Block WAGO 236-103, 45Degree (cable under 45degree), 3 pins, pitch 5mm, size 17.3x14mm^2, drill diamater 1.15mm, pad diameter 3mm, see , script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_WAGO")
    (tags "THT Terminal Block WAGO 236-103 45Degree pitch 5mm size 17.3x14mm^2 drill 1.15mm pad 3mm")
    (fp_text reference JB1 (at 5 2.65 90) (layer F.SilkS))
    (fp_text value AC_IN (at 5.15 10.12 90) (layer F.Fab))
    (fp_text user %R (at 5.15 1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 8 Board_1-LINE))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 3 thru_hole oval (at 10 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 9 Board_1-NEUT))
    (model ${KIPRJMOD}/shapes3D/TerminalBlock_WAGO_236-103_1x03_P5.00mm_45Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:1605540000" (layer F.Cu) (tedit 602379B0)
    (at 76.250001 119.580001 90)
    (fp_text reference JA1 (at 5.08 -4.75 90) (layer F.SilkS))
    (fp_text value AC_IN (at 5.05 4.85 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 8 Board_1-LINE))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 Board_1-NEUT))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (model ${KIPRJMOD}/shapes3D/1605540000.stp
      (offset (xyz -3.54 -9.5 -3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EltekFlatpack2:Amass_XT60PW-M_Kombifootprint (layer F.Cu) (tedit 60237AFA)
    (at 83.050001 69.000001 270)
    (fp_text reference JC3 (at 0 0.75 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 1 90) (layer F.Fab) hide)
    (pad 2 thru_hole custom (at 3.6 0 270) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.949 0.127) (xy -2.10902 -3.1877) (xy -1.5045 -4.064) (xy -0.552 -4.064) (xy -0.19894 -3.75158)
           (xy 1.44698 -1.30556)) (width 0.1))
        (gr_poly (pts
           (xy -2.11664 -3.175) (xy -2.11664 -7.4295) (xy -0.2345 -7.4295) (xy -0.2345 -3.175)) (width 0.1))
      ))
    (pad 1 thru_hole custom (at -3.6 0 270) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.861 0) (xy 1.949 0) (xy 2.10394 -3.14706) (xy 1.695 -3.937) (xy 1.441 -4.064)
           (xy 0.1075 -3.6195) (xy -1.734 -0.889)) (width 0.1))
        (gr_poly (pts
           (xy 0.21786 -3.175) (xy 0.21786 -7.4295) (xy 2.1 -7.4295) (xy 2.1 -3.175)) (width 0.1))
      ))
    (pad 2 thru_hole circle (at 2.54 -3.175 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.54 -3.175 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-) (zone_connect 2))
    (pad MP thru_hole oval (at -6.75 -6 270) (size 1.6 2.8) (drill oval 0.8 1.8) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad MP thru_hole oval (at 6.75 -6 270) (size 1.6 2.8) (drill oval 0.8 1.8) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
  )
  (module "1 My Footprints:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Combi_3D-V" (layer F.Cu) (tedit 6023867E)
    (at 72.500001 87.000001)
    (descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference JA2 (at -3 3.75 90) (layer F.SilkS))
    (fp_text value CTRL (at 0 10.42) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 5 Board_1-/VCCD))
    (pad 2 thru_hole oval (at 0 2.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 Board_1-/CAN+))
    (pad 3 thru_hole oval (at 0 5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Board_1-/CAN-))
    (pad 4 thru_hole oval (at 0 7.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 Board_1-GNDD))
    (pad "" np_thru_hole circle (at -1.34 3.75) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.18 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.18 7.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.step
      (offset (xyz 0 -3.75 4.85))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_Horizontal.step
      (offset (xyz 6.15 -3.75 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module EltekFlatpack2:CON_Edge_Flatpack2_AllContacts locked (layer F.Cu) (tedit 6023AC13)
    (at 50.000001 56.250001)
    (fp_text reference PC1 (at 6 13.75) (layer F.SilkS) hide)
    (fp_text value Flatpack2 (at 6 14.75) (layer F.Fab))
    (fp_text user H (at 12.675 31 90 unlocked) (layer F.SilkS))
    (fp_text user L (at 12.675 33.5 90 unlocked) (layer F.SilkS))
    (pad DC-POS smd roundrect (at 11.5 20) (size 5 8.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 3 Board_1-/VBUS+) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 11.5 5.5) (size 5 8.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 4 Board_1-/VBUS-) (solder_mask_margin 0.1016))
    (pad DC-POS smd roundrect (at 5.05 20) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 3 Board_1-/VBUS+) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 5.05 5.5) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 4 Board_1-/VBUS-) (solder_mask_margin 0.1016))
    (pad AC-N smd roundrect (at 5.05 49) (size 9.9 8) (layers B.Cu B.Mask) (roundrect_rratio 0.062)
      (net 9 Board_1-NEUT) (solder_mask_margin 0.1016))
    (pad AC-L smd roundrect (at 5.05 63.5) (size 9.9 8) (layers B.Cu B.Mask) (roundrect_rratio 0.062)
      (net 8 Board_1-LINE) (solder_mask_margin 0.1016))
    (pad AC-N smd roundrect (at 5.05 49) (size 9.9 8) (layers F.Cu F.Mask) (roundrect_rratio 0.062)
      (net 9 Board_1-NEUT) (solder_mask_margin 0.1016))
    (pad AC-L smd roundrect (at 5.05 63.5) (size 9.9 8) (layers F.Cu F.Mask) (roundrect_rratio 0.062)
      (net 8 Board_1-LINE) (solder_mask_margin 0.1016))
    (pad GNDD smd roundrect (at 5.05 36) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 7 Board_1-GNDD) (solder_mask_margin 0.1016))
    (pad DC-POS smd roundrect (at 7.05 20) (size 13.9 8.5) (layers F.Cu F.Mask) (roundrect_rratio 0.059)
      (net 3 Board_1-/VBUS+) (solder_mask_margin 0.1016))
    (pad AC-E smd roundrect (at 5.05 34.5) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 6 Board_1-Earth) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 7.05 5.5) (size 13.9 8.5) (layers F.Cu F.Mask) (roundrect_rratio 0.059)
      (net 4 Board_1-/VBUS-) (solder_mask_margin 0.1016))
    (pad CAN-H smd roundrect (at 5.05 31) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 1 Board_1-/CAN+) (solder_mask_margin 0.1016))
    (pad CAN-L smd roundrect (at 5.05 33.5) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 2 Board_1-/CAN-) (solder_mask_margin 0.1016))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 66.500001 91.050001 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.92 90) (layer F.SilkS) hide)
    (fp_text value 120R (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 Board_1-/CAN-))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:Connector_Keystone_4912_Overlaid" locked (layer F.Cu) (tedit 603C8B9E)
    (at 75.450001 77.240001 90)
    (fp_text reference T1 (at -3.175 -2.54 270) (layer F.Fab))
    (fp_text value "Keystone 4912" (at 0 5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 1 thru_hole circle (at -2.54 2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
  )
  (module "1 My Footprints:Connector_Keystone_4912_Overlaid" locked (layer F.Cu) (tedit 603C8BCB)
    (at 75.450001 60.750001 90)
    (fp_text reference T2 (at -3.175 -2.54 270) (layer F.Fab))
    (fp_text value "Keystone 4912" (at 0 5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 1 thru_hole circle (at 2.54 2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
  )
  (module SnapEDA-zip:TE_2204535-1 locked (layer F.Cu) (tedit 603C8BDE)
    (at 82.300001 69.000001 90)
    (fp_text reference JB3 (at 3.325 -3.15 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.7 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 4 thru_hole circle (at -5.7 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 2 thru_hole circle (at 0 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 5 thru_hole circle (at 0 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 3 thru_hole circle (at 5.7 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 6 thru_hole circle (at 5.7 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad "" np_thru_hole circle (at -7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -5.7 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 2 thru_hole circle (at 0 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 3 thru_hole circle (at 5.7 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 4 thru_hole circle (at -5.7 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 5 thru_hole circle (at 0 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 6 thru_hole circle (at 5.7 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (model ${KIPRJMOD}/shapes3D/TE_2204535-1.stp
      (offset (xyz 0 -9.949999999999999 10.7))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:TE_2204529-1" (layer F.Cu) (tedit 603C8C5D)
    (at 76.250001 69.000001 270)
    (fp_text reference JA3 (at -3.4 3.15 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 -0.45 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 5.7 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 3 thru_hole circle (at -5.7 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 2 thru_hole circle (at 0 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 2 thru_hole circle (at 0 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad "" np_thru_hole circle (at -7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.7 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 1 thru_hole circle (at 5.7 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
  )
  (gr_line (start 121.2598 133.749) (end 89.4902 133.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.357 133.7442) (end 121.2598 133.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.4531 133.73) (end 121.357 133.7442) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.5474 133.7064) (end 121.4531 133.73) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.6389 133.6736) (end 121.5474 133.7064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.7267 133.6321) (end 121.6389 133.6736) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.81 133.5821) (end 121.7267 133.6321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.8881 133.5243) (end 121.81 133.5821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.96 133.459) (end 121.8881 133.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0253 133.387) (end 121.96 133.459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0832 133.309) (end 122.0253 133.387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1331 133.2257) (end 122.0832 133.309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1746 133.1379) (end 122.1331 133.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2074 133.0464) (end 122.1746 133.1379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.231 132.9521) (end 122.2074 133.0464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2452 132.856) (end 122.231 132.9521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.25 132.7588) (end 122.2452 132.856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.25 131.9912) (end 122.25 132.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2452 131.894) (end 122.25 131.9912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.231 131.7979) (end 122.2452 131.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2074 131.7036) (end 122.231 131.7979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1746 131.6121) (end 122.2074 131.7036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1331 131.5243) (end 122.1746 131.6121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0832 131.441) (end 122.1331 131.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0253 131.363) (end 122.0832 131.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.96 131.291) (end 122.0253 131.363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.8881 131.2257) (end 121.96 131.291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.81 131.1679) (end 121.8881 131.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.7267 131.1179) (end 121.81 131.1679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.6389 131.0764) (end 121.7267 131.1179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.5474 131.0436) (end 121.6389 131.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.4531 131.02) (end 121.5474 131.0436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.357 131.0058) (end 121.4531 131.02) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.2598 131.001) (end 121.357 131.0058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.2501 131.0009) (end 121.2598 131.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.0406 130.9897) (end 119.2501 131.0009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.8338 130.9569) (end 119.0406 130.9897) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.632 130.9028) (end 118.8338 130.9569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.4484 130.8327) (end 118.632 130.9028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.4244 130.822) (end 118.4484 130.8327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.2612 130.7389) (end 118.4244 130.822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.2385 130.7258) (end 118.2612 130.7389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.0738 130.6184) (end 118.2385 130.7258) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.9115 130.4869) (end 118.0738 130.6184) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.7634 130.3389) (end 117.9115 130.4869) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.6395 130.1864) (end 117.7634 130.3389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.624 130.1651) (end 117.6395 130.1864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5175 130.0005) (end 117.624 130.1651) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.428 129.8256) (end 117.5175 130.0005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.4173 129.8016) (end 117.428 129.8256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.3473 129.6185) (end 117.4173 129.8016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2961 129.4288) (end 117.3473 129.6185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2907 129.4031) (end 117.2961 129.4288) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2603 129.2088) (end 117.2907 129.4031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.249 128.9934) (end 117.2603 129.2088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.249 125.7761) (end 117.249 128.9934) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2463 125.6977) (end 117.249 125.7761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2353 125.5938) (end 117.2463 125.6977) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2136 125.4917) (end 117.2353 125.5938) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.1814 125.3926) (end 117.2136 125.4917) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.1388 125.297) (end 117.1814 125.3926) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0866 125.2065) (end 117.1388 125.297) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0252 125.1221) (end 117.0866 125.2065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9555 125.0447) (end 117.0252 125.1221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8779 124.9748) (end 116.9555 125.0447) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7932 124.9132) (end 116.8779 124.9748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7028 124.861) (end 116.7932 124.9132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6074 124.8186) (end 116.7028 124.861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5083 124.7864) (end 116.6074 124.8186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4059 124.7646) (end 116.5083 124.7864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3024 124.7537) (end 116.4059 124.7646) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2239 124.751) (end 116.3024 124.7537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.2564 124.751) (end 116.2239 124.751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1979 124.7479) (end 99.2564 124.751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1589 124.7421) (end 99.1979 124.7479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1331 124.7367) (end 99.1589 124.7421) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0829 124.7218) (end 99.1331 124.7367) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0461 124.7073) (end 99.0829 124.7218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9994 124.6834) (end 99.0461 124.7073) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9555 124.6549) (end 98.9994 124.6834) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9152 124.6222) (end 98.9555 124.6549) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8778 124.5848) (end 98.9152 124.6222) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8448 124.544) (end 98.8778 124.5848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8163 124.5001) (end 98.8448 124.544) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7925 124.4534) (end 98.8163 124.5001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7738 124.4044) (end 98.7925 124.4534) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7602 124.3538) (end 98.7738 124.4044) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7521 124.302) (end 98.7602 124.3538) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.749 124.2436) (end 98.7521 124.302) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.749 108.9913) (end 98.749 124.2436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7442 108.894) (end 98.749 108.9913) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.73 108.7979) (end 98.7442 108.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7064 108.7036) (end 98.73 108.7979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.6736 108.6122) (end 98.7064 108.7036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.6321 108.5243) (end 98.6736 108.6122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.5821 108.441) (end 98.6321 108.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.5243 108.363) (end 98.5821 108.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.459 108.291) (end 98.5243 108.363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.387 108.2257) (end 98.459 108.291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.309 108.1679) (end 98.387 108.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.2257 108.1179) (end 98.309 108.1679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.1379 108.0764) (end 98.2257 108.1179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.0464 108.0436) (end 98.1379 108.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.9521 108.02) (end 98.0464 108.0436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.856 108.0058) (end 97.9521 108.02) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.7588 108.001) (end 97.856 108.0058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.7412 108.001) (end 97.7588 108.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.644 108.0058) (end 94.7412 108.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.5479 108.02) (end 94.644 108.0058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.4536 108.0436) (end 94.5479 108.02) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.3621 108.0764) (end 94.4536 108.0436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.2743 108.1179) (end 94.3621 108.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.191 108.1679) (end 94.2743 108.1179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.113 108.2257) (end 94.191 108.1679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.041 108.291) (end 94.113 108.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.9757 108.363) (end 94.041 108.291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.9179 108.441) (end 93.9757 108.363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.8679 108.5243) (end 93.9179 108.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.8264 108.6122) (end 93.8679 108.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7936 108.7036) (end 93.8264 108.6122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.77 108.7979) (end 93.7936 108.7036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7558 108.894) (end 93.77 108.7979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.751 108.9913) (end 93.7558 108.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.751 128.9934) (end 93.751 108.9913) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7397 129.2089) (end 93.751 128.9934) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.707 129.4157) (end 93.7397 129.2089) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.6526 129.6185) (end 93.707 129.4157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.5827 129.8016) (end 93.6526 129.6185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.572 129.8256) (end 93.5827 129.8016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.4827 130.0001) (end 93.572 129.8256) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.376 130.1651) (end 93.4827 130.0001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.3606 130.1864) (end 93.376 130.1651) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.2369 130.3385) (end 93.3606 130.1864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.0885 130.487) (end 93.2369 130.3385) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.9364 130.6106) (end 93.0885 130.487) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.9151 130.626) (end 92.9364 130.6106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.7615 130.7257) (end 92.9151 130.626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.7388 130.7389) (end 92.7615 130.7257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.564 130.8276) (end 92.7388 130.7389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.3806 130.8983) (end 92.564 130.8276) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.3556 130.9065) (end 92.3806 130.8983) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1788 130.9539) (end 92.3556 130.9065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1531 130.9593) (end 92.1788 130.9539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.9588 130.9897) (end 92.1531 130.9593) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7501 131.0009) (end 91.9588 130.9897) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.4902 131.001) (end 91.7501 131.0009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.393 131.0058) (end 89.4902 131.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2969 131.02) (end 89.393 131.0058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2026 131.0436) (end 89.2969 131.02) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.1111 131.0764) (end 89.2026 131.0436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.0233 131.1179) (end 89.1111 131.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.94 131.1679) (end 89.0233 131.1179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.862 131.2257) (end 88.94 131.1679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.79 131.291) (end 88.862 131.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.7247 131.363) (end 88.79 131.291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6669 131.441) (end 88.7247 131.363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6169 131.5243) (end 88.6669 131.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5754 131.6121) (end 88.6169 131.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5426 131.7036) (end 88.5754 131.6121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.519 131.7979) (end 88.5426 131.7036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5048 131.894) (end 88.519 131.7979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5 131.9912) (end 88.5048 131.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5 132.7588) (end 88.5 131.9912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5048 132.856) (end 88.5 132.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.519 132.9521) (end 88.5048 132.856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5426 133.0464) (end 88.519 132.9521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5754 133.1379) (end 88.5426 133.0464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6169 133.2257) (end 88.5754 133.1379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6669 133.309) (end 88.6169 133.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.7247 133.387) (end 88.6669 133.309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.79 133.459) (end 88.7247 133.387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.862 133.5243) (end 88.79 133.459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.94 133.5821) (end 88.862 133.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.0233 133.6321) (end 88.94 133.5821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.1111 133.6736) (end 89.0233 133.6321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2026 133.7064) (end 89.1111 133.6736) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2969 133.73) (end 89.2026 133.7064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.393 133.7442) (end 89.2969 133.73) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.4902 133.749) (end 89.393 133.7442) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5 49.0088) (end 88.5 48.4912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5048 49.106) (end 88.5 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.519 49.2021) (end 88.5048 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5426 49.2964) (end 88.519 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5754 49.3879) (end 88.5426 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6169 49.4757) (end 88.5754 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6669 49.559) (end 88.6169 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.7247 49.637) (end 88.6669 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.79 49.709) (end 88.7247 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.862 49.7743) (end 88.79 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.94 49.8321) (end 88.862 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.0233 49.8821) (end 88.94 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.1111 49.9236) (end 89.0233 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2026 49.9564) (end 89.1111 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2969 49.98) (end 89.2026 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.393 49.9942) (end 89.2969 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.4902 49.999) (end 89.393 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.7502 49.9991) (end 89.4902 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 91.9589 50.0103) (end 91.7502 49.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.153 50.0407) (end 91.9589 50.0103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.1787 50.0461) (end 92.153 50.0407) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.3556 50.0935) (end 92.1787 50.0461) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.3804 50.1016) (end 92.3556 50.0935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.5516 50.1673) (end 92.3804 50.1016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.5756 50.178) (end 92.5516 50.1673) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.7501 50.2673) (end 92.5756 50.178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.9151 50.374) (end 92.7501 50.2673) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 92.9364 50.3894) (end 92.9151 50.374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.0885 50.5131) (end 92.9364 50.3894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.2366 50.6611) (end 93.0885 50.5131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.3687 50.8243) (end 93.2366 50.6611) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.4757 50.9885) (end 93.3687 50.8243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.4889 51.0112) (end 93.4757 50.9885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.572 51.1744) (end 93.4889 51.0112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.5827 51.1984) (end 93.572 51.1744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.6527 51.3815) (end 93.5827 51.1984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7039 51.5712) (end 93.6527 51.3815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7093 51.597) (end 93.7039 51.5712) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7397 51.7906) (end 93.7093 51.597) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.751 52.0065) (end 93.7397 51.7906) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.751 72.0088) (end 93.751 52.0065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7558 72.106) (end 93.751 72.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.77 72.2021) (end 93.7558 72.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.7936 72.2964) (end 93.77 72.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.8264 72.3879) (end 93.7936 72.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.8679 72.4757) (end 93.8264 72.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.9179 72.559) (end 93.8679 72.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 93.9757 72.637) (end 93.9179 72.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.041 72.709) (end 93.9757 72.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.113 72.7743) (end 94.041 72.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.191 72.8321) (end 94.113 72.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.2743 72.8821) (end 94.191 72.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.3621 72.9236) (end 94.2743 72.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.4536 72.9564) (end 94.3621 72.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.5479 72.98) (end 94.4536 72.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.644 72.9942) (end 94.5479 72.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.7412 72.999) (end 94.644 72.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.7588 72.999) (end 94.7412 72.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.856 72.9942) (end 97.7588 72.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 97.9521 72.98) (end 97.856 72.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.0464 72.9564) (end 97.9521 72.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.1379 72.9236) (end 98.0464 72.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.2257 72.8821) (end 98.1379 72.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.309 72.8321) (end 98.2257 72.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.3871 72.7743) (end 98.309 72.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.459 72.709) (end 98.3871 72.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.5243 72.637) (end 98.459 72.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.5822 72.559) (end 98.5243 72.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.6321 72.4757) (end 98.5822 72.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.6736 72.3879) (end 98.6321 72.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7064 72.2964) (end 98.6736 72.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.73 72.2021) (end 98.7064 72.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7442 72.106) (end 98.73 72.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.749 72.0088) (end 98.7442 72.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.749 69.5066) (end 98.749 72.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7521 69.4479) (end 98.749 69.5066) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7579 69.4086) (end 98.7521 69.4479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7738 69.3455) (end 98.7579 69.4086) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7982 69.2847) (end 98.7738 69.3455) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8163 69.2499) (end 98.7982 69.2847) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8375 69.2166) (end 98.8163 69.2499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8778 69.1652) (end 98.8375 69.2166) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.925 69.1194) (end 98.8778 69.1652) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9555 69.0951) (end 98.925 69.1194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9885 69.0733) (end 98.9555 69.0951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0462 69.0427) (end 98.9885 69.0733) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0956 69.0238) (end 99.0462 69.0427) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1457 69.0103) (end 99.0956 69.0238) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1846 69.0038) (end 99.1457 69.0103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.2105 69.0011) (end 99.1846 69.0038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.2565 68.999) (end 99.2105 69.0011) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.2248 68.999) (end 99.2565 68.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.3007 68.9964) (end 109.2248 68.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.401 68.9862) (end 109.3007 68.9964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.5 68.9659) (end 109.401 68.9862) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.5967 68.9356) (end 109.5 68.9659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.6893 68.8958) (end 109.5967 68.9356) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.7776 68.8468) (end 109.6893 68.8958) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.8606 68.7891) (end 109.7776 68.8468) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.9373 68.7232) (end 109.8606 68.7891) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0071 68.6498) (end 109.9373 68.7232) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0688 68.5701) (end 110.0071 68.6498) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1223 68.4843) (end 110.0688 68.5701) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1669 68.3933) (end 110.1223 68.4843) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.202 68.2985) (end 110.1669 68.3933) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2273 68.201) (end 110.202 68.2985) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2426 68.1008) (end 110.2273 68.201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2477 67.9999) (end 110.2426 68.1008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2426 67.8989) (end 110.2477 67.9999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2273 67.799) (end 110.2426 67.8989) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.2019 67.7012) (end 110.2273 67.799) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1668 67.6064) (end 110.2019 67.7012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1223 67.5157) (end 110.1668 67.6064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0688 67.4299) (end 110.1223 67.5157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.0069 67.35) (end 110.0688 67.4299) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.9373 67.2768) (end 110.0069 67.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.8606 67.2109) (end 109.9373 67.2768) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.7776 67.1532) (end 109.8606 67.2109) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.6893 67.1042) (end 109.7776 67.1532) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.5964 67.0643) (end 109.6893 67.1042) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.5 67.0341) (end 109.5964 67.0643) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.401 67.0138) (end 109.5 67.0341) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.3007 67.0036) (end 109.401 67.0138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 109.2248 67.001) (end 109.3007 67.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.2501 67.0009) (end 109.2248 67.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1974 66.9979) (end 99.2501 67.0009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1456 66.9897) (end 99.1974 66.9979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.095 66.9761) (end 99.1456 66.9897) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0466 66.9575) (end 99.095 66.9761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9999 66.9337) (end 99.0466 66.9575) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9559 66.9052) (end 98.9999 66.9337) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9152 66.8722) (end 98.9559 66.9052) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8868 66.8444) (end 98.9152 66.8722) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.853 66.8047) (end 98.8868 66.8444) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8375 66.7835) (end 98.853 66.8047) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8163 66.7501) (end 98.8375 66.7835) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7877 66.6917) (end 98.8163 66.7501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7738 66.6544) (end 98.7877 66.6917) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7602 66.6038) (end 98.7738 66.6544) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7521 66.5526) (end 98.7602 66.6038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7491 66.4999) (end 98.7521 66.5526) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.749 56.7566) (end 98.7491 66.4999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7521 56.6979) (end 98.749 56.7566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7602 56.6461) (end 98.7521 56.6979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7738 56.5955) (end 98.7602 56.6461) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.7925 56.5466) (end 98.7738 56.5955) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8166 56.4994) (end 98.7925 56.5466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8451 56.4555) (end 98.8166 56.4994) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.8781 56.4148) (end 98.8451 56.4555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9152 56.3778) (end 98.8781 56.4148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.956 56.3448) (end 98.9152 56.3778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.9995 56.3165) (end 98.956 56.3448) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0462 56.2927) (end 98.9995 56.3165) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.0829 56.2782) (end 99.0462 56.2927) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1079 56.2701) (end 99.0829 56.2782) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.1588 56.2579) (end 99.1079 56.2701) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.198 56.2521) (end 99.1588 56.2579) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 99.2564 56.249) (end 99.198 56.2521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.2239 56.249) (end 99.2564 56.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.3024 56.2463) (end 116.2239 56.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.4059 56.2354) (end 116.3024 56.2463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.5083 56.2136) (end 116.4059 56.2354) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.6074 56.1814) (end 116.5083 56.2136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7028 56.139) (end 116.6074 56.1814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.7932 56.0868) (end 116.7028 56.139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.8779 56.0252) (end 116.7932 56.0868) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.9555 55.9553) (end 116.8779 56.0252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0252 55.8779) (end 116.9555 55.9553) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.0866 55.7935) (end 117.0252 55.8779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.139 55.7028) (end 117.0866 55.7935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.1814 55.6074) (end 117.139 55.7028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2136 55.5083) (end 117.1814 55.6074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2353 55.4062) (end 117.2136 55.5083) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2463 55.3023) (end 117.2353 55.4062) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.249 55.224) (end 117.2463 55.3023) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.249 52.0066) (end 117.249 55.224) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2603 51.7911) (end 117.249 52.0066) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2907 51.597) (end 117.2603 51.7911) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.2961 51.5713) (end 117.2907 51.597) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.3472 51.382) (end 117.2961 51.5713) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.4173 51.1984) (end 117.3472 51.382) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.428 51.1744) (end 117.4173 51.1984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.5173 50.9999) (end 117.428 51.1744) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.624 50.8349) (end 117.5173 50.9999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.6394 50.8136) (end 117.624 50.8349) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.7634 50.6611) (end 117.6394 50.8136) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 117.9111 50.5134) (end 117.7634 50.6611) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.0739 50.3816) (end 117.9111 50.5134) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.2385 50.2743) (end 118.0739 50.3816) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.2612 50.2611) (end 118.2385 50.2743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.4244 50.178) (end 118.2612 50.2611) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.4484 50.1673) (end 118.4244 50.178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.632 50.0972) (end 118.4484 50.1673) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.8338 50.0431) (end 118.632 50.0972) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.0406 50.0103) (end 118.8338 50.0431) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.2501 49.9991) (end 119.0406 50.0103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.2598 49.999) (end 119.2501 49.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.357 49.9942) (end 121.2598 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.4531 49.98) (end 121.357 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.5474 49.9564) (end 121.4531 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.6389 49.9236) (end 121.5474 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.7267 49.8821) (end 121.6389 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.81 49.8321) (end 121.7267 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.8881 49.7743) (end 121.81 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.96 49.709) (end 121.8881 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0253 49.637) (end 121.96 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0832 49.559) (end 122.0253 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1331 49.4757) (end 122.0832 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1746 49.3879) (end 122.1331 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2074 49.2964) (end 122.1746 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.231 49.2021) (end 122.2074 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2452 49.106) (end 122.231 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.25 49.0088) (end 122.2452 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.25 48.4912) (end 122.25 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2452 48.394) (end 122.25 48.4912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.231 48.2979) (end 122.2452 48.394) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.2074 48.2036) (end 122.231 48.2979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1746 48.1121) (end 122.2074 48.2036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.1331 48.0243) (end 122.1746 48.1121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0832 47.941) (end 122.1331 48.0243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.0253 47.863) (end 122.0832 47.941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.96 47.791) (end 122.0253 47.863) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.8881 47.7257) (end 121.96 47.791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.81 47.6679) (end 121.8881 47.7257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.7267 47.6179) (end 121.81 47.6679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.6389 47.5764) (end 121.7267 47.6179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.5474 47.5436) (end 121.6389 47.5764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.4531 47.52) (end 121.5474 47.5436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.357 47.5058) (end 121.4531 47.52) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.2598 47.501) (end 121.357 47.5058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.4902 47.501) (end 121.2598 47.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.393 47.5058) (end 89.4902 47.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2969 47.52) (end 89.393 47.5058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.2026 47.5436) (end 89.2969 47.52) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.1111 47.5764) (end 89.2026 47.5436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 89.0233 47.6179) (end 89.1111 47.5764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.94 47.6679) (end 89.0233 47.6179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.862 47.7257) (end 88.94 47.6679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.79 47.791) (end 88.862 47.7257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.7247 47.863) (end 88.79 47.791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6669 47.941) (end 88.7247 47.863) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.6169 48.0243) (end 88.6669 47.941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5754 48.1121) (end 88.6169 48.0243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5426 48.2036) (end 88.5754 48.1121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.519 48.2979) (end 88.5426 48.2036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5048 48.394) (end 88.519 48.2979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 88.5 48.4912) (end 88.5048 48.394) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4765 42.5) (end 50.0092 42.5007) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4918 42.5008) (end 142.4765 42.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4977 42.504) (end 142.4918 42.5008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.5002 42.5092) (end 142.4977 42.504) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.501 42.5245) (end 142.5002 42.5092) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.501 47.4765) (end 142.501 42.5245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.5002 47.4918) (end 142.501 47.4765) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4977 47.497) (end 142.5002 47.4918) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4918 47.5002) (end 142.4977 47.497) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4765 47.501) (end 142.4918 47.5002) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.2403 47.501) (end 142.4765 47.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.143 47.5058) (end 138.2403 47.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.0469 47.52) (end 138.143 47.5058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.9526 47.5436) (end 138.0469 47.52) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.8612 47.5764) (end 137.9526 47.5436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.7733 47.6179) (end 137.8612 47.5764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.69 47.6679) (end 137.7733 47.6179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.612 47.7257) (end 137.69 47.6679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.54 47.791) (end 137.612 47.7257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4747 47.863) (end 137.54 47.791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4169 47.941) (end 137.4747 47.863) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3669 48.0243) (end 137.4169 47.941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3254 48.1121) (end 137.3669 48.0243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2926 48.2036) (end 137.3254 48.1121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.269 48.2979) (end 137.2926 48.2036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2548 48.394) (end 137.269 48.2979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.25 48.4912) (end 137.2548 48.394) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.25 49.0088) (end 137.25 48.4912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2548 49.106) (end 137.25 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.269 49.2021) (end 137.2548 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2926 49.2964) (end 137.269 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3254 49.3879) (end 137.2926 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3669 49.4757) (end 137.3254 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4169 49.559) (end 137.3669 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4747 49.637) (end 137.4169 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.54 49.709) (end 137.4747 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.612 49.7743) (end 137.54 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.69 49.8321) (end 137.612 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.7733 49.8821) (end 137.69 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.8612 49.9236) (end 137.7733 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.9526 49.9564) (end 137.8612 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.0469 49.98) (end 137.9526 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.143 49.9942) (end 138.0469 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.2403 49.999) (end 138.143 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.4935 49.999) (end 138.2403 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.696 50.0093) (end 140.4935 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.7222 50.012) (end 140.696 50.0093) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.903 50.0407) (end 140.7222 50.012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.9287 50.0461) (end 140.903 50.0407) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.1185 50.0974) (end 140.9287 50.0461) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.3018 50.1674) (end 141.1185 50.0974) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.3256 50.178) (end 141.3018 50.1674) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.5006 50.2675) (end 141.3256 50.178) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.6651 50.374) (end 141.5006 50.2675) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.6864 50.3894) (end 141.6651 50.374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.8385 50.5131) (end 141.6864 50.3894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.9777 50.6518) (end 141.8385 50.5131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.9953 50.6713) (end 141.9777 50.6518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.1187 50.8243) (end 141.9953 50.6713) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2258 50.9885) (end 142.1187 50.8243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2389 51.0112) (end 142.2258 50.9885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3276 51.186) (end 142.2389 51.0112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3984 51.3694) (end 142.3276 51.186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4065 51.3944) (end 142.3984 51.3694) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4569 51.5838) (end 142.4065 51.3944) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.488 51.7778) (end 142.4569 51.5838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4907 51.804) (end 142.488 51.7778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.501 52.0065) (end 142.4907 51.804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.501 128.9934) (end 142.501 52.0065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4907 129.196) (end 142.501 128.9934) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.488 129.2221) (end 142.4907 129.196) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.457 129.4157) (end 142.488 129.2221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4065 129.6056) (end 142.457 129.4157) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3984 129.6306) (end 142.4065 129.6056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.3278 129.8135) (end 142.3984 129.6306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2389 129.9888) (end 142.3278 129.8135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.2258 130.0115) (end 142.2389 129.9888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.1187 130.1758) (end 142.2258 130.0115) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.9953 130.3287) (end 142.1187 130.1758) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.9777 130.3482) (end 141.9953 130.3287) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.8389 130.4866) (end 141.9777 130.3482) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.6864 130.6106) (end 141.8389 130.4866) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.6651 130.626) (end 141.6864 130.6106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.5005 130.7325) (end 141.6651 130.626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.3256 130.822) (end 141.5005 130.7325) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.3019 130.8326) (end 141.3256 130.822) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.1185 130.9027) (end 141.3019 130.8326) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.9288 130.9539) (end 141.1185 130.9027) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.9031 130.9593) (end 140.9288 130.9539) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.7222 130.988) (end 140.9031 130.9593) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.696 130.9907) (end 140.7222 130.988) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.4935 131.001) (end 140.696 130.9907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.2403 131.001) (end 140.4935 131.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.143 131.0058) (end 138.2403 131.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.0469 131.02) (end 138.143 131.0058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.9526 131.0436) (end 138.0469 131.02) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.8612 131.0764) (end 137.9526 131.0436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.7733 131.1179) (end 137.8612 131.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.69 131.1679) (end 137.7733 131.1179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.612 131.2257) (end 137.69 131.1679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.54 131.291) (end 137.612 131.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4747 131.363) (end 137.54 131.291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4169 131.441) (end 137.4747 131.363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3669 131.5243) (end 137.4169 131.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3254 131.6121) (end 137.3669 131.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2926 131.7036) (end 137.3254 131.6121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.269 131.7979) (end 137.2926 131.7036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2548 131.894) (end 137.269 131.7979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.25 131.9912) (end 137.2548 131.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.25 132.7588) (end 137.25 131.9912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2548 132.856) (end 137.25 132.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.269 132.9521) (end 137.2548 132.856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2926 133.0464) (end 137.269 132.9521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3254 133.1379) (end 137.2926 133.0464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3669 133.2257) (end 137.3254 133.1379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4169 133.309) (end 137.3669 133.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4747 133.387) (end 137.4169 133.309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.54 133.459) (end 137.4747 133.387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.612 133.5243) (end 137.54 133.459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.69 133.5821) (end 137.612 133.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.7733 133.6321) (end 137.69 133.5821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.8612 133.6736) (end 137.7733 133.6321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.9526 133.7064) (end 137.8612 133.6736) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.0469 133.73) (end 137.9526 133.7064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.143 133.7442) (end 138.0469 133.73) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.2403 133.749) (end 138.143 133.7442) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4765 133.749) (end 138.2403 133.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4918 133.7498) (end 142.4765 133.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4977 133.753) (end 142.4918 133.7498) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.5002 133.7582) (end 142.4977 133.753) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.501 133.7735) (end 142.5002 133.7582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.501 138.7255) (end 142.501 133.7735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.5002 138.7408) (end 142.501 138.7255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.497 138.7467) (end 142.5002 138.7408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4918 138.7492) (end 142.497 138.7467) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.4765 138.75) (end 142.4918 138.7492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0235 138.75) (end 142.4765 138.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0082 138.7492) (end 50.0235 138.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0023 138.746) (end 50.0082 138.7492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.9998 138.7408) (end 50.0023 138.746) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 138.7255) (end 49.9998 138.7408) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 133.7735) (end 49.999 138.7255) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0003 133.7563) (end 49.999 133.7735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.003 133.7523) (end 50.0003 133.7563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0073 133.75) (end 50.003 133.7523) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.5098 133.749) (end 50.0073 133.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.607 133.7442) (end 72.5098 133.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7031 133.73) (end 72.607 133.7442) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7974 133.7064) (end 72.7031 133.73) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8889 133.6736) (end 72.7974 133.7064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9767 133.6321) (end 72.8889 133.6736) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.06 133.5821) (end 72.9767 133.6321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.138 133.5243) (end 73.06 133.5821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.21 133.459) (end 73.138 133.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2753 133.387) (end 73.21 133.459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3331 133.309) (end 73.2753 133.387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3831 133.2257) (end 73.3331 133.309) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4246 133.1379) (end 73.3831 133.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4574 133.0464) (end 73.4246 133.1379) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.481 132.9521) (end 73.4574 133.0464) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4952 132.856) (end 73.481 132.9521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5 132.7588) (end 73.4952 132.856) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5 131.9912) (end 73.5 132.7588) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4952 131.894) (end 73.5 131.9912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.481 131.7979) (end 73.4952 131.894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4574 131.7036) (end 73.481 131.7979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4246 131.6121) (end 73.4574 131.7036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3831 131.5243) (end 73.4246 131.6121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3331 131.441) (end 73.3831 131.5243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2753 131.363) (end 73.3331 131.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.21 131.291) (end 73.2753 131.363) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.138 131.2257) (end 73.21 131.291) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.06 131.1679) (end 73.138 131.2257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9767 131.1179) (end 73.06 131.1679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8889 131.0764) (end 72.9767 131.1179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7974 131.0436) (end 72.8889 131.0764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7031 131.02) (end 72.7974 131.0436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.607 131.0058) (end 72.7031 131.02) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.5098 131.001) (end 72.607 131.0058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.5001 131.0009) (end 72.5098 131.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.2906 130.9897) (end 70.5001 131.0009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.0838 130.9569) (end 70.2906 130.9897) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.882 130.9028) (end 70.0838 130.9569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.6865 130.8278) (end 69.882 130.9028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.4999 130.7327) (end 69.6865 130.8278) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.3349 130.626) (end 69.4999 130.7327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.3136 130.6106) (end 69.3349 130.626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1713 130.4953) (end 69.3136 130.6106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1518 130.4777) (end 69.1713 130.4953) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.013 130.3385) (end 69.1518 130.4777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8813 130.1757) (end 69.013 130.3385) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7743 130.0115) (end 68.8813 130.1757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7611 129.9888) (end 68.7743 130.0115) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6724 129.814) (end 68.7611 129.9888) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6017 129.6306) (end 68.6724 129.814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5935 129.6056) (end 68.6017 129.6306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5431 129.4162) (end 68.5935 129.6056) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5103 129.2088) (end 68.5431 129.4162) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.499 128.9935) (end 68.5103 129.2088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.499 125.7761) (end 68.499 128.9935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4963 125.6977) (end 68.499 125.7761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4853 125.5938) (end 68.4963 125.6977) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4636 125.4917) (end 68.4853 125.5938) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4314 125.3926) (end 68.4636 125.4917) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.389 125.2972) (end 68.4314 125.3926) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3366 125.2065) (end 68.389 125.2972) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2752 125.1221) (end 68.3366 125.2065) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2053 125.0445) (end 68.2752 125.1221) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1279 124.9748) (end 68.2053 125.0445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.0435 124.9134) (end 68.1279 124.9748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.953 124.8612) (end 68.0435 124.9134) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.8574 124.8186) (end 67.953 124.8612) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.7583 124.7864) (end 67.8574 124.8186) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.6562 124.7647) (end 67.7583 124.7864) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.5524 124.7537) (end 67.6562 124.7647) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.4739 124.751) (end 67.5524 124.7537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4998 124.7509) (end 67.4739 124.751) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4474 124.7479) (end 50.4998 124.7509) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3956 124.7397) (end 50.4474 124.7479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.345 124.7261) (end 50.3956 124.7397) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2966 124.7075) (end 50.345 124.7261) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2499 124.6837) (end 50.2966 124.7075) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2059 124.6552) (end 50.2499 124.6837) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1652 124.6222) (end 50.2059 124.6552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.137 124.5945) (end 50.1652 124.6222) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1194 124.575) (end 50.137 124.5945) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0875 124.5335) (end 50.1194 124.575) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0603 124.489) (end 50.0875 124.5335) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0376 124.4415) (end 50.0603 124.489) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0238 124.4044) (end 50.0376 124.4415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0102 124.3538) (end 50.0238 124.4044) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0021 124.302) (end 50.0102 124.3538) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 124.2435) (end 50.0021 124.302) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 69.5066) (end 49.999 124.2435) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0021 69.4479) (end 49.999 69.5066) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0102 69.3961) (end 50.0021 69.4479) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0238 69.3455) (end 50.0102 69.3961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0376 69.3085) (end 50.0238 69.3455) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0666 69.2494) (end 50.0376 69.3085) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0948 69.2059) (end 50.0666 69.2494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1196 69.1748) (end 50.0948 69.2059) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1555 69.137) (end 50.1196 69.1748) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.175 69.1194) (end 50.1555 69.137) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.206 69.0948) (end 50.175 69.1194) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2495 69.0665) (end 50.206 69.0948) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2962 69.0427) (end 50.2495 69.0665) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3329 69.0282) (end 50.2962 69.0427) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3579 69.0201) (end 50.3329 69.0282) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4086 69.0079) (end 50.3579 69.0201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.448 69.0021) (end 50.4086 69.0079) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4999 68.9991) (end 50.448 69.0021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.4748 68.999) (end 50.4999 68.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.5507 68.9964) (end 60.4748 68.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.6509 68.9862) (end 60.5507 68.9964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.7499 68.9659) (end 60.6509 68.9862) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.8464 68.9357) (end 60.7499 68.9659) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.9395 68.8957) (end 60.8464 68.9357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.0279 68.8466) (end 60.9395 68.8957) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.1106 68.7891) (end 61.0279 68.8466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.1873 68.7232) (end 61.1106 68.7891) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.2569 68.65) (end 61.1873 68.7232) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.319 68.5699) (end 61.2569 68.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.3724 68.4841) (end 61.319 68.5699) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4169 68.3933) (end 61.3724 68.4841) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4519 68.2988) (end 61.4169 68.3933) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4773 68.201) (end 61.4519 68.2988) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4926 68.1011) (end 61.4773 68.201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4977 68.0001) (end 61.4926 68.1011) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4926 67.8992) (end 61.4977 68.0001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4773 67.7993) (end 61.4926 67.8992) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.452 67.7015) (end 61.4773 67.7993) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.4169 67.6067) (end 61.452 67.7015) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.3724 67.5159) (end 61.4169 67.6067) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.319 67.4302) (end 61.3724 67.5159) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.2569 67.35) (end 61.319 67.4302) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.1873 67.2768) (end 61.2569 67.35) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.1108 67.2111) (end 61.1873 67.2768) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 61.0279 67.1534) (end 61.1108 67.2111) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.9395 67.1043) (end 61.0279 67.1534) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.8466 67.0644) (end 60.9395 67.1043) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.7502 67.0342) (end 60.8466 67.0644) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.6512 67.0138) (end 60.7502 67.0342) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.5507 67.0036) (end 60.6512 67.0138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60.4748 67.001) (end 60.5507 67.0036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.5001 67.0009) (end 60.4748 67.001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4474 66.9979) (end 50.5001 67.0009) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3961 66.9898) (end 50.4474 66.9979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3455 66.9762) (end 50.3961 66.9898) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3083 66.9623) (end 50.3455 66.9762) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2499 66.9337) (end 50.3083 66.9623) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2166 66.9125) (end 50.2499 66.9337) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1953 66.897) (end 50.2166 66.9125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1555 66.863) (end 50.1953 66.897) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1278 66.8348) (end 50.1555 66.863) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0948 66.794) (end 50.1278 66.8348) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0663 66.7501) (end 50.0948 66.794) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0425 66.7034) (end 50.0663 66.7501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0238 66.6544) (end 50.0425 66.7034) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0102 66.6038) (end 50.0238 66.6544) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0021 66.552) (end 50.0102 66.6038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 66.4936) (end 50.0021 66.552) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 56.7566) (end 49.999 66.4936) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0038 56.6847) (end 49.999 56.7566) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0103 56.6456) (end 50.0038 56.6847) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0238 56.5955) (end 50.0103 56.6456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0483 56.5345) (end 50.0238 56.5955) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0666 56.4994) (end 50.0483 56.5345) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0948 56.4559) (end 50.0666 56.4994) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.137 56.4055) (end 50.0948 56.4559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.1652 56.3778) (end 50.137 56.4055) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2055 56.3451) (end 50.1652 56.3778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2612 56.3102) (end 50.2055 56.3451) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.2966 56.2925) (end 50.2612 56.3102) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.3451 56.2739) (end 50.2966 56.2925) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.4088 56.2579) (end 50.3451 56.2739) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.448 56.2521) (end 50.4088 56.2579) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.5001 56.2491) (end 50.448 56.2521) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.4739 56.249) (end 50.5001 56.2491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.5524 56.2463) (end 67.4739 56.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.6562 56.2353) (end 67.5524 56.2463) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.7581 56.2137) (end 67.6562 56.2353) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.8574 56.1814) (end 67.7581 56.2137) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 67.9528 56.139) (end 67.8574 56.1814) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.0435 56.0866) (end 67.9528 56.139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.1279 56.0252) (end 68.0435 56.0866) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2055 55.9553) (end 68.1279 56.0252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.2752 55.8779) (end 68.2055 55.9553) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.3366 55.7935) (end 68.2752 55.8779) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.389 55.7028) (end 68.3366 55.7935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4314 55.6074) (end 68.389 55.7028) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4636 55.5083) (end 68.4314 55.6074) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4853 55.4062) (end 68.4636 55.5083) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.4963 55.3023) (end 68.4853 55.4062) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.499 55.2239) (end 68.4963 55.3023) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.499 52.0066) (end 68.499 55.2239) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5103 51.7911) (end 68.499 52.0066) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5431 51.5838) (end 68.5103 51.7911) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.5935 51.3944) (end 68.5431 51.5838) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6016 51.3694) (end 68.5935 51.3944) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.6722 51.1865) (end 68.6016 51.3694) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7611 51.0112) (end 68.6722 51.1865) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.7742 50.9885) (end 68.7611 51.0112) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 68.8813 50.8242) (end 68.7742 50.9885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.0131 50.6615) (end 68.8813 50.8242) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1518 50.5223) (end 69.0131 50.6615) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.1713 50.5047) (end 69.1518 50.5223) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.3136 50.3894) (end 69.1713 50.5047) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.3349 50.374) (end 69.3136 50.3894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.4999 50.2672) (end 69.3349 50.374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.6865 50.1722) (end 69.4999 50.2672) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 69.8815 50.0973) (end 69.6865 50.1722) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.0838 50.0431) (end 69.8815 50.0973) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.2906 50.0103) (end 70.0838 50.0431) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70.5001 49.9991) (end 70.2906 50.0103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.5098 49.999) (end 70.5001 49.9991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.607 49.9942) (end 72.5098 49.999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7031 49.98) (end 72.607 49.9942) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7974 49.9564) (end 72.7031 49.98) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8889 49.9236) (end 72.7974 49.9564) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9767 49.8821) (end 72.8889 49.9236) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.06 49.8321) (end 72.9767 49.8821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.138 49.7743) (end 73.06 49.8321) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.21 49.709) (end 73.138 49.7743) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2753 49.637) (end 73.21 49.709) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3331 49.559) (end 73.2753 49.637) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3831 49.4757) (end 73.3331 49.559) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4246 49.3879) (end 73.3831 49.4757) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4574 49.2964) (end 73.4246 49.3879) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.481 49.2021) (end 73.4574 49.2964) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4952 49.106) (end 73.481 49.2021) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5 49.0088) (end 73.4952 49.106) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.5 48.4912) (end 73.5 49.0088) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4952 48.394) (end 73.5 48.4912) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.481 48.2979) (end 73.4952 48.394) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4574 48.2036) (end 73.481 48.2979) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.4246 48.1121) (end 73.4574 48.2036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3831 48.0243) (end 73.4246 48.1121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.3331 47.941) (end 73.3831 48.0243) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.2753 47.863) (end 73.3331 47.941) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.21 47.791) (end 73.2753 47.863) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.138 47.7257) (end 73.21 47.791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73.06 47.6679) (end 73.138 47.7257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.9767 47.6179) (end 73.06 47.6679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.8889 47.5764) (end 72.9767 47.6179) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7974 47.5436) (end 72.8889 47.5764) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.7031 47.52) (end 72.7974 47.5436) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.607 47.5058) (end 72.7031 47.52) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 72.5098 47.501) (end 72.607 47.5058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0073 47.5) (end 72.5098 47.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.003 47.4977) (end 50.0073 47.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0003 47.4937) (end 50.003 47.4977) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 47.4765) (end 50.0003 47.4937) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 49.999 42.5245) (end 49.999 47.4765) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0006 42.5064) (end 49.999 42.5245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0037 42.5027) (end 50.0006 42.5064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50.0092 42.5007) (end 50.0037 42.5027) (layer Edge.Cuts) (width 0.1))
  (gr_text JLCJLCJLCJLC (at 128.750009 100.250001) (layer B.SilkS))
  (gr_text N (at 136.750009 109.500001 90) (layer F.SilkS))
  (gr_text L (at 136.750009 119.500001 90) (layer F.SilkS))
  (dimension 43.750029 (width 0.1524) (layer Dwgs.User)
    (gr_text "43.750 mm" (at 120.621214 46.154187 0.06548086236) (layer Dwgs.User))
    (feature1 (pts (xy 142.500009 49.450001) (xy 142.497053 46.863566)))
    (feature2 (pts (xy 98.750009 49.500001) (xy 98.747053 46.913566)))
    (crossbar (pts (xy 98.747723 47.499986) (xy 142.497723 47.449986)))
    (arrow1a (pts (xy 142.497723 47.449986) (xy 141.37189 48.037694)))
    (arrow1b (pts (xy 142.497723 47.449986) (xy 141.37055 46.864853)))
    (arrow2a (pts (xy 98.747723 47.499986) (xy 99.874896 48.085119)))
    (arrow2b (pts (xy 98.747723 47.499986) (xy 99.873556 46.912278)))
  )
  (gr_text JLCJLCJLCJLC (at 80.000001 100.250001) (layer B.SilkS))
  (gr_text N (at 88.000001 109.500001 90) (layer F.SilkS))
  (gr_text L (at 88.000001 119.500001 90) (layer F.SilkS))
  (dimension 43.750029 (width 0.1524) (layer Dwgs.User)
    (gr_text "43.750 mm" (at 71.871206 46.154187 0.06548086236) (layer Dwgs.User))
    (feature1 (pts (xy 93.750001 49.450001) (xy 93.747045 46.863566)))
    (feature2 (pts (xy 50.000001 49.500001) (xy 49.997045 46.913566)))
    (crossbar (pts (xy 49.997715 47.499986) (xy 93.747715 47.449986)))
    (arrow1a (pts (xy 93.747715 47.449986) (xy 92.621882 48.037694)))
    (arrow1b (pts (xy 93.747715 47.449986) (xy 92.620542 46.864853)))
    (arrow2a (pts (xy 49.997715 47.499986) (xy 51.124888 48.085119)))
    (arrow2b (pts (xy 49.997715 47.499986) (xy 51.123548 46.912278)))
  )
  (zone (net 8) (net_name Board_1-LINE) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 84.500001 123.750001) (xy 84.500001 117.400001) (xy 70.000001 117.400001) (xy 64.500001 115.750001) (xy 51.000001 115.750001)
        (xy 51.000001 123.750001)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 90.525001 70.425001) (xy 85.850001 70.425001) (xy 82.525001 70.600001) (xy 79.150001 71.250001) (xy 75.175001 71.250001)
        (xy 65.425001 71.250001) (xy 55.425001 71.250001) (xy 55.450001 81.250001) (xy 82.650001 81.250001) (xy 86.650001 77.250001)
        (xy 86.650001 74.250001) (xy 90.525001 74.250001)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 90.525001 70.425001) (xy 86.225001 70.425001) (xy 86.225001 73.200001) (xy 90.525001 73.200001)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 90.525001 70.425001) (xy 86.250001 70.425001) (xy 86.250001 73.200001) (xy 90.525001 73.200001)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 90.525001 70.425001) (xy 85.850001 70.425001) (xy 82.525001 70.600001) (xy 79.150001 71.250001) (xy 75.175001 71.250001)
        (xy 65.425001 71.250001) (xy 55.425001 71.250001) (xy 55.425001 81.250001) (xy 82.650001 81.250001) (xy 86.650001 77.250001)
        (xy 86.650001 74.250001) (xy 90.525001 74.250001)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 50.000001 81.250001) (xy 63.750001 81.250001) (xy 63.750001 71.250001) (xy 50.000001 71.250001)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 50.000001 81.250001) (xy 63.750001 81.250001) (xy 63.750001 71.250001) (xy 50.000001 71.250001)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 90.525001 67.550001) (xy 85.850001 67.550001) (xy 82.525001 67.375001) (xy 79.150001 66.750001) (xy 71.925001 66.725001)
        (xy 55.400001 66.750001) (xy 55.400001 56.750001) (xy 82.650001 56.750001) (xy 86.650001 60.750001) (xy 86.650001 63.750001)
        (xy 90.525001 63.750001)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 90.525001 67.550001) (xy 85.850001 67.550001) (xy 82.525001 67.375001) (xy 79.150001 66.750001) (xy 55.400001 66.750001)
        (xy 55.400001 56.750001) (xy 82.650001 56.750001) (xy 86.650001 60.750001) (xy 86.650001 63.750001) (xy 90.525001 63.750001)
      )
    )
  )
  (zone (net 9) (net_name Board_1-NEUT) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 64.500001 101.250001) (xy 71.000001 105.250001) (xy 84.500001 105.250001) (xy 84.500001 111.600001) (xy 70.500001 111.600001)
        (xy 64.500001 109.250001) (xy 51.000001 109.250001) (xy 51.000001 101.250001)
      )
    )
  )
  (zone (net 9) (net_name Board_1-NEUT) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 64.500001 101.250001) (xy 71.000001 105.250001) (xy 84.500001 105.250001) (xy 84.500001 111.600001) (xy 70.500001 111.600001)
        (xy 64.500001 109.250001) (xy 51.000001 109.250001) (xy 51.000001 101.250001)
      )
    )
  )
  (zone (net 8) (net_name Board_1-LINE) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 84.500001 123.750001) (xy 84.500001 117.400001) (xy 70.000001 117.400001) (xy 64.500001 115.750001) (xy 51.000001 115.750001)
        (xy 51.000001 123.750001)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 50.000001 66.750001) (xy 63.750001 66.750001) (xy 63.750001 56.750001) (xy 50.000001 56.750001)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 50.000001 66.750001) (xy 63.750001 66.750001) (xy 63.750001 56.750001) (xy 50.000001 56.750001)
      )
    )
  )
  (zone (net 6) (net_name Board_1-Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 93.725001 131.000001) (xy 68.600001 131.000001) (xy 67.725001 125.250001) (xy 85.975001 125.250001) (xy 85.975001 116.350001)
        (xy 72.475001 116.350001) (xy 72.475001 112.650001) (xy 85.975001 112.650001) (xy 85.975001 103.750001) (xy 71.475001 103.750001)
        (xy 64.975001 99.750001) (xy 61.475001 97.600001) (xy 61.475001 96.250001) (xy 50.100001 96.250001) (xy 50.100001 93.050001)
        (xy 61.475001 93.050001) (xy 61.475001 85.250001) (xy 61.475001 81.700001) (xy 82.700001 81.700001) (xy 87.100001 77.450001)
        (xy 87.100001 74.700001) (xy 90.975001 74.700001) (xy 90.975001 69.975001) (xy 86.200001 69.975001) (xy 79.150001 70.750001)
        (xy 69.700001 70.750001) (xy 69.725001 67.200001) (xy 79.150001 67.200001) (xy 86.200001 68.050001) (xy 90.975001 68.000001)
        (xy 90.975001 63.300001) (xy 87.100001 63.300001) (xy 87.100001 60.500001) (xy 82.850001 56.300001) (xy 67.475001 56.300001)
        (xy 67.475001 50.000001) (xy 93.750001 50.000001)
      )
    )
  )
  (zone (net 7) (net_name Board_1-GNDD) (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.154)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 88.500001 96.800001) (xy 69.000001 96.750001) (xy 69.000001 93.500001) (xy 50.100001 93.500001) (xy 50.100001 84.750001)
        (xy 69.000001 84.750001) (xy 88.500001 84.700001)
      )
    )
  )
  (zone (net 7) (net_name Board_1-GNDD) (layer B.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.154)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 88.500001 96.800001) (xy 69.000001 96.750001) (xy 69.000001 84.750001) (xy 88.500001 84.700001)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 90.525001 64.775001) (xy 86.234871 64.775001) (xy 86.234871 67.550001) (xy 90.525001 67.550001)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 90.525001 64.775001) (xy 86.225001 64.775001) (xy 86.225001 67.550001) (xy 90.525001 67.550001)
      )
    )
  )
  (zone (net 6) (net_name Board_1-Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 93.750001 131.000001) (xy 68.600001 131.000001) (xy 67.725001 125.250001) (xy 85.975001 125.250001) (xy 85.975001 116.350001)
        (xy 72.475001 116.350001) (xy 72.475001 112.650001) (xy 85.975001 112.650001) (xy 85.975001 103.750001) (xy 71.475001 103.750001)
        (xy 61.475001 97.600001) (xy 61.475001 96.250001) (xy 50.000001 96.250001) (xy 50.025001 85.250001) (xy 61.500001 85.250001)
        (xy 61.500001 81.700001) (xy 82.700001 81.700001) (xy 87.100001 77.450001) (xy 87.100001 74.700001) (xy 90.975001 74.700001)
        (xy 90.975001 69.975001) (xy 86.200001 69.975001) (xy 79.150001 70.750001) (xy 69.725001 70.750001) (xy 69.750001 67.200001)
        (xy 79.150001 67.200001) (xy 86.200001 68.050001) (xy 90.975001 68.000001) (xy 90.975001 63.300001) (xy 87.100001 63.300001)
        (xy 87.100001 60.500001) (xy 82.850001 56.300001) (xy 67.500001 56.325001) (xy 67.500001 50.000001) (xy 93.750001 50.000001)
      )
    )
  )
  (zone (net 6) (net_name Board_1-Earth) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 50.000001 96.250001) (xy 56.500001 96.250001) (xy 56.500001 85.250001) (xy 50.000001 85.250001)
      )
    )
  )
  (zone (net 17) (net_name Board_2-LINE) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 133.250009 123.750001) (xy 133.250009 117.400001) (xy 118.750009 117.400001) (xy 113.250009 115.750001) (xy 99.750009 115.750001)
        (xy 99.750009 123.750001)
      )
    )
  )
  (zone (net 12) (net_name Board_2-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 139.275009 70.425001) (xy 134.600009 70.425001) (xy 131.275009 70.600001) (xy 127.900009 71.250001) (xy 123.925009 71.250001)
        (xy 114.175009 71.250001) (xy 104.175009 71.250001) (xy 104.200009 81.250001) (xy 131.400009 81.250001) (xy 135.400009 77.250001)
        (xy 135.400009 74.250001) (xy 139.275009 74.250001)
      )
    )
  )
  (zone (net 12) (net_name Board_2-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 139.275009 70.425001) (xy 134.975009 70.425001) (xy 134.975009 73.200001) (xy 139.275009 73.200001)
      )
    )
  )
  (zone (net 12) (net_name Board_2-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 139.275009 70.425001) (xy 135.000009 70.425001) (xy 135.000009 73.200001) (xy 139.275009 73.200001)
      )
    )
  )
  (zone (net 12) (net_name Board_2-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 139.275009 70.425001) (xy 134.600009 70.425001) (xy 131.275009 70.600001) (xy 127.900009 71.250001) (xy 123.925009 71.250001)
        (xy 114.175009 71.250001) (xy 104.175009 71.250001) (xy 104.175009 81.250001) (xy 131.400009 81.250001) (xy 135.400009 77.250001)
        (xy 135.400009 74.250001) (xy 139.275009 74.250001)
      )
    )
  )
  (zone (net 12) (net_name Board_2-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 98.750009 81.250001) (xy 112.500009 81.250001) (xy 112.500009 71.250001) (xy 98.750009 71.250001)
      )
    )
  )
  (zone (net 12) (net_name Board_2-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 98.750009 81.250001) (xy 112.500009 81.250001) (xy 112.500009 71.250001) (xy 98.750009 71.250001)
      )
    )
  )
  (zone (net 13) (net_name Board_2-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 139.275009 67.550001) (xy 134.600009 67.550001) (xy 131.275009 67.375001) (xy 127.900009 66.750001) (xy 120.675009 66.725001)
        (xy 104.150009 66.750001) (xy 104.150009 56.750001) (xy 131.400009 56.750001) (xy 135.400009 60.750001) (xy 135.400009 63.750001)
        (xy 139.275009 63.750001)
      )
    )
  )
  (zone (net 13) (net_name Board_2-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 139.275009 67.550001) (xy 134.600009 67.550001) (xy 131.275009 67.375001) (xy 127.900009 66.750001) (xy 104.150009 66.750001)
        (xy 104.150009 56.750001) (xy 131.400009 56.750001) (xy 135.400009 60.750001) (xy 135.400009 63.750001) (xy 139.275009 63.750001)
      )
    )
  )
  (zone (net 18) (net_name Board_2-NEUT) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 113.250009 101.250001) (xy 119.750009 105.250001) (xy 133.250009 105.250001) (xy 133.250009 111.600001) (xy 119.250009 111.600001)
        (xy 113.250009 109.250001) (xy 99.750009 109.250001) (xy 99.750009 101.250001)
      )
    )
  )
  (zone (net 18) (net_name Board_2-NEUT) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 113.250009 101.250001) (xy 119.750009 105.250001) (xy 133.250009 105.250001) (xy 133.250009 111.600001) (xy 119.250009 111.600001)
        (xy 113.250009 109.250001) (xy 99.750009 109.250001) (xy 99.750009 101.250001)
      )
    )
  )
  (zone (net 17) (net_name Board_2-LINE) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 133.250009 123.750001) (xy 133.250009 117.400001) (xy 118.750009 117.400001) (xy 113.250009 115.750001) (xy 99.750009 115.750001)
        (xy 99.750009 123.750001)
      )
    )
  )
  (zone (net 13) (net_name Board_2-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 98.750009 66.750001) (xy 112.500009 66.750001) (xy 112.500009 56.750001) (xy 98.750009 56.750001)
      )
    )
  )
  (zone (net 13) (net_name Board_2-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 98.750009 66.750001) (xy 112.500009 66.750001) (xy 112.500009 56.750001) (xy 98.750009 56.750001)
      )
    )
  )
  (zone (net 15) (net_name Board_2-Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 142.475009 131.000001) (xy 117.350009 131.000001) (xy 116.475009 125.250001) (xy 134.725009 125.250001) (xy 134.725009 116.350001)
        (xy 121.225009 116.350001) (xy 121.225009 112.650001) (xy 134.725009 112.650001) (xy 134.725009 103.750001) (xy 120.225009 103.750001)
        (xy 113.725009 99.750001) (xy 110.225009 97.600001) (xy 110.225009 96.250001) (xy 98.850009 96.250001) (xy 98.850009 93.050001)
        (xy 110.225009 93.050001) (xy 110.225009 85.250001) (xy 110.225009 81.700001) (xy 131.450009 81.700001) (xy 135.850009 77.450001)
        (xy 135.850009 74.700001) (xy 139.725009 74.700001) (xy 139.725009 69.975001) (xy 134.950009 69.975001) (xy 127.900009 70.750001)
        (xy 118.450009 70.750001) (xy 118.475009 67.200001) (xy 127.900009 67.200001) (xy 134.950009 68.050001) (xy 139.725009 68.000001)
        (xy 139.725009 63.300001) (xy 135.850009 63.300001) (xy 135.850009 60.500001) (xy 131.600009 56.300001) (xy 116.225009 56.300001)
        (xy 116.225009 50.000001) (xy 142.500009 50.000001)
      )
    )
  )
  (zone (net 16) (net_name Board_2-GNDD) (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.154)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 137.250009 96.800001) (xy 117.750009 96.750001) (xy 117.750009 93.500001) (xy 98.850009 93.500001) (xy 98.850009 84.750001)
        (xy 117.750009 84.750001) (xy 137.250009 84.700001)
      )
    )
  )
  (zone (net 16) (net_name Board_2-GNDD) (layer B.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.154)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 137.250009 96.800001) (xy 117.750009 96.750001) (xy 117.750009 84.750001) (xy 137.250009 84.700001)
      )
    )
  )
  (zone (net 13) (net_name Board_2-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 139.275009 64.775001) (xy 134.984879 64.775001) (xy 134.984879 67.550001) (xy 139.275009 67.550001)
      )
    )
  )
  (zone (net 13) (net_name Board_2-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 139.275009 64.775001) (xy 134.975009 64.775001) (xy 134.975009 67.550001) (xy 139.275009 67.550001)
      )
    )
  )
  (zone (net 15) (net_name Board_2-Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 142.500009 131.000001) (xy 117.350009 131.000001) (xy 116.475009 125.250001) (xy 134.725009 125.250001) (xy 134.725009 116.350001)
        (xy 121.225009 116.350001) (xy 121.225009 112.650001) (xy 134.725009 112.650001) (xy 134.725009 103.750001) (xy 120.225009 103.750001)
        (xy 110.225009 97.600001) (xy 110.225009 96.250001) (xy 98.750009 96.250001) (xy 98.775009 85.250001) (xy 110.250009 85.250001)
        (xy 110.250009 81.700001) (xy 131.450009 81.700001) (xy 135.850009 77.450001) (xy 135.850009 74.700001) (xy 139.725009 74.700001)
        (xy 139.725009 69.975001) (xy 134.950009 69.975001) (xy 127.900009 70.750001) (xy 118.475009 70.750001) (xy 118.500009 67.200001)
        (xy 127.900009 67.200001) (xy 134.950009 68.050001) (xy 139.725009 68.000001) (xy 139.725009 63.300001) (xy 135.850009 63.300001)
        (xy 135.850009 60.500001) (xy 131.600009 56.300001) (xy 116.250009 56.325001) (xy 116.250009 50.000001) (xy 142.500009 50.000001)
      )
    )
  )
  (zone (net 15) (net_name Board_2-Earth) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 98.750009 96.250001) (xy 105.250009 96.250001) (xy 105.250009 85.250001) (xy 98.750009 85.250001)
      )
    )
  )
)
