(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 211)
    (tracks 142)
    (zones 0)
    (modules 17)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.4)
    (user_via 0.9 0.4)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.05)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 0.8128 0.8128)
    (mod_text_width 0.1524)
    (pad_size 2.2 1.7)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-/CAN+)
  (net 2 Board_1-/CAN-)
  (net 3 Board_1-/VBUS+)
  (net 4 Board_1-/VBUS-)
  (net 5 Board_1-/VCCD)
  (net 6 Board_1-Earth)
  (net 7 Board_1-GNDD)
  (net 8 Board_1-LINE)
  (net 9 Board_1-NEUT)
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-/CAN+)
    (add_net Board_1-/CAN-)
    (add_net Board_1-/VBUS+)
    (add_net Board_1-/VBUS-)
    (add_net Board_1-/VCCD)
    (add_net Board_1-Earth)
    (add_net Board_1-GNDD)
    (add_net Board_1-LINE)
    (add_net Board_1-NEUT)
  )
  (net_class CANBUS ""
    (clearance 0.154)
    (trace_width 0.154)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class PWR_AC ""
    (clearance 1)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class PWR_DC ""
    (clearance 0.5)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class PWR_IO ""
    (clearance 0.154)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 144.625 98 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.55 90) (layer F.SilkS))
    (fp_text value 120R (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 Board_1-/CAN-))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Phoenix_MC:PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal (layer F.Cu) (tedit 5B784ED0)
    (at 163.625 103.75 90)
    (descr "Generic Phoenix Contact connector footprint for: MC_1,5/3-G-3.5; number of pins: 03; pin pitch: 3.50mm; Angled || order number: 1844223 8A 160V")
    (tags "phoenix_contact connector MC_01x03_G_3.5mm")
    (fp_text reference JB2 (at 3.5 3.4 270) (layer F.SilkS))
    (fp_text value CANBUS (at 3.5 9.2 90) (layer F.Fab))
    (fp_text user %R (at 3.5 -0.5 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 7 Board_1-GNDD))
    (pad 2 thru_hole oval (at 3.5 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Board_1-/CAN-))
    (pad 3 thru_hole oval (at 7 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/PhoenixContact_MC_1,5_3-G-3.5_1x03_P3.50mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm (layer F.Cu) (tedit 5B391E66)
    (at 150.625 92.475 270)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 1.6 90) (layer F.SilkS))
    (fp_text value CTRL_VBUS+ (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 3 Board_1-/VBUS+) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy 0 0.75)) (width 0))
      ))
    (pad 2 smd custom (at 0.65 0 270) (size 1 0.5) (layers F.Cu F.Mask)
      (net 5 Board_1-/VCCD) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0))
        (gr_poly (pts
           (xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)) (width 0))
      ))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 149.375 137.75)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H1 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 149.375 62.25)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H3 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 169.125 62.25)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H4 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5_ISO7380_Pad_TopBottom (layer F.Cu) (tedit 56D1B4CB)
    (at 169.125 137.75)
    (descr "Mounting Hole 2.7mm, M2.5, ISO7380")
    (tags "mounting hole 2.7mm m2.5 iso7380")
    (attr virtual)
    (fp_text reference H2 (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value M3 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.1 3.1) (drill 2.7) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers F.Cu F.Mask)
      (net 6 Board_1-Earth))
    (pad 1 connect circle (at 0 0) (size 4.5 4.5) (layers B.Cu B.Mask)
      (net 6 Board_1-Earth))
  )
  (module "1 My Footprints:TerminalBlock_WAGO_236-103_1x03_P5.00mm_PadsOnly" (layer F.Cu) (tedit 601D1331)
    (at 159.375 129 90)
    (descr "Terminal Block WAGO 236-103, 45Degree (cable under 45degree), 3 pins, pitch 5mm, size 17.3x14mm^2, drill diamater 1.15mm, pad diameter 3mm, see , script-generated with , script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_WAGO")
    (tags "THT Terminal Block WAGO 236-103 45Degree pitch 5mm size 17.3x14mm^2 drill 1.15mm pad 3mm")
    (fp_text reference JB1 (at 5 2.65 90) (layer F.SilkS))
    (fp_text value AC_IN (at 5.15 10.12 90) (layer F.Fab))
    (fp_text user %R (at 5.15 1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 8 Board_1-LINE))
    (pad 2 thru_hole oval (at 5 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 3 thru_hole oval (at 10 0 90) (size 1.5 3) (drill 1.15) (layers *.Cu *.Mask)
      (net 9 Board_1-NEUT))
    (model ${KIPRJMOD}/shapes3D/TerminalBlock_WAGO_236-103_1x03_P5.00mm_45Degree.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:1605540000" (layer F.Cu) (tedit 602379B0)
    (at 154.375 129.08 90)
    (fp_text reference JA1 (at 5.08 -4.75 90) (layer F.SilkS))
    (fp_text value AC_IN (at 5.05 4.85 90) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask) (roundrect_rratio 0.120192)
      (net 8 Board_1-LINE))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 Board_1-NEUT))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (model ${KIPRJMOD}/shapes3D/1605540000.stp
      (offset (xyz -3.54 -9.5 -3.2))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EltekFlatpack2:Amass_XT60PW-M_Kombifootprint (layer F.Cu) (tedit 60237AFA)
    (at 161.175 78.5 270)
    (fp_text reference JC3 (at 0 0.75 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 1 90) (layer F.Fab) hide)
    (pad 2 thru_hole custom (at 3.6 0 270) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.949 0.127) (xy -2.10902 -3.1877) (xy -1.5045 -4.064) (xy -0.552 -4.064) (xy -0.19894 -3.75158)
           (xy 1.44698 -1.30556)) (width 0.1))
        (gr_poly (pts
           (xy -2.11664 -3.175) (xy -2.11664 -7.4295) (xy -0.2345 -7.4295) (xy -0.2345 -3.175)) (width 0.1))
      ))
    (pad 1 thru_hole custom (at -3.6 0 270) (size 4 4) (drill 2.7) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -1.861 0) (xy 1.949 0) (xy 2.10394 -3.14706) (xy 1.695 -3.937) (xy 1.441 -4.064)
           (xy 0.1075 -3.6195) (xy -1.734 -0.889)) (width 0.1))
        (gr_poly (pts
           (xy 0.21786 -3.175) (xy 0.21786 -7.4295) (xy 2.1 -7.4295) (xy 2.1 -3.175)) (width 0.1))
      ))
    (pad 2 thru_hole circle (at 2.54 -3.175 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.54 -3.175 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-) (zone_connect 2))
    (pad MP thru_hole oval (at -6.75 -6 270) (size 1.6 2.8) (drill oval 0.8 1.8) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad MP thru_hole oval (at 6.75 -6 270) (size 1.6 2.8) (drill oval 0.8 1.8) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
  )
  (module "1 My Footprints:Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Combi_3D-V" (layer F.Cu) (tedit 6023867E)
    (at 150.625 96.5)
    (descr "Molex Nano-Fit Power Connectors, 105309-xx04, 4 Pins per row (http://www.molex.com/pdm_docs/sd/1053091203_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Nano-Fit side entry")
    (fp_text reference JA2 (at -3 3.75 90) (layer F.SilkS))
    (fp_text value CTRL (at 0 10.42) (layer F.Fab))
    (pad 1 thru_hole roundrect (at 0 0) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.147059)
      (net 5 Board_1-/VCCD))
    (pad 2 thru_hole oval (at 0 2.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 Board_1-/CAN+))
    (pad 3 thru_hole oval (at 0 5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 Board_1-/CAN-))
    (pad 4 thru_hole oval (at 0 7.5) (size 2.2 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 7 Board_1-GNDD))
    (pad "" np_thru_hole circle (at -1.34 3.75) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.18 0) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.18 7.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105309-xx04_1x04_P2.50mm_Vertical.step
      (offset (xyz 0 -3.75 4.85))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model ${KIPRJMOD}/shapes3D/Molex_Nano-Fit_105313-xx04_1x04_P2.50mm_Horizontal.step
      (offset (xyz 6.15 -3.75 2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 -90))
    )
  )
  (module EltekFlatpack2:CON_Edge_Flatpack2_AllContacts locked (layer F.Cu) (tedit 6023AC13)
    (at 128.125 65.75)
    (fp_text reference PC1 (at 6 13.75) (layer F.SilkS) hide)
    (fp_text value Flatpack2 (at 6 14.75) (layer F.Fab))
    (fp_text user H (at 12.675 31 90 unlocked) (layer F.SilkS))
    (fp_text user L (at 12.675 33.5 90 unlocked) (layer F.SilkS))
    (pad DC-POS smd roundrect (at 11.5 20) (size 5 8.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 3 Board_1-/VBUS+) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 11.5 5.5) (size 5 8.5) (layers B.Cu) (roundrect_rratio 0.1)
      (net 4 Board_1-/VBUS-) (solder_mask_margin 0.1016))
    (pad DC-POS smd roundrect (at 5.05 20) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 3 Board_1-/VBUS+) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 5.05 5.5) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 4 Board_1-/VBUS-) (solder_mask_margin 0.1016))
    (pad AC-N smd roundrect (at 5.05 49) (size 9.9 8) (layers B.Cu B.Mask) (roundrect_rratio 0.062)
      (net 9 Board_1-NEUT) (solder_mask_margin 0.1016))
    (pad AC-L smd roundrect (at 5.05 63.5) (size 9.9 8) (layers B.Cu B.Mask) (roundrect_rratio 0.062)
      (net 8 Board_1-LINE) (solder_mask_margin 0.1016))
    (pad AC-N smd roundrect (at 5.05 49) (size 9.9 8) (layers F.Cu F.Mask) (roundrect_rratio 0.062)
      (net 9 Board_1-NEUT) (solder_mask_margin 0.1016))
    (pad AC-L smd roundrect (at 5.05 63.5) (size 9.9 8) (layers F.Cu F.Mask) (roundrect_rratio 0.062)
      (net 8 Board_1-LINE) (solder_mask_margin 0.1016))
    (pad GNDD smd roundrect (at 5.05 36) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 7 Board_1-GNDD) (solder_mask_margin 0.1016))
    (pad DC-POS smd roundrect (at 7.05 20) (size 13.9 8.5) (layers F.Cu F.Mask) (roundrect_rratio 0.059)
      (net 3 Board_1-/VBUS+) (solder_mask_margin 0.1016))
    (pad AC-E smd roundrect (at 5.05 34.5) (size 9.9 8.5) (layers B.Cu B.Mask) (roundrect_rratio 0.059)
      (net 6 Board_1-Earth) (solder_mask_margin 0.1016))
    (pad DC-NEG smd roundrect (at 7.05 5.5) (size 13.9 8.5) (layers F.Cu F.Mask) (roundrect_rratio 0.059)
      (net 4 Board_1-/VBUS-) (solder_mask_margin 0.1016))
    (pad CAN-H smd roundrect (at 5.05 31) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 1 Board_1-/CAN+) (solder_mask_margin 0.1016))
    (pad CAN-L smd roundrect (at 5.05 33.5) (size 9.9 1.5) (layers F.Cu F.Mask) (roundrect_rratio 0.167)
      (net 2 Board_1-/CAN-) (solder_mask_margin 0.1016))
  )
  (module Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 144.625 100.55 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 2.54 -1.92 90) (layer F.SilkS) hide)
    (fp_text value 120R (at 2.54 1.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 Board_1-/CAN-))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 Board_1-/CAN+))
    (model ${KIPRJMOD}/shapes3D/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:Connector_Keystone_4912_Overlaid" locked (layer F.Cu) (tedit 603C8B9E)
    (at 153.575 86.74 90)
    (fp_text reference T1 (at -3.175 -2.54 270) (layer F.Fab))
    (fp_text value "Keystone 4912" (at 0 5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 1 thru_hole circle (at -2.54 2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
  )
  (module "1 My Footprints:Connector_Keystone_4912_Overlaid" locked (layer F.Cu) (tedit 603C8BCB)
    (at 153.575 70.25 90)
    (fp_text reference T2 (at -3.175 -2.54 270) (layer F.Fab))
    (fp_text value "Keystone 4912" (at 0 5.715 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 1 thru_hole circle (at 2.54 2.54 90) (size 2 2) (drill 1.32) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
  )
  (module SnapEDA-zip:TE_2204535-1 locked (layer F.Cu) (tedit 603C8BDE)
    (at 160.425 78.5 90)
    (fp_text reference JB3 (at 3.325 -3.15 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 5 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.7 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 4 thru_hole circle (at -5.7 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 2 thru_hole circle (at 0 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 5 thru_hole circle (at 0 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 3 thru_hole circle (at 5.7 -2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 6 thru_hole circle (at 5.7 -8.05 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad "" np_thru_hole circle (at -7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -5.7 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 2 thru_hole circle (at 0 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 3 thru_hole circle (at 5.7 -4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 4 thru_hole circle (at -5.7 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 5 thru_hole circle (at 0 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 6 thru_hole circle (at 5.7 -10.35 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (model ${KIPRJMOD}/shapes3D/TE_2204535-1.stp
      (offset (xyz 0 -9.949999999999999 10.7))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:TE_2204529-1" (layer F.Cu) (tedit 603C8C5D)
    (at 154.375 78.5 270)
    (fp_text reference JA3 (at -3.4 3.15 90) (layer F.SilkS) hide)
    (fp_text value "DC OUT" (at 0 -0.45 270) (layer F.Fab))
    (pad "" np_thru_hole circle (at 7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 5.7 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
    (pad 3 thru_hole circle (at -5.7 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 2 thru_hole circle (at 0 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad 2 thru_hole circle (at 0 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 6 Board_1-Earth))
    (pad "" np_thru_hole circle (at -7.96 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at -5.7 2 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 4 Board_1-/VBUS-))
    (pad 1 thru_hole circle (at 5.7 4.3 90) (size 2.46 2.46) (drill 1.64) (layers *.Cu *.Mask)
      (net 3 Board_1-/VBUS+))
  )
  (gr_line (start 145.7294 134.2565) (end 145.625 134.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.8327 134.2728) (end 145.7294 134.2565) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.9337 134.2999) (end 145.8327 134.2728) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.0313 134.3374) (end 145.9337 134.2999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.1245 134.3848) (end 146.0313 134.3374) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.2122 134.4418) (end 146.1245 134.3848) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.2935 134.5076) (end 146.2122 134.4418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.3674 134.5815) (end 146.2935 134.5076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4332 134.6628) (end 146.3674 134.5815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4902 134.7505) (end 146.4332 134.6628) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.5376 134.8437) (end 146.4902 134.7505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.5751 134.9413) (end 146.5376 134.8437) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6022 135.0423) (end 146.5751 134.9413) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6185 135.1456) (end 146.6022 135.0423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.624 135.25) (end 146.6185 135.1456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.624 138.5001) (end 146.624 135.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.635 138.7092) (end 146.624 138.5001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6677 138.916) (end 146.635 138.7092) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7219 139.1183) (end 146.6677 138.916) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.797 139.3138) (end 146.7219 139.1183) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8921 139.5005) (end 146.797 139.3138) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.0061 139.6761) (end 146.8921 139.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.1379 139.8389) (end 147.0061 139.6761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.2861 139.9871) (end 147.1379 139.8389) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.4489 140.1189) (end 147.2861 139.9871) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.6245 140.2329) (end 147.4489 140.1189) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8111 140.328) (end 147.6245 140.2329) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.0067 140.4031) (end 147.8111 140.328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.209 140.4573) (end 148.0067 140.4031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4159 140.49) (end 148.209 140.4573) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.625 140.501) (end 148.4159 140.49) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.875 140.501) (end 148.625 140.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.0841 140.49) (end 169.875 140.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.2911 140.4573) (end 170.0841 140.49) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.4933 140.4031) (end 170.2911 140.4573) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.6888 140.328) (end 170.4933 140.4031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.8755 140.2329) (end 170.6888 140.328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.0512 140.1188) (end 170.8755 140.2329) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2139 139.9871) (end 171.0512 140.1188) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.362 139.839) (end 171.2139 139.9871) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4939 139.6761) (end 171.362 139.839) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.6079 139.5005) (end 171.4939 139.6761) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.703 139.3139) (end 171.6079 139.5005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.778 139.1184) (end 171.703 139.3139) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.8323 138.916) (end 171.778 139.1184) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.865 138.7091) (end 171.8323 138.916) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.876 138.5) (end 171.865 138.7091) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.876 61.5) (end 171.876 138.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.865 61.2908) (end 171.876 61.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.8323 61.084) (end 171.865 61.2908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.7781 60.8817) (end 171.8323 61.084) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.703 60.6861) (end 171.7781 60.8817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.6079 60.4995) (end 171.703 60.6861) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.4939 60.3239) (end 171.6079 60.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.362 60.161) (end 171.4939 60.3239) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.2139 60.0129) (end 171.362 60.161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.0512 59.8812) (end 171.2139 60.0129) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.8755 59.7671) (end 171.0512 59.8812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.6888 59.672) (end 170.8755 59.7671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.4934 59.597) (end 170.6888 59.672) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.291 59.5427) (end 170.4934 59.597) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.0841 59.51) (end 170.291 59.5427) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.875 59.499) (end 170.0841 59.51) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.625 59.499) (end 169.875 59.499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.4158 59.51) (end 148.625 59.499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.209 59.5427) (end 148.4158 59.51) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.0067 59.5969) (end 148.209 59.5427) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8112 59.672) (end 148.0067 59.5969) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.6245 59.7671) (end 147.8112 59.672) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.4488 59.8812) (end 147.6245 59.7671) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.286 60.013) (end 147.4488 59.8812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.1379 60.1611) (end 147.286 60.013) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.0062 60.3238) (end 147.1379 60.1611) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8921 60.4995) (end 147.0062 60.3238) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.797 60.6862) (end 146.8921 60.4995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7219 60.8817) (end 146.797 60.6862) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6677 61.084) (end 146.7219 60.8817) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.635 61.2908) (end 146.6677 61.084) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.624 61.4999) (end 146.635 61.2908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.624 64.75) (end 146.624 61.4999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6185 64.8544) (end 146.624 64.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6022 64.9577) (end 146.6185 64.8544) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.5751 65.0587) (end 146.6022 64.9577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.5376 65.1563) (end 146.5751 65.0587) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4902 65.2495) (end 146.5376 65.1563) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4332 65.3372) (end 146.4902 65.2495) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.3674 65.4185) (end 146.4332 65.3372) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.2935 65.4924) (end 146.3674 65.4185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.2122 65.5582) (end 146.2935 65.4924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.1245 65.6152) (end 146.2122 65.5582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.0313 65.6626) (end 146.1245 65.6152) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.9337 65.7001) (end 146.0313 65.6626) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.8327 65.7272) (end 145.9337 65.7001) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.7294 65.7435) (end 145.8327 65.7272) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.625 65.749) (end 145.7294 65.7435) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.625 65.749) (end 145.625 65.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5726 65.7518) (end 128.625 65.749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5209 65.7599) (end 128.5726 65.7518) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4702 65.7735) (end 128.5209 65.7599) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4212 65.7923) (end 128.4702 65.7735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3745 65.8161) (end 128.4212 65.7923) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3306 65.8447) (end 128.3745 65.8161) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2897 65.8777) (end 128.3306 65.8447) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2527 65.9148) (end 128.2897 65.8777) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2197 65.9555) (end 128.2527 65.9148) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1911 65.9995) (end 128.2197 65.9555) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1673 66.0462) (end 128.1911 65.9995) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1485 66.0951) (end 128.1673 66.0462) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1349 66.1459) (end 128.1485 66.0951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1267 66.1977) (end 128.1349 66.1459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.124 66.25) (end 128.1267 66.1977) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.124 76) (end 128.124 66.25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1267 76.0523) (end 128.124 76) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1349 76.1041) (end 128.1267 76.0523) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1485 76.1548) (end 128.1349 76.1041) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1673 76.2037) (end 128.1485 76.1548) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1911 76.2505) (end 128.1673 76.2037) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2197 76.2944) (end 128.1911 76.2505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2527 76.3352) (end 128.2197 76.2944) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2897 76.3723) (end 128.2527 76.3352) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3306 76.4053) (end 128.2897 76.3723) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3745 76.4339) (end 128.3306 76.4053) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4213 76.4577) (end 128.3745 76.4339) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4702 76.4765) (end 128.4213 76.4577) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5209 76.4901) (end 128.4702 76.4765) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5727 76.4983) (end 128.5209 76.4901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.625 76.501) (end 128.5727 76.4983) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.625 76.501) (end 128.625 76.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.7261 76.5061) (end 138.625 76.501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.8261 76.5215) (end 138.7261 76.5061) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.9241 76.5468) (end 138.8261 76.5215) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.019 76.582) (end 138.9241 76.5468) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.1098 76.6265) (end 139.019 76.582) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.1957 76.6801) (end 139.1098 76.6265) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.2757 76.742) (end 139.1957 76.6801) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.3491 76.8117) (end 139.2757 76.742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.415 76.8885) (end 139.3491 76.8117) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.4728 76.9716) (end 139.415 76.8885) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5219 77.06) (end 139.4728 76.9716) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5618 77.153) (end 139.5219 77.06) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5921 77.2496) (end 139.5618 77.153) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.6125 77.3487) (end 139.5921 77.2496) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.6227 77.4494) (end 139.6125 77.3487) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.6227 77.5506) (end 139.6227 77.4494) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.6125 77.6513) (end 139.6227 77.5506) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5921 77.7504) (end 139.6125 77.6513) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5618 77.847) (end 139.5921 77.7504) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.5219 77.94) (end 139.5618 77.847) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.4728 78.0284) (end 139.5219 77.94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.415 78.1115) (end 139.4728 78.0284) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.3491 78.1883) (end 139.415 78.1115) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.2757 78.258) (end 139.3491 78.1883) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.1957 78.3199) (end 139.2757 78.258) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.1098 78.3735) (end 139.1957 78.3199) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.019 78.418) (end 139.1098 78.3735) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.9241 78.4532) (end 139.019 78.418) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.8261 78.4785) (end 138.9241 78.4532) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.7261 78.4939) (end 138.8261 78.4785) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.625 78.499) (end 138.7261 78.4939) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.6249 78.499) (end 138.625 78.499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5727 78.5017) (end 128.6249 78.499) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5209 78.5099) (end 128.5727 78.5017) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4701 78.5235) (end 128.5209 78.5099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4212 78.5423) (end 128.4701 78.5235) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3745 78.5661) (end 128.4212 78.5423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3305 78.5947) (end 128.3745 78.5661) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2898 78.6277) (end 128.3305 78.5947) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2527 78.6648) (end 128.2898 78.6277) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2197 78.7055) (end 128.2527 78.6648) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1911 78.7495) (end 128.2197 78.7055) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1673 78.7963) (end 128.1911 78.7495) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1485 78.8452) (end 128.1673 78.7963) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1349 78.8959) (end 128.1485 78.8452) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1267 78.9477) (end 128.1349 78.8959) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.124 79) (end 128.1267 78.9477) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.124 133.75) (end 128.124 79) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1268 133.8024) (end 128.124 133.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.135 133.8542) (end 128.1268 133.8024) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1485 133.9048) (end 128.135 133.8542) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1673 133.9537) (end 128.1485 133.9048) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.1911 134.0005) (end 128.1673 133.9537) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2197 134.0444) (end 128.1911 134.0005) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2527 134.0853) (end 128.2197 134.0444) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.2898 134.1223) (end 128.2527 134.0853) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3305 134.1553) (end 128.2898 134.1223) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.3745 134.1839) (end 128.3305 134.1553) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4213 134.2077) (end 128.3745 134.1839) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4701 134.2265) (end 128.4213 134.2077) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5209 134.2401) (end 128.4701 134.2265) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.5727 134.2483) (end 128.5209 134.2401) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.625 134.251) (end 128.5727 134.2483) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.625 134.251) (end 128.625 134.251) (layer Edge.Cuts) (width 0.1))
  (gr_text JLCJLCJLCJLC (at 158.125 109.75) (layer B.SilkS))
  (gr_text N (at 166.125 119 90) (layer F.SilkS))
  (gr_text L (at 166.125 129 90) (layer F.SilkS))
  (zone (net 8) (net_name Board_1-LINE) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 162.625 133.25) (xy 162.625 126.9) (xy 148.125 126.9) (xy 142.625 125.25) (xy 129.125 125.25)
        (xy 129.125 133.25)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 168.65 79.925) (xy 163.975 79.925) (xy 160.65 80.1) (xy 157.275 80.75) (xy 153.3 80.75)
        (xy 143.55 80.75) (xy 133.55 80.75) (xy 133.575 90.75) (xy 160.775 90.75) (xy 164.775 86.75)
        (xy 164.775 83.75) (xy 168.65 83.75)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 168.65 79.925) (xy 164.35 79.925) (xy 164.35 82.7) (xy 168.65 82.7)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 168.65 79.925) (xy 164.375 79.925) (xy 164.375 82.7) (xy 168.65 82.7)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 168.65 79.925) (xy 163.975 79.925) (xy 160.65 80.1) (xy 157.275 80.75) (xy 153.3 80.75)
        (xy 143.55 80.75) (xy 133.55 80.75) (xy 133.55 90.75) (xy 160.775 90.75) (xy 164.775 86.75)
        (xy 164.775 83.75) (xy 168.65 83.75)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 128.125 90.75) (xy 141.875 90.75) (xy 141.875 80.75) (xy 128.125 80.75)
      )
    )
  )
  (zone (net 3) (net_name Board_1-/VBUS+) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 128.125 90.75) (xy 141.875 90.75) (xy 141.875 80.75) (xy 128.125 80.75)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 168.65 77.05) (xy 163.975 77.05) (xy 160.65 76.875) (xy 157.275 76.25) (xy 150.05 76.225)
        (xy 133.525 76.25) (xy 133.525 66.25) (xy 160.775 66.25) (xy 164.775 70.25) (xy 164.775 73.25)
        (xy 168.65 73.25)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 168.65 77.05) (xy 163.975 77.05) (xy 160.65 76.875) (xy 157.275 76.25) (xy 133.525 76.25)
        (xy 133.525 66.25) (xy 160.775 66.25) (xy 164.775 70.25) (xy 164.775 73.25) (xy 168.65 73.25)
      )
    )
  )
  (zone (net 9) (net_name Board_1-NEUT) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 142.625 110.75) (xy 149.125 114.75) (xy 162.625 114.75) (xy 162.625 121.1) (xy 148.625 121.1)
        (xy 142.625 118.75) (xy 129.125 118.75) (xy 129.125 110.75)
      )
    )
  )
  (zone (net 9) (net_name Board_1-NEUT) (layer F.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 142.625 110.75) (xy 149.125 114.75) (xy 162.625 114.75) (xy 162.625 121.1) (xy 148.625 121.1)
        (xy 142.625 118.75) (xy 129.125 118.75) (xy 129.125 110.75)
      )
    )
  )
  (zone (net 8) (net_name Board_1-LINE) (layer B.Cu) (hatch edge 0.508)
    (priority 5)
    (connect_pads yes (clearance 1))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 162.625 133.25) (xy 162.625 126.9) (xy 148.125 126.9) (xy 142.625 125.25) (xy 129.125 125.25)
        (xy 129.125 133.25)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 128.125 76.25) (xy 141.875 76.25) (xy 141.875 66.25) (xy 128.125 66.25)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 128.125 76.25) (xy 141.875 76.25) (xy 141.875 66.25) (xy 128.125 66.25)
      )
    )
  )
  (zone (net 6) (net_name Board_1-Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 171.85 140.5) (xy 146.725 140.5) (xy 145.85 134.75) (xy 164.1 134.75) (xy 164.1 125.85)
        (xy 150.6 125.85) (xy 150.6 122.15) (xy 164.1 122.15) (xy 164.1 113.25) (xy 149.6 113.25)
        (xy 143.1 109.25) (xy 139.6 107.1) (xy 139.6 105.75) (xy 128.225 105.75) (xy 128.225 102.55)
        (xy 139.6 102.55) (xy 139.6 94.75) (xy 139.6 91.2) (xy 160.825 91.2) (xy 165.225 86.95)
        (xy 165.225 84.2) (xy 169.1 84.2) (xy 169.1 79.475) (xy 164.325 79.475) (xy 157.275 80.25)
        (xy 147.825 80.25) (xy 147.85 76.7) (xy 157.275 76.7) (xy 164.325 77.55) (xy 169.1 77.5)
        (xy 169.1 72.8) (xy 165.225 72.8) (xy 165.225 70) (xy 160.975 65.8) (xy 145.6 65.8)
        (xy 145.6 59.5) (xy 171.875 59.5)
      )
    )
  )
  (zone (net 7) (net_name Board_1-GNDD) (layer F.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.154)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 166.625 106.3) (xy 147.125 106.25) (xy 147.125 103) (xy 128.225 103) (xy 128.225 94.25)
        (xy 147.125 94.25) (xy 166.625 94.2)
      )
    )
  )
  (zone (net 7) (net_name Board_1-GNDD) (layer B.Cu) (hatch edge 0.508)
    (priority 7)
    (connect_pads thru_hole_only (clearance 0.2))
    (min_thickness 0.154)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 166.625 106.3) (xy 147.125 106.25) (xy 147.125 94.25) (xy 166.625 94.2)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer F.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 168.65 74.275) (xy 164.35987 74.275) (xy 164.35987 77.05) (xy 168.65 77.05)
      )
    )
  )
  (zone (net 4) (net_name Board_1-/VBUS-) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 168.65 74.275) (xy 164.35 74.275) (xy 164.35 77.05) (xy 168.65 77.05)
      )
    )
  )
  (zone (net 6) (net_name Board_1-Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 171.875 140.5) (xy 146.725 140.5) (xy 145.85 134.75) (xy 164.1 134.75) (xy 164.1 125.85)
        (xy 150.6 125.85) (xy 150.6 122.15) (xy 164.1 122.15) (xy 164.1 113.25) (xy 149.6 113.25)
        (xy 139.6 107.1) (xy 139.6 105.75) (xy 128.125 105.75) (xy 128.15 94.75) (xy 139.625 94.75)
        (xy 139.625 91.2) (xy 160.825 91.2) (xy 165.225 86.95) (xy 165.225 84.2) (xy 169.1 84.2)
        (xy 169.1 79.475) (xy 164.325 79.475) (xy 157.275 80.25) (xy 147.85 80.25) (xy 147.875 76.7)
        (xy 157.275 76.7) (xy 164.325 77.55) (xy 169.1 77.5) (xy 169.1 72.8) (xy 165.225 72.8)
        (xy 165.225 70) (xy 160.975 65.8) (xy 145.625 65.825) (xy 145.625 59.5) (xy 171.875 59.5)
      )
    )
  )
  (zone (net 6) (net_name Board_1-Earth) (layer B.Cu) (hatch edge 0.508)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.5) (smoothing fillet) (radius 0.2))
    (polygon
      (pts
        (xy 128.125 105.75) (xy 134.625 105.75) (xy 134.625 94.75) (xy 128.125 94.75)
      )
    )
  )
)
