(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1)
    (drawings 75)
    (tracks 198)
    (zones 0)
    (modules 27)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (user_trace_width 1)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.8 0.3)
    (user_via 0.9 0.4)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 0.8128 0.8128)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 0 0)
    (grid_origin 120 77.5)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-+3.3V)
  (net 2 Board_1-/1PPS)
  (net 3 Board_1-/AADET_N)
  (net 4 Board_1-/EX_ANT)
  (net 5 Board_1-/GPS_RX)
  (net 6 Board_1-/GPS_TX)
  (net 7 Board_1-/U232_D+)
  (net 8 Board_1-/U232_D-)
  (net 9 Board_1-/USB_D+)
  (net 10 Board_1-/USB_D-)
  (net 11 Board_1-/VBAT)
  (net 12 Board_1-/~LED_WLAN)
  (net 13 Board_1-/~RESET)
  (net 14 Board_1-GND)
  (net 15 "Board_1-Net-(D1-Pad1)")
  (net 16 "Board_1-Net-(LED1-Pad1)")
  (net 17 "Board_1-Net-(LED2-Pad1)")
  (net 18 "Board_1-Net-(LED3-Pad1)")
  (net 19 "Board_1-Net-(Q2-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-+3.3V)
    (add_net Board_1-/1PPS)
    (add_net Board_1-/AADET_N)
    (add_net Board_1-/EX_ANT)
    (add_net Board_1-/GPS_RX)
    (add_net Board_1-/GPS_TX)
    (add_net Board_1-/U232_D+)
    (add_net Board_1-/U232_D-)
    (add_net Board_1-/USB_D+)
    (add_net Board_1-/USB_D-)
    (add_net Board_1-/VBAT)
    (add_net Board_1-/~LED_WLAN)
    (add_net Board_1-/~RESET)
    (add_net Board_1-GND)
    (add_net "Board_1-Net-(D1-Pad1)")
    (add_net "Board_1-Net-(LED1-Pad1)")
    (add_net "Board_1-Net-(LED2-Pad1)")
    (add_net "Board_1-Net-(LED3-Pad1)")
    (add_net "Board_1-Net-(Q2-Pad3)")
  )
  (net_class "GPS RF" ""
    (clearance 0.23093)
    (trace_width 1.02)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.254)
    (via_dia 0.8)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class "USB Data" ""
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.127)
    (diff_pair_gap 0.152)
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 146.5 119.25)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at -1.8 0 270) (layer F.SilkS))
    (fp_text value RB520S30T1G (at 0 1.4) (layer F.Fab))
    (fp_text user %R (at 0 -1.3) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3.3V))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Board_1-Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Coaxial:U.FL_Hirose_U.FL-R-SMT-1_Vertical (layer F.Cu) (tedit 5A1DBFC3)
    (at 156.465 78.45 90)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J2 (at 0.5 0) (layer F.SilkS))
    (fp_text value ANT (at 2.4 -0.015 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.475 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-GND))
    (pad 1 smd rect (at -1.05 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 4 Board_1-/EX_ANT))
    (pad 2 smd rect (at 0.475 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (offset (xyz 0.4749999928262157 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:JST_SH_SM02B-SRSS-TB_1x02-1MP_P1.00mm_Horizontal_3D" (layer F.Cu) (tedit 5FFD7A35)
    (at 139.65 107 270)
    (descr "JST SH series connector, SM02B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J1 (at 0 0 270) (layer F.SilkS))
    (fp_text value 1PPS (at 0 4.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0.5 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Board_1-/1PPS))
    (pad 2 smd roundrect (at 0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (pad MP smd roundrect (at -1.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at 1.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (model :SnapEDA-3D:JST/SM02B-SRSS-TB.STEP
      (offset (xyz 0 1.3 -0.35))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:Q_EMT3F" (layer F.Cu) (tedit 5FFD7510)
    (at 164.45 99.15 90)
    (fp_text reference Q1 (at -1.8796 0.4572) (layer F.SilkS))
    (fp_text value DTC143Z (at 0 2.5 -90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.66 -0.5 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-/1PPS))
    (pad 2 smd rect (at -0.66 0.5 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-GND))
    (pad 3 smd rect (at 0.66 0 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 12 Board_1-/~LED_WLAN))
    (model :SnapEDA-3D:DTC143ZEBTL.STEP
      (offset (xyz 0 0 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:Q_EMT3F" (layer F.Cu) (tedit 5FFD7510)
    (at 164.45 95.34 90)
    (fp_text reference Q2 (at -1.8796 0.4572) (layer F.SilkS))
    (fp_text value DTA043T (at 0 2.5 -90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.66 -0.5 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 Board_1-/AADET_N))
    (pad 2 smd rect (at -0.66 0.5 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-GND))
    (pad 3 smd rect (at 0.66 0 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 19 "Board_1-Net-(Q2-Pad3)"))
    (model :SnapEDA-3D:DTC143ZEBTL.STEP
      (offset (xyz 0 0 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:XCVR_LC86L" (layer F.Cu) (tedit 600A618C)
    (at 150.94 93.484)
    (fp_text reference GNSS1 (at 0.01 0.016) (layer F.SilkS))
    (fp_text value LC86L (at -5.08 11.365) (layer F.Fab))
    (pad 3 smd oval (at -7.75 -1.27) (size 2.5 1) (layers F.Cu F.Mask)
      (net 14 Board_1-GND))
    (pad 10 smd oval (at 7.75 -1.27) (size 2.5 1) (layers F.Cu F.Mask))
    (pad 4 smd oval (at -7.75 1.27) (size 2.5 1) (layers F.Cu F.Mask)
      (net 1 Board_1-+3.3V))
    (pad 2 smd oval (at -7.75 -3.81) (size 2.5 1) (layers F.Cu F.Mask)
      (net 6 Board_1-/GPS_TX))
    (pad 1 smd oval (at -7.75 -6.35) (size 2.5 1) (layers F.Cu F.Mask)
      (net 5 Board_1-/GPS_RX))
    (pad 5 smd oval (at -7.75 3.81) (size 2.5 1) (layers F.Cu F.Mask)
      (net 11 Board_1-/VBAT))
    (pad 6 smd oval (at -7.75 6.35) (size 2.5 1) (layers F.Cu F.Mask)
      (net 2 Board_1-/1PPS))
    (pad 11 smd oval (at 7.75 -3.81) (size 2.5 1) (layers F.Cu F.Mask)
      (net 4 Board_1-/EX_ANT))
    (pad 12 smd oval (at 7.75 -6.35) (size 2.5 1) (layers F.Cu F.Mask)
      (net 14 Board_1-GND))
    (pad 9 smd oval (at 7.75 1.27) (size 2.5 1) (layers F.Cu F.Mask))
    (pad 8 smd oval (at 7.75 3.81) (size 2.5 1) (layers F.Cu F.Mask)
      (net 3 Board_1-/AADET_N))
    (pad 7 smd oval (at 7.75 6.35) (size 2.5 1) (layers F.Cu F.Mask))
    (model :SnapEDA-3D:L80.step
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 180))
    )
  )
  (module "1 My Footprints:CAP_DSK-3R3H224U-HL" (layer F.Cu) (tedit 600A6160)
    (at 143.8 114.65 90)
    (fp_text reference C1 (at 0.52584 -3.89117 90) (layer F.Fab))
    (fp_text value DSK-3R3H224U-HL (at 1.27 3.81 90) (layer F.SilkS) hide)
    (fp_text user + (at 1.8 -3.1 90) (layer F.SilkS))
    (fp_text user BAT (at 0 0 270) (layer F.SilkS))
    (fp_text user - (at 3.54863 3.63306 90) (layer F.Fab))
    (pad 1 smd rect (at 0 -5.075 90) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 11 Board_1-/VBAT))
    (pad 2 smd rect (at 0 5.075 90) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-GND))
    (model :SnapEDA-3D:DSK-3R3H224U-HL.step
      (offset (xyz 0 0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.2 97.785 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 1.565 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 Board_1-/VBAT))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.25 94.265 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at -1.6 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.25 94.265 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.6 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 155.8 114.35 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -1.55 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 156.85 114.35 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 1.55 0 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.55 111.4 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -1.6 0) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 158.55 112.45)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 1.6 0) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.15 119.25 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.5 0 270) (layer F.SilkS))
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Board_1-Net-(D1-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 Board_1-/VBAT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 143.865 79.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.535 0 180) (layer F.SilkS))
    (fp_text value 51R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Board_1-Net-(LED1-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 147.6 79.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 1.55 0) (layer F.SilkS))
    (fp_text value 220R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Board_1-Net-(LED2-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Board_1-/~LED_WLAN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 151.3 79.2)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 1.55 0) (layer F.SilkS))
    (fp_text value 220R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Board_1-Net-(LED3-Pad1)"))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Board_1-Net-(Q2-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.55 110.35 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -1.6 0) (layer F.SilkS))
    (fp_text value 4.7K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/~RESET))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 138.25 97.785 270)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.565 0 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 Board_1-/VBAT))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:QFN28G_0.5-5X5MM" (layer F.Cu) (tedit 600A657C)
    (at 153.95 109.7 90)
    (fp_text reference U1 (at -0.976228 -3.805681 90) (layer F.SilkS))
    (fp_text value CP2102N-A01-GQFN28 (at 2.876918 3.695357 90) (layer F.Fab))
    (pad 1 smd rect (at -2.59 -1.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -2.59 -1 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -2.59 -0.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-GND))
    (pad 4 smd rect (at -2.59 0 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-/U232_D+))
    (pad 5 smd rect (at -2.59 0.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask)
      (net 8 Board_1-/U232_D-))
    (pad 6 smd rect (at -2.59 1 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3.3V))
    (pad 7 smd rect (at -2.59 1.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3.3V))
    (pad 8 smd rect (at -1.5 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3.3V))
    (pad 9 smd rect (at -1 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 Board_1-/~RESET))
    (pad 10 smd rect (at -0.5 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 0 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 0.5 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 1 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.5 2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 2.59 1.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 16 smd rect (at 2.59 1 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 2.59 0.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.59 0 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.59 -0.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 2.59 -1 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 2.59 -1.5 90) (size 0.9 0.254) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at 1.5 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 1 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-/1PPS))
    (pad 24 smd rect (at 0.5 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 0 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 Board_1-/GPS_TX))
    (pad 26 smd rect (at -0.5 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 Board_1-/GPS_RX))
    (pad 27 smd rect (at -1 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at -1.5 -2.59 90) (size 0.254 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at 0 0 90) (size 3.1 3.1) (layers F.Cu F.Mask)
      (net 14 Board_1-GND))
    (model :SnapEDA-3D:INTERFACE-CP2102-GMR_QFN28_.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:LED_0603_1608Metric_SnapModel" (layer F.Cu) (tedit 5FFD7569)
    (at 144.3 77.85)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED1 (at 0 -1.43) (layer F.Fab))
    (fp_text value PWR (at 0 -1.3) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Board_1-Net-(LED1-Pad1)"))
    (model :SnapEDA-3D:LTST-C193TBKT-5A.STEP
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:LED_0603_1608Metric_SnapModel" (layer F.Cu) (tedit 5FFD7569)
    (at 148.05 77.85)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED2 (at 0 -1.43) (layer F.Fab))
    (fp_text value 1PPS (at 0 -1.3) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 "Board_1-Net-(LED2-Pad1)"))
    (model :SnapEDA-3D:LTST-C193TBKT-5A.STEP
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module "1 My Footprints:LED_0603_1608Metric_SnapModel" (layer F.Cu) (tedit 5FFD7569)
    (at 151.75 77.85)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED3 (at 0 -1.43) (layer F.Fab))
    (fp_text value ANT (at 0 -1.3) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Board_1-Net-(LED3-Pad1)"))
    (model :SnapEDA-3D:LTST-C193TBKT-5A.STEP
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 153.7 114.35 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at -1.55 0 270) (layer F.SilkS))
    (fp_text value 33R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 Board_1-/USB_D+))
    (pad 2 smd roundrect (at 0.485 0 90) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-/U232_D+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 154.7 114.35 270)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 1.55 0 90) (layer F.SilkS))
    (fp_text value 33R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 Board_1-/U232_D-))
    (pad 2 smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 Board_1-/USB_D-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "1 My Footprints:mini-PCIe_F1_Full_v600" (layer F.Cu) (tedit 6008FD16)
    (at 147.1 126.25)
    (zone_connect 2)
    (fp_text reference PC1 (at 0 0.8) (layer F.Fab) hide)
    (fp_text value miniPCIe (at 3.85 -26.8) (layer F.Fab))
    (pad 55 thru_hole custom (at 15.95 -48.05) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 14 Board_1-GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
      ))
    (pad 54 thru_hole custom (at -8.25 -48.05) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 14 Board_1-GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
      ))
    (pad 2 smd rect (at -7.55 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 4 smd rect (at -6.75 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 6 smd rect (at -5.95 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 8 smd rect (at -5.15 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 10 smd rect (at -4.35 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 12 smd rect (at -3.55 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 14 smd rect (at -2.75 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 16 smd rect (at -1.95 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 52 smd rect (at 15.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 50 smd rect (at 14.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 48 smd rect (at 14.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 46 smd rect (at 13.25 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 44 smd rect (at 12.45 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 12 Board_1-/~LED_WLAN) (zone_connect 2))
    (pad 42 smd rect (at 11.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 40 smd rect (at 10.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 38 smd rect (at 10.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 9 Board_1-/USB_D+) (zone_connect 2))
    (pad 36 smd rect (at 9.25 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 10 Board_1-/USB_D-) (zone_connect 2))
    (pad 34 smd rect (at 8.45 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 32 smd rect (at 7.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 30 smd rect (at 6.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 28 smd rect (at 6.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 26 smd rect (at 5.25 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 24 smd rect (at 4.45 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 22 smd rect (at 3.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 13 Board_1-/~RESET) (zone_connect 2))
    (pad 20 smd rect (at 2.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 18 smd rect (at 2.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 17 smd rect (at 1.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at -7.95 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 3 smd rect (at -7.15 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -6.35 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 7 smd rect (at -5.55 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 9 smd rect (at -4.75 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 11 smd rect (at -3.95 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 13 smd rect (at -3.15 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 51 smd rect (at 15.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 49 smd rect (at 14.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 47 smd rect (at 13.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 45 smd rect (at 12.85 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 43 smd rect (at 12.05 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 41 smd rect (at 11.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 39 smd rect (at 10.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 37 smd rect (at 9.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 35 smd rect (at 8.85 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 33 smd rect (at 8.05 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 31 smd rect (at 7.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 29 smd rect (at 6.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 27 smd rect (at 5.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 25 smd rect (at 4.85 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 23 smd rect (at 4.05 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 21 smd rect (at 3.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
    (pad 19 smd rect (at 2.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 15 smd rect (at -2.35 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 14 Board_1-GND) (zone_connect 2))
  )
  (gr_line (start 146.3548 122.9242) (end 146.351 123) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.3663 122.8492) (end 146.3548 122.9242) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.3854 122.7758) (end 146.3663 122.8492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4117 122.7046) (end 146.3854 122.7758) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4451 122.6365) (end 146.4117 122.7046) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4852 122.5721) (end 146.4451 122.6365) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.5317 122.5121) (end 146.4852 122.5721) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.584 122.4571) (end 146.5317 122.5121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6415 122.4077) (end 146.584 122.4571) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7038 122.3644) (end 146.6415 122.4077) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7701 122.3275) (end 146.7038 122.3644) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8399 122.2976) (end 146.7701 122.3275) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9123 122.2749) (end 146.8399 122.2976) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.9866 122.2596) (end 146.9123 122.2749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.0621 122.252) (end 146.9866 122.2596) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.1379 122.252) (end 147.0621 122.252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.2134 122.2596) (end 147.1379 122.252) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.2877 122.2749) (end 147.2134 122.2596) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.3601 122.2976) (end 147.2877 122.2749) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.4299 122.3275) (end 147.3601 122.2976) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.4962 122.3644) (end 147.4299 122.3275) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.5585 122.4077) (end 147.4962 122.3644) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.616 122.4571) (end 147.5585 122.4077) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.6683 122.5121) (end 147.616 122.4571) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7148 122.5721) (end 147.6683 122.5121) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7549 122.6365) (end 147.7148 122.5721) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.7883 122.7046) (end 147.7549 122.6365) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8146 122.7758) (end 147.7883 122.7046) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8337 122.8492) (end 147.8146 122.7758) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8452 122.9242) (end 147.8337 122.8492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.849 123) (end 147.8452 122.9242) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.8498 126.251) (end 147.849 123) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.75 126.251) (end 147.8498 126.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.751 123.75) (end 163.75 126.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.7554 123.6665) (end 163.751 123.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.7685 123.5839) (end 163.7554 123.6665) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.7901 123.5031) (end 163.7685 123.5839) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.8201 123.425) (end 163.7901 123.5031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.858 123.3505) (end 163.8201 123.425) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.9036 123.2804) (end 163.858 123.3505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.9562 123.2154) (end 163.9036 123.2804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.0154 123.1562) (end 163.9562 123.2154) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.0804 123.1036) (end 164.0154 123.1562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.1505 123.058) (end 164.0804 123.1036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.225 123.0201) (end 164.1505 123.058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3031 122.9901) (end 164.225 123.0201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.3839 122.9685) (end 164.3031 122.9901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.4665 122.9554) (end 164.3839 122.9685) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.55 122.951) (end 164.4665 122.9554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.9509 122.9504) (end 164.55 122.951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.9504 75.2991) (end 165.9509 122.9504) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.9491 75.2996) (end 165.9504 75.2991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 135.949 122.9502) (end 135.9491 75.2996) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.35 122.951) (end 135.949 122.9502) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.4335 122.9554) (end 137.35 122.951) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.5161 122.9685) (end 137.4335 122.9554) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.5969 122.9901) (end 137.5161 122.9685) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.675 123.0201) (end 137.5969 122.9901) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.7495 123.058) (end 137.675 123.0201) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.8196 123.1036) (end 137.7495 123.058) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.8846 123.1562) (end 137.8196 123.1036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.9438 123.2154) (end 137.8846 123.1562) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.9964 123.2804) (end 137.9438 123.2154) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.042 123.3505) (end 137.9964 123.2804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.0799 123.425) (end 138.042 123.3505) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.1099 123.5031) (end 138.0799 123.425) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.1315 123.5839) (end 138.1099 123.5031) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.1446 123.6665) (end 138.1315 123.5839) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.149 123.75) (end 138.1446 123.6665) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.15 126.251) (end 138.149 123.75) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.3504 126.2509) (end 138.15 126.251) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.351 123) (end 146.3504 126.2509) (layer Edge.Cuts) (width 0.1))
  (gr_text JLCJLCJLCJLC (at 150.95 105.75) (layer B.SilkS))
  (zone (net 14) (net_name Board_1-GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 165.95 75.3) (xy 165.95 126.25) (xy 135.95 126.25) (xy 135.95 75.3)
      )
    )
  )
  (zone (net 14) (net_name Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.15))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.154) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 165.95 75.3) (xy 165.95 126.25) (xy 135.95 126.25) (xy 135.95 75.3)
      )
    )
  )
  (zone (net 14) (net_name Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads thru_hole_only (clearance 0.15))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 157.925 88) (xy 157.15 88) (xy 157.15 86.25) (xy 157.925 86.25)
      )
    )
  )
  (zone (net 1) (net_name Board_1-+3.3V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads thru_hole_only (clearance 0.154))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 158.35 112.45) (xy 158.35 113.4) (xy 157.6 114.15) (xy 157.075 114.15) (xy 155.475 114.15)
        (xy 155.45 113.375) (xy 154.825 112.75) (xy 154.825 111.85) (xy 155.6 111.85) (xy 156.1 111.35)
        (xy 156.1 111.1) (xy 157.825 111.1) (xy 158.325 111.1)
      )
    )
  )
)
