(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1)
    (drawings 72)
    (tracks 206)
    (zones 0)
    (modules 23)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.154)
    (user_trace_width 0.127)
    (user_trace_width 0.15427)
    (user_trace_width 0.254)
    (user_trace_width 0.305)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.0889)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.45)
    (via_min_drill 0.2)
    (user_via 0.45 0.2)
    (user_via 0.6 0.3)
    (user_via 0.6858 0.3302)
    (user_via 0.889 0.381)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 0.8128 0.8128)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Board_1-+3.3V)
  (net 2 Board_1-/GNSS_ANT)
  (net 3 Board_1-/GPS_D+)
  (net 4 Board_1-/GPS_D-)
  (net 5 Board_1-/RXD)
  (net 6 Board_1-/TP1)
  (net 7 Board_1-/TP2)
  (net 8 Board_1-/TXD)
  (net 9 Board_1-/USB_D+)
  (net 10 Board_1-/USB_D-)
  (net 11 Board_1-/VCC_RF)
  (net 12 Board_1-/V_ANT)
  (net 13 Board_1-/V_BCKP)
  (net 14 Board_1-/~LED_WLAN)
  (net 15 Board_1-/~LED_WWAN)
  (net 16 Board_1-/~RESET)
  (net 17 Board_1-GND)
  (net 18 "Board_1-Net-(D1-Pad1)")
  (net 19 "Board_1-Net-(LED1-Pad1)")
  (net 20 "Board_1-Net-(LED2-Pad1)")
  (net 21 "Board_1-Net-(LED3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.154)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net Board_1-+3.3V)
    (add_net Board_1-/GNSS_ANT)
    (add_net Board_1-/GPS_D+)
    (add_net Board_1-/GPS_D-)
    (add_net Board_1-/RXD)
    (add_net Board_1-/TP1)
    (add_net Board_1-/TP2)
    (add_net Board_1-/TXD)
    (add_net Board_1-/USB_D+)
    (add_net Board_1-/USB_D-)
    (add_net Board_1-/VCC_RF)
    (add_net Board_1-/V_ANT)
    (add_net Board_1-/V_BCKP)
    (add_net Board_1-/~LED_WLAN)
    (add_net Board_1-/~LED_WWAN)
    (add_net Board_1-/~RESET)
    (add_net Board_1-GND)
    (add_net "Board_1-Net-(D1-Pad1)")
    (add_net "Board_1-Net-(LED1-Pad1)")
    (add_net "Board_1-Net-(LED2-Pad1)")
    (add_net "Board_1-Net-(LED3-Pad1)")
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.3048)
    (via_dia 0.7)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class RF_ANT ""
    (clearance 0.1527)
    (trace_width 0.29337)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
  )
  (net_class USB_DATA ""
    (clearance 0.154)
    (trace_width 0.1615)
    (via_dia 0.45)
    (via_drill 0.2)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1615)
    (diff_pair_gap 0.154)
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.7375 103.175 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.9375 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-523 (layer F.Cu) (tedit 586419F0)
    (at 161.3 105.85 270)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at -1.8 0.025) (layer F.SilkS))
    (fp_text value RB520S30T1G (at 0 1.4 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Board_1-Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.7 0 90) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 1 Board_1-+3.3V))
    (model ${KIPRJMOD}/shapes3D/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.15 81.125)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.35 0 270) (layer F.SilkS))
    (fp_text value 33R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 Board_1-/USB_D-))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Board_1-/GPS_D-))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:LED_0603_1608Metric_SnapModel (layer F.Cu) (tedit 5FFD7569)
    (at 151.2 76.525)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED3 (at 0 -1.43) (layer F.Fab))
    (fp_text value TP2 (at 0 -1.25) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Board_1-Net-(LED3-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KIPRJMOD}/shapes3D/LTST-C193TBKT-5A.STEP
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module mPCIe-GNSS:U.FL_Hirose_U.FL-R-SMT-1_Vertical_Tweaked (layer F.Cu) (tedit 5FF9340A)
    (at 156.6 77.275 90)
    (descr "Hirose U.FL Coaxial https://www.hirose.com/product/en/products/U.FL/U.FL-R-SMT-1%2810%29/")
    (tags "Hirose U.FL Coaxial")
    (attr smd)
    (fp_text reference J1 (at 0.05 0 unlocked) (layer F.SilkS))
    (fp_text value ANT (at 2 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0 -1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-GND))
    (pad 1 smd rect (at -1.525 0 90) (size 1.05 1) (layers F.Cu F.Paste F.Mask)
      (net 2 Board_1-/GNSS_ANT))
    (pad 2 smd rect (at 0 1.475 90) (size 2.2 1.05) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/U.FL_Hirose_U.FL-R-SMT-1_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.89 103.65)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 1.6 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/V_BCKP))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:LED_0603_1608Metric_SnapModel (layer F.Cu) (tedit 5FFD7569)
    (at 143.1875 76.525)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED1 (at 0 -1.2) (layer F.Fab) hide)
    (fp_text value PWR (at 0 -1.25) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Board_1-Net-(LED1-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KIPRJMOD}/shapes3D/LTST-C193TBKT-5A.STEP
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.15 80.025 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -1.35 0 270) (layer F.SilkS))
    (fp_text value 33R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Board_1-/GPS_D+))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 Board_1-/USB_D+))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 142.7 77.875)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.565 0) (layer F.SilkS))
    (fp_text value 51R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 "Board_1-Net-(LED1-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:CAP_DSK-3R3H224U-HL (layer F.Cu) (tedit 600A6160)
    (at 156.8 110.6)
    (fp_text reference BAT1 (at 0 0) (layer F.SilkS))
    (fp_text value DSK-3R3H224U (at 2.05 4.635598) (layer F.Fab))
    (fp_text user - (at 3.54863 3.63306) (layer F.Fab))
    (fp_text user + (at 1.8 -3.1) (layer F.SilkS))
    (pad 2 smd rect (at 0 5.075) (size 4 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-GND))
    (pad 1 smd rect (at 0 -5.075) (size 5 2) (layers F.Cu F.Paste F.Mask)
      (net 13 Board_1-/V_BCKP))
    (model ${KIPRJMOD}/shapes3D/DSK-3R3H224U-HL.step
      (offset (xyz 0 0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Capacitor_SMD:C_0402_1005Metric (layer F.Cu) (tedit 5B301BBE)
    (at 154.885 102.6)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 1.615 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/V_BCKP))
    (model ${KIPRJMOD}/shapes3D/C_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 146.75 77.875)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.55 0) (layer F.SilkS))
    (fp_text value 220R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 Board_1-/~LED_WWAN))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Board_1-Net-(LED2-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:LED_0603_1608Metric_SnapModel (layer F.Cu) (tedit 5FFD7569)
    (at 147.25 76.525)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference LED2 (at 0 -1.2) (layer F.Fab) hide)
    (fp_text value TP1 (at 0 -1.25) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Board_1-Net-(LED2-Pad1)"))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KIPRJMOD}/shapes3D/LTST-C193TBKT-5A.STEP
      (offset (xyz 0 0 -0.01))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module mPCIe-GNSS:Q_EMT3F (layer F.Cu) (tedit 5FFD7510)
    (at 163.05 87.8 90)
    (fp_text reference Q2 (at -1.8 0.5) (layer F.SilkS))
    (fp_text value DTC143ZEBTL (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 0.66 0 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 14 Board_1-/~LED_WLAN))
    (pad 2 smd rect (at -0.66 0.5 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-GND))
    (pad 1 smd rect (at -0.66 -0.5 90) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 Board_1-/TP2))
    (model ${KIPRJMOD}/shapes3D/DTC143ZEBTL.STEP
      (offset (xyz 0 0 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 150.65 77.875)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 1.55 0) (layer F.SilkS))
    (fp_text value 220R (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 Board_1-/~LED_WLAN))
    (pad 1 smd roundrect (at -0.485 0) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Board_1-Net-(LED3-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.7375 104.675 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 1.95 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:Q_EMT3F (layer F.Cu) (tedit 5FFD7510)
    (at 136.45 84.395 270)
    (fp_text reference Q1 (at -1.75 0.53) (layer F.SilkS))
    (fp_text value DTC143ZEBTL (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 0.66 0 270) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 15 Board_1-/~LED_WWAN))
    (pad 2 smd rect (at -0.66 0.5 270) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 17 Board_1-GND))
    (pad 1 smd rect (at -0.66 -0.5 270) (size 0.81 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 Board_1-/TP1))
    (model ${KIPRJMOD}/shapes3D/DTC143ZEBTL.STEP
      (offset (xyz 0 0 -0.03))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module Resistor_SMD:R_0402_1005Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.1 103.65 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -1.55 0) (layer F.SilkS))
    (fp_text value 1K (at 0 1.17) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/V_BCKP))
    (pad 1 smd roundrect (at -0.485 0 180) (size 0.59 0.64) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Board_1-Net-(D1-Pad1)"))
    (model ${KIPRJMOD}/shapes3D/R_0402_1005Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:ublox_LEA (layer F.Cu) (tedit 6008DDC5)
    (at 149.2 91.375 90)
    (descr "ublox LEA 6/7/8, (https://www.u-blox.com/sites/default/files/LEA-M8S-M8T-FW3_HardwareIntegrationManual_%28UBX-15030060%29.pdf)")
    (tags "GPS ublox LEA 6/7/8")
    (attr smd)
    (fp_text reference U1 (at 0 0 90) (layer F.SilkS))
    (fp_text value LEA-M8T (at 0 1.3 90) (layer F.Fab))
    (fp_text user %R (at 0 -0.7 90) (layer F.Fab))
    (pad 28 smd roundrect (at 8.4 -8.5 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-/TP1))
    (pad 27 smd roundrect (at 8.4 -7.4 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 26 smd roundrect (at 8.4 -6.3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 Board_1-/GPS_D+))
    (pad 25 smd roundrect (at 8.4 -5.2 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 Board_1-/GPS_D-))
    (pad 24 smd roundrect (at 8.4 -4.1 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 23 smd roundrect (at 8.4 -3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 22 smd roundrect (at 8.4 -1.9 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 21 smd roundrect (at 8.4 -0.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 20 smd roundrect (at 8.4 3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 19 smd roundrect (at 8.4 4.1 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Board_1-/V_ANT))
    (pad 18 smd roundrect (at 8.4 5.2 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 Board_1-/VCC_RF))
    (pad 17 smd roundrect (at 8.4 6.3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 16 smd roundrect (at 8.4 7.4 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 Board_1-/GNSS_ANT))
    (pad 15 smd roundrect (at 8.4 8.5 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 14 smd roundrect (at -8.4 8.5 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 13 smd roundrect (at -8.4 7.4 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 12 smd roundrect (at -8.4 6.3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-/TP2))
    (pad 11 smd roundrect (at -8.4 5.2 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 Board_1-/V_BCKP))
    (pad 10 smd roundrect (at -8.4 4.1 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 Board_1-/~RESET))
    (pad 9 smd roundrect (at -8.4 3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -8.4 -0.8 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 7 smd roundrect (at -8.4 -1.9 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 6 smd roundrect (at -8.4 -3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 5 smd roundrect (at -8.4 -4.1 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 4 smd roundrect (at -8.4 -5.2 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Board_1-/RXD))
    (pad 3 smd roundrect (at -8.4 -6.3 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 Board_1-/TXD))
    (pad 2 smd roundrect (at -8.4 -7.4 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -8.4 -8.5 90) (size 1.8 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (model ${KIPRJMOD}/shapes3D/LEA.STEP
      (offset (xyz 0 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 146.7375 101.675)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.9375 0 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (model ${KIPRJMOD}/shapes3D/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "mini-PCIe Cards:mini-PCIe_F1_Full_v517" locked (layer F.Cu) (tedit 6008FD16)
    (at 146.15 125.475)
    (zone_connect 2)
    (fp_text reference PC1 (at -11.6 -1.3) (layer F.SilkS))
    (fp_text value miniPCIe (at 3.9 1.3) (layer F.Fab))
    (pad 15 smd rect (at -2.35 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 19 smd rect (at 2.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 21 smd rect (at 3.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 23 smd rect (at 4.05 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 25 smd rect (at 4.85 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 27 smd rect (at 5.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 29 smd rect (at 6.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 31 smd rect (at 7.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 33 smd rect (at 8.05 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 35 smd rect (at 8.85 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 37 smd rect (at 9.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 39 smd rect (at 10.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 41 smd rect (at 11.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 43 smd rect (at 12.05 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 45 smd rect (at 12.85 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 47 smd rect (at 13.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 49 smd rect (at 14.45 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 51 smd rect (at 15.25 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 13 smd rect (at -3.15 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 11 smd rect (at -3.95 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 9 smd rect (at -4.75 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 7 smd rect (at -5.55 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 5 smd rect (at -6.35 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 3 smd rect (at -7.15 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 1 smd rect (at -7.95 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 17 smd rect (at 1.65 -1.375) (size 0.6 2.35) (layers F.Cu F.Mask)
      (zone_connect 2))
    (pad 18 smd rect (at 2.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 20 smd rect (at 2.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 22 smd rect (at 3.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 16 Board_1-/~RESET) (zone_connect 2))
    (pad 24 smd rect (at 4.45 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 26 smd rect (at 5.25 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 28 smd rect (at 6.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 30 smd rect (at 6.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 32 smd rect (at 7.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 34 smd rect (at 8.45 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 36 smd rect (at 9.25 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 10 Board_1-/USB_D-) (zone_connect 2))
    (pad 38 smd rect (at 10.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 9 Board_1-/USB_D+) (zone_connect 2))
    (pad 40 smd rect (at 10.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 42 smd rect (at 11.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 44 smd rect (at 12.45 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 46 smd rect (at 13.25 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 48 smd rect (at 14.05 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 50 smd rect (at 14.85 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 52 smd rect (at 15.65 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 16 smd rect (at -1.95 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 14 smd rect (at -2.75 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 12 smd rect (at -3.55 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 10 smd rect (at -4.35 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 8 smd rect (at -5.15 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 6 smd rect (at -5.95 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (zone_connect 2))
    (pad 4 smd rect (at -6.75 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 17 Board_1-GND) (zone_connect 2))
    (pad 2 smd rect (at -7.55 -1.375) (size 0.6 2.35) (layers B.Cu B.Mask)
      (net 1 Board_1-+3.3V) (zone_connect 2))
    (pad 54 thru_hole custom (at -8.25 -48.05) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 17 Board_1-GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
      ))
    (pad 55 thru_hole custom (at 15.95 -48.05) (size 2.6 2.6) (drill 2.6) (layers *.Cu *.Mask)
      (net 17 Board_1-GND) (zone_connect 2)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
        (gr_poly (pts
           (xy 2.9 2.9) (xy -2.9 2.9) (xy -2.9 -2.9) (xy 2.9 -2.9)) (width 0.05))
      ))
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 153.3 80.425)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -1.85 0 90) (layer F.SilkS))
    (fp_text value 10R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 Board_1-/VCC_RF))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 Board_1-/V_ANT))
    (model ${KIPRJMOD}/shapes3D/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mPCIe-GNSS:JST_SH_SM06B-SRSS-TB_1x06-1MP_P1.00mm_Horizontal_3D (layer F.Cu) (tedit 60207903)
    (at 138.9 108.125 270)
    (descr "JST SH series connector, SM06B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (attr smd)
    (fp_text reference J2 (at 0 0 270) (layer F.SilkS))
    (fp_text value IO (at 0 3.98 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad MP smd roundrect (at 3.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad MP smd roundrect (at -3.8 1.875 270) (size 1.2 1.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.208333))
    (pad 6 smd roundrect (at 2.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 Board_1-+3.3V))
    (pad 5 smd roundrect (at 1.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 Board_1-/TP2))
    (pad 4 smd roundrect (at 0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 Board_1-/RXD))
    (pad 3 smd roundrect (at -0.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 Board_1-/TXD))
    (pad 2 smd roundrect (at -1.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 Board_1-/TP1))
    (pad 1 smd roundrect (at -2.5 -2 270) (size 0.6 1.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 Board_1-GND))
  )
  (gr_line (start 146.8998 125.476) (end 146.899 122.225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.8 125.476) (end 146.8998 125.476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.801 122.975) (end 162.8 125.476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.8054 122.8915) (end 162.801 122.975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.8185 122.8089) (end 162.8054 122.8915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.8401 122.7281) (end 162.8185 122.8089) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.8701 122.65) (end 162.8401 122.7281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.908 122.5755) (end 162.8701 122.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.9536 122.5054) (end 162.908 122.5755) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.0062 122.4404) (end 162.9536 122.5054) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.0654 122.3812) (end 163.0062 122.4404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.1304 122.3286) (end 163.0654 122.3812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.2005 122.283) (end 163.1304 122.3286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.275 122.2451) (end 163.2005 122.283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.3531 122.2151) (end 163.275 122.2451) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.4339 122.1935) (end 163.3531 122.2151) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.5165 122.1804) (end 163.4339 122.1935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.6 122.176) (end 163.5165 122.1804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0009 122.1754) (end 163.6 122.176) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0004 74.5241) (end 165.0009 122.1754) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.9991 74.5246) (end 165.0004 74.5241) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.999 122.1752) (end 134.9991 74.5246) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.4 122.176) (end 134.999 122.1752) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.4835 122.1804) (end 136.4 122.176) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.5661 122.1935) (end 136.4835 122.1804) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.6469 122.2151) (end 136.5661 122.1935) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.725 122.2451) (end 136.6469 122.2151) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.7995 122.283) (end 136.725 122.2451) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.8696 122.3286) (end 136.7995 122.283) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.9346 122.3812) (end 136.8696 122.3286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.9938 122.4404) (end 136.9346 122.3812) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.0464 122.5054) (end 136.9938 122.4404) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.092 122.5755) (end 137.0464 122.5054) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.1299 122.65) (end 137.092 122.5755) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.1599 122.7281) (end 137.1299 122.65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.1815 122.8089) (end 137.1599 122.7281) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.1946 122.8915) (end 137.1815 122.8089) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.199 122.975) (end 137.1946 122.8915) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.2 125.476) (end 137.199 122.975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.4003 125.476) (end 137.2 125.476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.401 122.225) (end 145.4003 125.476) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.4048 122.1492) (end 145.401 122.225) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.4163 122.0742) (end 145.4048 122.1492) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.4354 122.0008) (end 145.4163 122.0742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.4617 121.9296) (end 145.4354 122.0008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.4951 121.8615) (end 145.4617 121.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.5352 121.7971) (end 145.4951 121.8615) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.5817 121.7371) (end 145.5352 121.7971) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.634 121.6821) (end 145.5817 121.7371) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.6915 121.6327) (end 145.634 121.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.7538 121.5894) (end 145.6915 121.6327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.8201 121.5525) (end 145.7538 121.5894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.8899 121.5226) (end 145.8201 121.5525) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 145.9623 121.4999) (end 145.8899 121.5226) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.0366 121.4846) (end 145.9623 121.4999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.1121 121.477) (end 146.0366 121.4846) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.1879 121.477) (end 146.1121 121.477) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.2634 121.4846) (end 146.1879 121.477) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.3377 121.4999) (end 146.2634 121.4846) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4101 121.5226) (end 146.3377 121.4999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.4799 121.5525) (end 146.4101 121.5226) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.5462 121.5894) (end 146.4799 121.5525) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6085 121.6327) (end 146.5462 121.5894) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.666 121.6821) (end 146.6085 121.6327) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7183 121.7371) (end 146.666 121.6821) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.7648 121.7971) (end 146.7183 121.7371) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8049 121.8615) (end 146.7648 121.7971) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8383 121.9296) (end 146.8049 121.8615) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8646 122.0008) (end 146.8383 121.9296) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8837 122.0742) (end 146.8646 122.0008) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.8952 122.1492) (end 146.8837 122.0742) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.899 122.225) (end 146.8952 122.1492) (layer Edge.Cuts) (width 0.1))
  (zone (net 17) (net_name Board_1-GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.154))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 0.4))
    (polygon
      (pts
        (xy 165 80.225) (xy 165 125.475) (xy 135 125.475) (xy 135 74.525) (xy 164.95 74.525)
      )
    )
  )
  (zone (net 17) (net_name Board_1-GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 164.95 74.525) (xy 164.95 80.225) (xy 165 125.475) (xy 135 125.475) (xy 135 80.275)
        (xy 135 74.525) (xy 140.75 74.525) (xy 159.3 74.525)
      )
    )
  )
  (zone (net 1) (net_name Board_1-+3.3V) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4) (smoothing fillet) (radius 0.75))
    (polygon
      (pts
        (xy 153.475 79.48125) (xy 146.725 79.46875) (xy 146.75 100.9375) (xy 161.05 100.975) (xy 161.05 81.825)
        (xy 165 81.825) (xy 165 100.975) (xy 165 120.375) (xy 165 122.125) (xy 162.750173 122.125)
        (xy 146.9 122.125) (xy 146.9 121.275) (xy 145.4 121.275) (xy 145.400001 122.125) (xy 137.2 122.125)
        (xy 135 122.125) (xy 135 120.375) (xy 135 80.475) (xy 140.95 80.475) (xy 140.95 74.675)
        (xy 153.5 74.675)
      )
    )
  )
  (zone (net 17) (net_name Board_1-GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.4))
    (polygon
      (pts
        (xy 164.95 74.525) (xy 165 80.225) (xy 165 125.475) (xy 135 125.475) (xy 135 80.275)
        (xy 135 74.525) (xy 140.75 74.525) (xy 159.3 74.525)
      )
    )
  )
)
